libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Fields
gprs_ra_id Struct Reference

`#include <gsm48.h>`

## Data Fields
uint16_t | mcc
uint16_t | mnc
bool | mnc_3_digits
uint16_t | lac
uint8_t | rac

## Field Documentation

## ◆ lac

uint16_t gprs_ra_id::lac

Referenced by gprs_rai_to_osmo(), gsm48_encode_ra(), gsm48_parse_ra(), gsm48_ra_equal(), osmo_rai_name_buf(), and osmo_rai_to_gprs().

## ◆ mcc

uint16_t gprs_ra_id::mcc

Referenced by gprs_rai_to_osmo(), gsm48_encode_ra(), gsm48_parse_ra(), gsm48_ra_equal(), osmo_rai_name_buf(), and osmo_rai_to_gprs().

## ◆ mnc

uint16_t gprs_ra_id::mnc

Referenced by gprs_rai_to_osmo(), gsm48_encode_ra(), gsm48_parse_ra(), gsm48_ra_equal(), osmo_rai_name_buf(), and osmo_rai_to_gprs().

## ◆ mnc_3_digits

bool gprs_ra_id::mnc_3_digits

Referenced by gprs_rai_to_osmo(), gsm48_encode_ra(), gsm48_parse_ra(), gsm48_ra_equal(), osmo_rai_name_buf(), and osmo_rai_to_gprs().

## ◆ rac

uint8_t gprs_ra_id::rac

Referenced by gprs_rai_to_osmo(), gsm48_encode_ra(), gsm48_parse_ra(), gsm48_ra_equal(), osmo_rai_name_buf(), and osmo_rai_to_gprs().

The documentation for this struct was generated from the following file:

- include/osmocom/gsm/gsm48.h