libosmogsm 1.13.1.1-afb4 Osmocom GSM library

gsm0808.h
Go to the documentation of this file.
1
4/*
5 * (C) 2009,2010 by Holger Hans Peter Freyther <zecke@selfish.org>
6 * (C) 2009,2010 by On-Waves
7 * All Rights Reserved
8 *
9 * This program is free software; you can redistribute it and/or modify
10 * it under the terms of the GNU General Public License as published by
11 * the Free Software Foundation; either version 2 of the License, or
12 * (at your option) any later version.
13 *
14 * This program is distributed in the hope that it will be useful,
15 * but WITHOUT ANY WARRANTY; without even the implied warranty of
16 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the
17 * GNU General Public License for more details.
18 *
19 */
20#pragma once
21
22#include "tlv.h"
23#include <osmocom/gsm/protocol/gsm_08_08.h>
24#include <osmocom/gsm/gsm0808_utils.h>
25#include <osmocom/gsm/gsm23003.h>
26#include <osmocom/gsm/protocol/gsm_23_003.h>
27#include <osmocom/core/utils.h>
28
29#include <osmocom/core/socket_compat.h>
30
31#define BSSMAP_MSG_SIZE 1024
32#define BSSMAP_MSG_HEADROOM 512
33
34 struct msgb;
35 struct gsm0808_cell_id_list2;
36
37 struct msgb *gsm0808_create_layer3(struct msgb *msg_l3, uint16_t nc,
38 uint16_t cc, int lac, uint16_t _ci)
39 OSMO_DEPRECATED("Use gsm0808_create_layer3_2() instead, to not lose leading zeros in the MNC");
40struct msgb *gsm0808_create_layer3_aoip(const struct msgb *msg_l3, uint16_t nc,
41 uint16_t cc, int lac, uint16_t _ci,
42 const struct gsm0808_speech_codec_list *scl)
43 OSMO_DEPRECATED("Use gsm0808_create_layer3_2() instead, to not lose leading zeros in the MNC");
44struct msgb *gsm0808_create_layer3_2(const struct msgb *msg_l3, const struct osmo_cell_global_id *cell,
45 const struct gsm0808_speech_codec_list *scl);
46struct msgb *gsm0808_create_reset(void);
47struct msgb *gsm0808_create_reset_ack(void);
48struct msgb *gsm0808_create_clear_command(uint8_t cause);
49struct msgb *gsm0808_create_clear_command2(uint8_t cause, bool csfb_ind);
50struct msgb *gsm0808_create_clear_complete(void);
51struct msgb *gsm0808_create_cipher(const struct gsm0808_encrypt_info *ei,
52 const uint8_t *cipher_response_mode);
53
54struct gsm0808_cipher_mode_command {
55 struct gsm0808_encrypt_info ei;
56
58 bool cipher_response_mode_present;
63 uint8_t cipher_response_mode;
64
65 bool kc128_present;
66 uint8_t kc128[16];
67
68 /* more items are defined in the spec and may be added later */
69 bool more_items; /*< always set this to false */
70};
71 struct msgb *gsm0808_create_cipher2(const struct gsm0808_cipher_mode_command *cmc);
72
73 struct msgb *gsm0808_create_cipher_complete(struct msgb *layer3, uint8_t alg_id);
74 struct msgb *gsm0808_create_cipher_reject(enum gsm0808_cause cause);
75 struct msgb *gsm0808_create_cipher_reject_ext(enum gsm0808_cause_class class, uint8_t ext);
76 struct msgb *gsm0808_create_classmark_request(void);
77 struct msgb *gsm0808_create_classmark_update(const uint8_t *cm2, uint8_t cm2_len,
78 const uint8_t *cm3, uint8_t cm3_len);
79 struct msgb *gsm0808_create_sapi_reject_cause(uint8_t link_id, uint16_t cause);
80 struct msgb *gsm0808_create_sapi_reject(uint8_t link_id)
81 OSMO_DEPRECATED("Use gsm0808_create_sapi_reject_cause() instead");
82 struct msgb *gsm0808_create_ass(const struct gsm0808_channel_type *ct,
83 const uint16_t *cic,
84 const struct sockaddr_storage *ss,
85 const struct gsm0808_speech_codec_list *scl,
86 const uint32_t *ci);
87 struct msgb *gsm0808_create_ass2(const struct gsm0808_channel_type *ct,
88 const uint16_t *cic,
89 const struct sockaddr_storage *ss,
90 const struct gsm0808_speech_codec_list *scl,
91 const uint32_t *ci,
92 const uint8_t *kc, const struct osmo_lcls *lcls);
93 struct msgb *gsm0808_create_ass_compl(uint8_t rr_cause, uint8_t chosen_channel,
94 uint8_t encr_alg_id, uint8_t speech_mode,
95 const struct sockaddr_storage *ss,
96 const struct gsm0808_speech_codec *sc,
97 const struct gsm0808_speech_codec_list
98 *scl);
99 struct msgb *gsm0808_create_ass_compl2(uint8_t rr_cause, uint8_t chosen_channel,
100 uint8_t encr_alg_id, uint8_t speech_mode,
101 const struct sockaddr_storage *ss,
102 const struct gsm0808_speech_codec *sc,
103 const struct gsm0808_speech_codec_list *scl,
104 enum gsm0808_lcls_status lcls_bss_status);
105 struct msgb *gsm0808_create_assignment_completed(uint8_t rr_cause,
106 uint8_t chosen_channel,
107 uint8_t encr_alg_id,
108 uint8_t speech_mode);
109 struct msgb *gsm0808_create_ass_fail(uint8_t cause, const uint8_t *rr_cause,
110 const struct gsm0808_speech_codec_list
111 *scl);
112 struct msgb *gsm0808_create_assignment_failure(uint8_t cause, uint8_t *rr_cause);
113 struct msgb *gsm0808_create_clear_rqst(uint8_t cause);
114 struct msgb *gsm0808_create_paging2(const char *imsi, const uint32_t *tmsi,
115 const struct gsm0808_cell_id_list2 *cil,
116 const uint8_t *chan_needed);
117 struct msgb *gsm0808_create_paging(const char *imsi, const uint32_t *tmsi,
118 const struct gsm0808_cell_id_list *cil,
119 const uint8_t *chan_needed)
120 OSMO_DEPRECATED("use gsm0808_create_paging2 instead");
121 struct msgb *gsm0808_create_lcls_conn_ctrl(enum gsm0808_lcls_config config,
122 enum gsm0808_lcls_control control);
123 struct msgb *gsm0808_create_lcls_conn_ctrl_ack(enum gsm0808_lcls_status status);
124 struct msgb *gsm0808_create_lcls_notification(enum gsm0808_lcls_status status, bool break_req);
125 struct msgb *gsm0808_create_common_id(const char *imsi,
126 const struct osmo_plmn_id *selected_plmn_id,
127 const struct osmo_plmn_id *last_used_eutran_plnm_id);
128
129
131 struct gsm0808_old_bss_to_new_bss_info {
132 bool extra_information_present;
133 struct {
134 bool prec;
135 bool lcs;
136 bool ue_prob;
137 } extra_information;
138
139 bool current_channel_type_2_present;
140 struct {
141 uint8_t mode;
142 uint8_t field;
143 } current_channel_type_2;
144
145 bool last_eutran_plmn_id_present;
146 struct osmo_plmn_id last_eutran_plmn_id;
147
148 /* more items are defined in the spec and may be added later */
149 bool more_items; /*< always set this to false */
150};
151
153 struct gsm0808_handover_required {
154 uint16_t cause;
155 struct gsm0808_cell_id_list2 cil;
156
157 bool current_channel_type_1_present;
158 uint8_t current_channel_type_1;
159
160 bool speech_version_used_present;
161 enum gsm0808_permitted_speech speech_version_used;
162
163 bool old_bss_to_new_bss_info_present;
164 struct gsm0808_old_bss_to_new_bss_info old_bss_to_new_bss_info;
165
166 /* more items are defined in the spec and may be added later */
167 bool more_items; /*< always set this to false */
168};
169 struct msgb *gsm0808_create_handover_required(const struct gsm0808_handover_required *params);
170
172 struct gsm0808_handover_required_reject {
173 uint16_t cause;
174
175 /* more items are defined in the spec and may be added later */
176 bool more_items; /*< always set this to false */
177};
178 struct msgb *gsm0808_create_handover_required_reject(const struct gsm0808_handover_required_reject *params);
179
181 struct gsm0808_handover_request {
182 struct gsm0808_channel_type channel_type;
183 struct gsm0808_encrypt_info encryption_information;
184 struct osmo_gsm48_classmark classmark_information;
185 struct gsm0808_cell_id cell_identifier_serving;
186 struct gsm0808_cell_id cell_identifier_target;
187 enum gsm0808_cause cause;
188
189 bool current_channel_type_1_present;
190 uint8_t current_channel_type_1;
191
192 enum gsm0808_permitted_speech speech_version_used;
193
194 uint8_t chosen_encryption_algorithm_serving;
195
197 bool old_bss_to_new_bss_info_present;
198 struct gsm0808_old_bss_to_new_bss_info old_bss_to_new_bss_info;
201 const uint8_t *old_bss_to_new_bss_info_raw;
202 uint8_t old_bss_to_new_bss_info_raw_len;
203
204 const char *imsi;
205
206 const struct sockaddr_storage *aoip_transport_layer;
207
208 const struct gsm0808_speech_codec_list *codec_list_msc_preferred;
209
210 bool call_id_present;
211 uint32_t call_id;
212
213 const uint8_t *global_call_reference;
214 uint8_t global_call_reference_len;
215
216 /* more items are defined in the spec and may be added later */
217 bool more_items;
219 bool kc128_present;
220 uint8_t kc128[16];
221
222 bool more_items2;
223};
224 struct msgb *gsm0808_create_handover_request(const struct gsm0808_handover_request *params);
225
226 struct msgb *gsm0808_create_handover_request_ack(const uint8_t *l3_info, uint8_t l3_info_len,
227 uint8_t chosen_channel, uint8_t chosen_encr_alg,
228 uint8_t chosen_speech_version);
229
230 struct gsm0808_handover_request_ack {
231 const uint8_t *l3_info;
232 uint8_t l3_info_len;
233
234 bool chosen_channel_present;
235 uint8_t chosen_channel;
236
239 uint8_t chosen_encr_alg;
240
241 /* chosen_speech_version == 0 omits the IE */
242 enum gsm0808_permitted_speech chosen_speech_version;
243
244 bool speech_codec_chosen_present;
245 struct gsm0808_speech_codec speech_codec_chosen;
246
247 const struct sockaddr_storage *aoip_transport_layer;
248
249 bool more_items;
251 struct gsm0808_speech_codec_list codec_list_bss_supported; /*< omit when .len == 0 */
252
253 /* more items are defined in the spec and may be added later */
254 bool more_items2;
255};
256 struct msgb *gsm0808_create_handover_request_ack2(const struct gsm0808_handover_request_ack *params);
257
258 struct gsm0808_handover_command {
259 const uint8_t *l3_info;
260 uint8_t l3_info_len;
261
262 struct gsm0808_cell_id cell_identifier;
263
264 const uint8_t *new_bss_to_old_bss_info_raw;
265 size_t new_bss_to_old_bss_info_raw_len;
266
267 /* more items are defined in the spec and may be added later */
268 bool more_items;
269};
270 struct msgb *gsm0808_create_handover_command(const struct gsm0808_handover_command *params);
271
272 struct msgb *gsm0808_create_handover_detect(void);
273 struct msgb *gsm0808_create_handover_succeeded(void);
274
275 struct gsm0808_handover_complete {
276 bool rr_cause_present;
277 uint8_t rr_cause;
278
279 bool speech_codec_chosen_present;
280 struct gsm0808_speech_codec speech_codec_chosen;
281
282 struct gsm0808_speech_codec_list codec_list_bss_supported; /*< omit when .len == 0 */
283
284 bool chosen_encr_alg_present;
285 uint8_t chosen_encr_alg;
286
287 bool chosen_channel_present;
288 uint8_t chosen_channel;
289
290 bool lcls_bss_status_present;
291 enum gsm0808_lcls_status lcls_bss_status;
292
293 /* more items are defined in the spec and may be added later */
294 bool more_items; /*< always set this to false */
295};
296 struct msgb *gsm0808_create_handover_complete(const struct gsm0808_handover_complete *params);
297
298 struct gsm0808_handover_failure {
299 uint16_t cause;
300
301 bool rr_cause_present;
302 uint8_t rr_cause;
303
304 struct gsm0808_speech_codec_list codec_list_bss_supported; /*< omit when .len == 0 */
305
306 /* more items are defined in the spec and may be added later */
307 bool more_items; /*< always set this to false */
308};
309 struct msgb *gsm0808_create_handover_failure(const struct gsm0808_handover_failure *params);
310
311 struct gsm0808_handover_performed {
312 uint16_t cause;
313 struct gsm0808_cell_id cell_id;
314
315 bool chosen_channel_present;
316 uint8_t chosen_channel;
317
318 bool chosen_encr_alg_present;
319 uint8_t chosen_encr_alg;
320
321 bool speech_version_chosen_present;
322 enum gsm0808_permitted_speech speech_version_chosen;
323
324 bool speech_codec_chosen_present;
325 struct gsm0808_speech_codec speech_codec_chosen;
326
327 bool lcls_bss_status_present;
328 enum gsm0808_lcls_status lcls_bss_status;
329
330 /* more items are defined in the spec and may be added later */
331 bool more_items; /*< always set this to false */
332};
333 struct msgb *gsm0808_create_handover_performed(const struct gsm0808_handover_performed *params);
334
336 struct gsm0808_vgcs_vbs_setup {
337 struct gsm0808_group_callref callref;
338
339 bool priority_present;
340 struct gsm0808_priority priority;
341
342 bool vgcs_feature_flags_present;
343 struct gsm0808_vgcs_feature_flags flags;
344};
345 struct msgb *gsm0808_create_vgcs_vbs_setup(const struct gsm0808_vgcs_vbs_setup *params);
346
348 struct gsm0808_vgcs_vbs_setup_ack {
349 bool vgcs_feature_flags_present;
350 struct gsm0808_vgcs_feature_flags flags;
351};
352 struct msgb *gsm0808_create_vgcs_vbs_setup_ack(const struct gsm0808_vgcs_vbs_setup_ack *params);
353
355 struct msgb *gsm0808_create_vgcs_vbs_setup_refuse(enum gsm0808_cause cause);
356
358 struct gsm0808_vgcs_vbs_assign_req {
359 struct gsm0808_channel_type channel_type;
360 enum gsm0808_assignment_requirement ass_req;
361 struct gsm0808_cell_id cell_identifier;
362 struct gsm0808_group_callref callref;
363
364 bool priority_present;
365 struct gsm0808_priority priority;
366
367 bool cic_present;
368 uint16_t cic;
369
370 bool downlink_dtx_flag_present;
371 enum gsm0808_downlink_dtx_flag downlink_dtx_flag;
372
373 bool encryption_information_present;
374 struct gsm0808_encrypt_info encryption_information;
375
376 bool vstk_rand_present;
377 uint8_t vstk_rand[5];
378
379 bool vstk_present;
380 uint8_t vstk[16];
381
382 bool cils_present;
383 struct gsm0808_cell_id_list_segment cils;
384
385 bool aoip_transport_layer_present;
386 struct sockaddr_storage aoip_transport_layer;
387
388 bool call_id_present;
389 uint32_t call_id;
390
391 bool codec_list_present;
392 struct gsm0808_speech_codec_list codec_list_msc_preferred;
393};
394 struct msgb *gsm0808_create_vgcs_vbs_assign_req(const struct gsm0808_vgcs_vbs_assign_req *params);
395
397 struct gsm0808_vgcs_vbs_assign_res {
398 struct gsm0808_channel_type channel_type;
399 struct gsm0808_cell_id cell_identifier;
400
401 bool chosen_channel_present;
402 uint8_t chosen_channel;
403
404 bool cic_present;
405 uint16_t cic;
406
407 bool circuit_pool_present;
408 uint8_t circuit_pool;
409
410 bool aoip_transport_layer_present;
411 struct sockaddr_storage aoip_transport_layer;
412
413 bool codec_present;
414 struct gsm0808_speech_codec codec_msc_chosen;
415
416 bool call_id_present;
417 uint32_t call_id;
418};
419 struct msgb *gsm0808_create_vgcs_vbs_assign_res(const struct gsm0808_vgcs_vbs_assign_res *params);
420
422 struct gsm0808_vgcs_vbs_assign_fail {
423 enum gsm0808_cause cause;
424
425 bool circuit_pool_present;
426 uint8_t circuit_pool;
427
428 bool cpl_present;
429 struct gsm0808_circuit_pool_list cpl;
430
431 bool codec_list_present;
432 struct gsm0808_speech_codec_list codec_list_bss_supported;
433};
434 struct msgb *gsm0808_create_vgcs_vbs_assign_fail(const struct gsm0808_vgcs_vbs_assign_fail *params);
435
437 struct gsm0808_uplink_request {
438 bool talker_priority_present;
439 enum gsm0808_talker_priority talker_priority;
440
441 bool cell_identifier_present;
442 struct gsm0808_cell_id cell_identifier;
443
444 bool l3_present;
445 struct gsm0808_layer_3_information l3;
446
447 bool mi_present;
448 struct osmo_mobile_identity mi;
449};
450 struct msgb *gsm0808_create_uplink_request(const struct gsm0808_uplink_request *params);
451
453 struct gsm0808_uplink_request_ack {
454 bool talker_priority_present;
455 enum gsm0808_talker_priority talker_priority;
456
457 bool emerg_set_ind_present;
458
459 bool talker_identity_present;
460 struct gsm0808_talker_identity talker_identity;
461};
462 struct msgb *gsm0808_create_uplink_request_ack(const struct gsm0808_uplink_request_ack *params);
463
465 struct gsm0808_uplink_request_cnf {
466 struct gsm0808_cell_id cell_identifier;
467
468 bool talker_identity_present;
469 struct gsm0808_talker_identity talker_identity;
470
471 /* mandatory! */
472 struct gsm0808_layer_3_information l3;
473};
474 struct msgb *gsm0808_create_uplink_request_cnf(const struct gsm0808_uplink_request_cnf *params);
475
477 struct gsm0808_uplink_app_data {
478 struct gsm0808_cell_id cell_identifier;
479 struct gsm0808_layer_3_information l3;
480 bool bt_ind;
481};
482 struct msgb *gsm0808_create_uplink_app_data(const struct gsm0808_uplink_app_data *params);
483
485 struct gsm0808_uplink_release_ind {
486 enum gsm0808_cause cause;
487
488 bool talker_priority_present;
489 enum gsm0808_talker_priority talker_priority;
490};
491 struct msgb *gsm0808_create_uplink_release_ind(const struct gsm0808_uplink_release_ind *params);
492
494 struct gsm0808_uplink_reject_cmd {
495 enum gsm0808_cause cause;
496
497 bool current_talker_priority_present;
498 enum gsm0808_talker_priority current_talker_priority;
499 bool rejected_talker_priority_present;
500 enum gsm0808_talker_priority rejected_talker_priority;
501
502 bool talker_identity_present;
503 struct gsm0808_talker_identity talker_identity;
504};
505 struct msgb *gsm0808_create_uplink_reject_cmd(const struct gsm0808_uplink_reject_cmd *params);
506
508 struct msgb *gsm0808_create_uplink_release_cmd(const enum gsm0808_cause cause);
509
511 struct gsm0808_uplink_seized_cmd {
512 enum gsm0808_cause cause;
513
514 bool talker_priority_present;
515 enum gsm0808_talker_priority talker_priority;
516
517 bool emerg_set_ind_present;
518
519 bool talker_identity_present;
520 struct gsm0808_talker_identity talker_identity;
521};
522 struct msgb *gsm0808_create_uplink_seized_cmd(const struct gsm0808_uplink_seized_cmd *params);
523
525 struct msgb *gsm0808_create_vgcs_additional_info(const struct gsm0808_talker_identity *ti);
526
528 struct gsm0808_vgcs_vbs_area_cell_info {
529 struct gsm0808_cell_id_list_segment cils;
530
531 bool ass_req_present;
532 enum gsm0808_assignment_requirement ass_req;
533};
534 struct msgb *gsm0808_create_vgcs_vbs_area_cell_info(const struct gsm0808_vgcs_vbs_area_cell_info *params);
535
537 struct gsm0808_vgcs_vbs_assign_stat {
538 /* established cells */
539 bool cils_est_present;
540 struct gsm0808_cell_id_list_segment cils_est;
541
542 /* cells to be established */
543 bool cils_tbe_present;
544 struct gsm0808_cell_id_list_segment cils_tbe;
545
546 /* released cells - no user present */
547 bool cils_rel_present;
548 struct gsm0808_cell_id_list_segment cils_rel;
549
550 /* not established cells - no establishment possible */
551 bool cils_ne_present;
552 struct gsm0808_cell_id_list_segment cils_ne;
553
554 bool cell_status_present;
555 enum gsm0808_vgcs_vbs_cell_status cell_status;
556};
557 struct msgb *gsm0808_create_vgcs_vbs_assign_stat(const struct gsm0808_vgcs_vbs_assign_stat *params);
558
560 struct msgb *gsm0808_create_vgcs_sms(const struct gsm0808_sms_to_vgcs *sms);
561
563 struct gsm0808_notification_data {
564 struct gsm0808_application_data app_data;
565 struct gsm0808_data_identity data_ident;
566
567 bool msisdn_present;
568 char msisdn[MSISDN_MAXLEN + 1];
569};
570 struct msgb *gsm0808_create_notification_data(const struct gsm0808_notification_data *parms);
571
572 struct msgb *gsm0808_create_dtap(struct msgb *msg, uint8_t link_id);
573 void gsm0808_prepend_dtap_header(struct msgb *msg, uint8_t link_id);
574
575 const struct tlv_definition *gsm0808_att_tlvdef(void);
576 extern const struct tlv_definition gsm0808_old_bss_to_new_bss_info_att_tlvdef;
577
579#define osmo_bssap_tlv_parse(dec, buf, len) tlv_parse(dec, gsm0808_att_tlvdef(), buf, len, 0, 0)
581#define osmo_bssap_tlv_parse2(dec, dec_multiples, buf, len) \
582 tlv_parse2(dec, dec_multiples, gsm0808_att_tlvdef(), buf, len, 0, 0)
583
584 const char *gsm0808_bssmap_name(uint8_t msg_type);
585 const char *gsm0808_bssap_name(uint8_t msg_type);
586 const char *gsm0808_cause_name(enum gsm0808_cause cause);
587 const char *gsm0808_cause_class_name(enum gsm0808_cause_class class);
588
591 enum gsm0808_cause gsm0808_get_cause(const struct tlv_parsed *tp);
592
593 const char *gsm0808_diagnostics_octet_location_str(uint8_t pointer);
594 const char *gsm0808_diagnostics_bit_location_str(uint8_t bit_pointer);
595
596 extern const struct value_string gsm0808_lcls_config_names[];
597 extern const struct value_string gsm0808_lcls_control_names[];
598 extern const struct value_string gsm0808_lcls_status_names[];
599
600 static inline const char *gsm0808_lcls_config_name(enum gsm0808_lcls_config val) {
601 return get_value_string(gsm0808_lcls_config_names, val);
602}
603 static inline const char *gsm0808_lcls_control_name(enum gsm0808_lcls_control val) {
604 return get_value_string(gsm0808_lcls_control_names, val);
605}
606 static inline const char *gsm0808_lcls_status_name(enum gsm0808_lcls_status val) {
607 return get_value_string(gsm0808_lcls_status_names, val);
608}
609
config
write Write running configuration to or terminal n Write configuration to the copy running config startup config
gsm0808_lcls_status_name
static const char * gsm0808_lcls_status_name(enum gsm0808_lcls_status val)
Definition: gsm0808.h:606
gsm0808_create_clear_rqst
struct msgb * gsm0808_create_clear_rqst(uint8_t cause)
Create BSSMAP Clear Request message.
Definition: gsm0808.c:746
gsm0808_create_handover_request_ack2
struct msgb * gsm0808_create_handover_request_ack2(const struct gsm0808_handover_request_ack *params)
Create BSSMAP HANDOVER REQUEST ACKNOWLEDGE message, 3GPP TS 48.008 3.2.1.10.
Definition: gsm0808.c:1055
gsm0808_create_reset
struct msgb * gsm0808_create_reset(void)
Create BSSMAP RESET message.
Definition: gsm0808.c:147
gsm0808_create_vgcs_vbs_assign_req
struct msgb * gsm0808_create_vgcs_vbs_assign_req(const struct gsm0808_vgcs_vbs_assign_req *params)
Create BSSMAP VGCS/VBS ASSIGNMENT REQUEST message, 3GPP TS 48.008 3.2.1.53.
Definition: gsm0808.c:1596
gsm0808_create_handover_request_ack
struct msgb * gsm0808_create_handover_request_ack(const uint8_t *l3_info, uint8_t l3_info_len, uint8_t chosen_channel, uint8_t chosen_encr_alg, uint8_t chosen_speech_version)
Same as gsm0808_create_handover_request_ack2() but with less parameters.
Definition: gsm0808.c:1108
gsm0808_create_common_id
struct msgb * gsm0808_create_common_id(const char *imsi, const struct osmo_plmn_id *selected_plmn_id, const struct osmo_plmn_id *last_used_eutran_plnm_id)
Create BSSMAP COMMON ID message, 3GPP TS 48.008 3.2.1.68.
Definition: gsm0808.c:1331
gsm0808_create_vgcs_vbs_assign_fail
struct msgb * gsm0808_create_vgcs_vbs_assign_fail(const struct gsm0808_vgcs_vbs_assign_fail *params)
Create BSSMAP VGCS/VBS ASSIGNMENT FAILURE message, 3GPP TS 48.008 3.2.1.55.
Definition: gsm0808.c:1736
gsm0808_create_cipher2
struct msgb * gsm0808_create_cipher2(const struct gsm0808_cipher_mode_command *cmc)
Create BSSMAP Cipher Mode Command message.
Definition: gsm0808.c:255
gsm0808_lcls_control_name
static const char * gsm0808_lcls_control_name(enum gsm0808_lcls_control val)
Definition: gsm0808.h:603
gsm0808_create_vgcs_vbs_setup
struct msgb * gsm0808_create_vgcs_vbs_setup(const struct gsm0808_vgcs_vbs_setup *params)
Create BSSMAP VGCS/VBS SETUP message, 3GPP TS 48.008 3.2.1.50.
Definition: gsm0808.c:1521
gsm0808_create_assignment_failure
struct msgb * gsm0808_create_assignment_failure(uint8_t cause, uint8_t *rr_cause)
Create BSSMAP Assignment Failure message.
Definition: gsm0808.c:737
gsm0808_diagnostics_octet_location_str
const char * gsm0808_diagnostics_octet_location_str(uint8_t pointer)
Definition: gsm0808.c:2626
gsm0808_create_handover_failure
struct msgb * gsm0808_create_handover_failure(const struct gsm0808_handover_failure *params)
Create BSSMAP HANDOVER FAILURE message, 3GPP TS 48.008 3.2.1.16.
Definition: gsm0808.c:1240
MSISDN_MAXLEN
#define MSISDN_MAXLEN
Parsed representation of a MSISDN IE (3GPP TS 48.008 3.2.2.101)
Definition: gsm0808_utils.h:223
gsm0808_create_vgcs_vbs_assign_res
struct msgb * gsm0808_create_vgcs_vbs_assign_res(const struct gsm0808_vgcs_vbs_assign_res *params)
Create BSSMAP VGCS/VBS ASSIGNMENT RESULT message, 3GPP TS 48.008 3.2.1.54.
Definition: gsm0808.c:1677
gsm0808_create_lcls_conn_ctrl
struct msgb * gsm0808_create_lcls_conn_ctrl(enum gsm0808_lcls_config config, enum gsm0808_lcls_control control)
Create BSSMAP LCLS CONNECT CONTROL message (TS 48.008 3.2.1.91).
Definition: gsm0808.c:367
gsm0808_create_layer3_aoip
struct msgb * gsm0808_create_layer3_aoip(const struct msgb *msg_l3, uint16_t nc, uint16_t cc, int lac, uint16_t _ci, const struct gsm0808_speech_codec_list *scl) OSMO_DEPRECATED("Use gsm0808_create_layer3_2() instead
Create "Complete L3 Info" for AoIP, legacy implementation.
Definition: gsm0808.c:52
gsm0808_create_layer3
struct msgb * gsm0808_create_layer3(struct msgb *msg_l3, uint16_t nc, uint16_t cc, int lac, uint16_t _ci) OSMO_DEPRECATED("Use gsm0808_create_layer3_2() instead
Create "Complete L3 Info" for A, legacy implementation.
Definition: gsm0808.c:129
gsm0808_create_handover_required
struct msgb * gsm0808_create_handover_required(const struct gsm0808_handover_required *params)
Create BSSMAP HANDOVER REQUIRED message.
Definition: gsm0808.c:886
gsm0808_create_handover_succeeded
struct msgb * gsm0808_create_handover_succeeded(void)
Create BSSMAP HANDOVER SUCCEEDED message, 3GPP TS 48.008 3.2.1.13.
Definition: gsm0808.c:1174
gsm0808_create_vgcs_sms
struct msgb * gsm0808_create_vgcs_sms(const struct gsm0808_sms_to_vgcs *sms)
3GPP TS 48.008 §3.2.1.81 VGCS SMS
Definition: gsm0808.c:2127
gsm0808_create_sapi_reject_cause
struct msgb * gsm0808_create_sapi_reject_cause(uint8_t link_id, uint16_t cause)
Create BSSMAP SAPI N Reject message.
Definition: gsm0808.c:470
gsm0808_bssmap_name
const char * gsm0808_bssmap_name(uint8_t msg_type)
Return string name of BSSMAP Message Type.
Definition: gsm0808.c:2461
gsm0808_lcls_config_name
static const char * gsm0808_lcls_config_name(enum gsm0808_lcls_config val)
Definition: gsm0808.h:600
gsm0808_att_tlvdef
const struct tlv_definition * gsm0808_att_tlvdef(void)
Definition: gsm0808.c:2320
gsm0808_create_cipher_reject
struct msgb * gsm0808_create_cipher_reject(enum gsm0808_cause cause)
Create BSSMAP Cipher Mode Reject message.
Definition: gsm0808.c:319
gsm0808_create_ass_compl
struct msgb * gsm0808_create_ass_compl(uint8_t rr_cause, uint8_t chosen_channel, uint8_t encr_alg_id, uint8_t speech_mode, const struct sockaddr_storage *ss, const struct gsm0808_speech_codec *sc, const struct gsm0808_speech_codec_list *scl)
Create BSSMAP Assignment Completed message.
Definition: gsm0808.c:668
gsm0808_create_classmark_update
struct msgb * gsm0808_create_classmark_update(const uint8_t *cm2, uint8_t cm2_len, const uint8_t *cm3, uint8_t cm3_len)
Create BSSMAP Classmark Update message.
Definition: gsm0808.c:447
gsm0808_create_uplink_release_cmd
struct msgb * gsm0808_create_uplink_release_cmd(const enum gsm0808_cause cause)
3GPP TS 48.008 §3.2.1.62 (VGCS) UPLINK RELEASE COMMAND
Definition: gsm0808.c:1984
gsm0808_create_vgcs_vbs_setup_ack
struct msgb * gsm0808_create_vgcs_vbs_setup_ack(const struct gsm0808_vgcs_vbs_setup_ack *params)
Create BSSMAP VGCS/VBS SETUP ACK message, 3GPP TS 48.008 3.2.1.51.
Definition: gsm0808.c:1551
gsm0808_vgcs_vbs_cell_status
gsm0808_vgcs_vbs_cell_status
Definition: gsm0808_utils.h:180
gsm0808_bssap_name
const char * gsm0808_bssap_name(uint8_t msg_type)
Return string name of BSSAP Message Type.
Definition: gsm0808.c:2473
gsm0808_create_ass2
struct msgb * gsm0808_create_ass2(const struct gsm0808_channel_type *ct, const uint16_t *cic, const struct sockaddr_storage *ss, const struct gsm0808_speech_codec_list *scl, const uint32_t *ci, const uint8_t *kc, const struct osmo_lcls *lcls)
Create BSSMAP Assignment Request message, 3GPP TS 48.008 §3.2.1.1.
Definition: gsm0808.c:506
gsm0808_talker_priority
gsm0808_talker_priority
Definition: gsm0808_utils.h:159
gsm0808_create_handover_detect
struct msgb * gsm0808_create_handover_detect(void)
Create BSSMAP HANDOVER DETECT message, 3GPP TS 48.008 3.2.1.40.
Definition: gsm0808.c:1155
gsm0808_create_vgcs_additional_info
struct msgb * gsm0808_create_vgcs_additional_info(const struct gsm0808_talker_identity *ti)
3GPP TS 48.008 §3.2.1.78 VGCS ADDITIONAL INFORMATION
Definition: gsm0808.c:2040
gsm0808_old_bss_to_new_bss_info_att_tlvdef
const struct tlv_definition gsm0808_old_bss_to_new_bss_info_att_tlvdef
Definition: gsm0808.c:2326
gsm0808_create_uplink_release_ind
struct msgb * gsm0808_create_uplink_release_ind(const struct gsm0808_uplink_release_ind *params)
Create BSSMAP (VGCS) UPLINK RELEASE INDICATION message, 3GPP TS 48.008 3.2.1.60.
Definition: gsm0808.c:1924
gsm0808_create_notification_data
struct msgb * gsm0808_create_notification_data(const struct gsm0808_notification_data *parms)
Create BSSMAP (VGCS/VBS) NOTIFICATION DATA message, 3GPP TS 48.008 3.2.1.82.
Definition: gsm0808.c:2146
gsm0808_create_ass_compl2
struct msgb * gsm0808_create_ass_compl2(uint8_t rr_cause, uint8_t chosen_channel, uint8_t encr_alg_id, uint8_t speech_mode, const struct sockaddr_storage *ss, const struct gsm0808_speech_codec *sc, const struct gsm0808_speech_codec_list *scl, enum gsm0808_lcls_status lcls_bss_status)
Create BSSMAP Assignment Completed message as per 3GPP TS 48.008 §3.2.1.2.
Definition: gsm0808.c:597
gsm0808_cause_name
const char * gsm0808_cause_name(enum gsm0808_cause cause)
Return string name of BSSMAP Cause name.
Definition: gsm0808.c:2605
MNC
struct msgb to not lose leading zeros in the MNC
Definition: gsm0808.h:39
gsm0808_lcls_config_names
const struct value_string gsm0808_lcls_config_names[]
Definition: gsm0808.c:2659
gsm0808_create_handover_command
struct msgb * gsm0808_create_handover_command(const struct gsm0808_handover_command *params)
Create BSSMAP HANDOVER COMMAND message, 3GPP TS 48.008 3.2.1.11.
Definition: gsm0808.c:1125
gsm0808_create_uplink_app_data
struct msgb * gsm0808_create_uplink_app_data(const struct gsm0808_uplink_app_data *params)
Create BSSMAP (VGCS) UPLINK APPLICATION DATA message, 3GPP TS 48.008 3.2.1.59a.
Definition: gsm0808.c:1894
gsm0808_create_uplink_request_cnf
struct msgb * gsm0808_create_uplink_request_cnf(const struct gsm0808_uplink_request_cnf *params)
Create BSSMAP (VGCS) UPLINK CONFIRM message, 3GPP TS 48.008 3.2.1.59.
Definition: gsm0808.c:1865
gsm0808_create_ass_fail
struct msgb * gsm0808_create_ass_fail(uint8_t cause, const uint8_t *rr_cause, const struct gsm0808_speech_codec_list *scl)
Create BSSMAP Assignment Failure message.
Definition: gsm0808.c:698
gsm0808_cause_class_name
const char * gsm0808_cause_class_name(enum gsm0808_cause_class class)
Return string name of BSSMAP Cause Class name.
Definition: gsm0808.c:2599
gsm0808_create_uplink_request_ack
struct msgb * gsm0808_create_uplink_request_ack(const struct gsm0808_uplink_request_ack *params)
Create BSSMAP (VGCS) UPLINK REQUEST ACKNOWLEDGE message, 3GPP TS 48.008 3.2.1.58.
Definition: gsm0808.c:1834
gsm0808_diagnostics_bit_location_str
const char * gsm0808_diagnostics_bit_location_str(uint8_t bit_pointer)
Definition: gsm0808.c:2645
gsm0808_create_classmark_request
struct msgb * gsm0808_create_classmark_request(void)
Create BSSMAP Classmark Request message.
Definition: gsm0808.c:429
gsm0808_create_cipher_reject_ext
struct msgb * gsm0808_create_cipher_reject_ext(enum gsm0808_cause_class class, uint8_t ext)
Create BSSMAP Cipher Mode Reject message.
Definition: gsm0808.c:339
gsm0808_create_paging
struct msgb * gsm0808_create_paging(const char *imsi, const uint32_t *tmsi, const struct gsm0808_cell_id_list *cil, const uint8_t *chan_needed) OSMO_DEPRECATED("use gsm0808_create_paging2 instead")
DEPRECATED: Use gsm0808_create_paging2 instead.
Definition: gsm0808.c:826
gsm0808_create_handover_request
struct msgb * gsm0808_create_handover_request(const struct gsm0808_handover_request *params)
Create BSSMAP HANDOVER REQUEST message, 3GPP TS 48.008 3.2.1.8.
Definition: gsm0808.c:946
gsm0808_create_vgcs_vbs_area_cell_info
struct msgb * gsm0808_create_vgcs_vbs_area_cell_info(const struct gsm0808_vgcs_vbs_area_cell_info *params)
Create BSSMAP VGCS/VBS AREA CELL INFO message, 3GPP TS 48.008 3.2.1.79.
Definition: gsm0808.c:2062
gsm0808_create_paging2
struct msgb * gsm0808_create_paging2(const char *imsi, const uint32_t *tmsi, const struct gsm0808_cell_id_list2 *cil, const uint8_t *chan_needed)
Create BSSMAP PAGING message.
Definition: gsm0808.c:768
gsm0808_get_cause
enum gsm0808_cause gsm0808_get_cause(const struct tlv_parsed *tp)
Parse Cause TLV 3GPP TS 08.08 §3.2.2.5.
Definition: gsm0808.c:2610
gsm0808_create_uplink_seized_cmd
struct msgb * gsm0808_create_uplink_seized_cmd(const struct gsm0808_uplink_seized_cmd *params)
Create BSSMAP (VGCS) UPLINK SEIZED COMMAND message, 3GPP TS 48.008 3.2.1.62.
Definition: gsm0808.c:2006
gsm0808_create_handover_performed
struct msgb * gsm0808_create_handover_performed(const struct gsm0808_handover_performed *params)
Create BSSMAP HANDOVER PERFORMED message, 3GPP TS 48.008 3.2.1.25.
Definition: gsm0808.c:1277
gsm0808_prepend_dtap_header
void gsm0808_prepend_dtap_header(struct msgb *msg, uint8_t link_id)
Prepend a DTAP header to given Message Buffer.
Definition: gsm0808.c:1384
gsm0808_lcls_control_names
const struct value_string gsm0808_lcls_control_names[]
Definition: gsm0808.c:2675
gsm0808_create_handover_complete
struct msgb * gsm0808_create_handover_complete(const struct gsm0808_handover_complete *params)
Create BSSMAP HANDOVER COMPLETE message, 3GPP TS 48.008 3.2.1.12.
Definition: gsm0808.c:1193
gsm0808_create_clear_command2
struct msgb * gsm0808_create_clear_command2(uint8_t cause, bool csfb_ind)
Create BSSMAP Clear Command message.
Definition: gsm0808.c:217
gsm0808_create_sapi_reject
struct msgb * gsm0808_create_sapi_reject(uint8_t link_id) OSMO_DEPRECATED("Use gsm0808_create_sapi_reject_cause() instead")
Create BSSMAP SAPI N Reject message (with hard-coded cause "BSS not equipped").
Definition: gsm0808.c:491
gsm0808_create_vgcs_vbs_assign_stat
struct msgb * gsm0808_create_vgcs_vbs_assign_stat(const struct gsm0808_vgcs_vbs_assign_stat *params)
Create BSSMAP VGCS/VBS ASSIGNMENT STATUS message, 3GPP TS 48.008 3.2.1.80.
Definition: gsm0808.c:2088
gsm0808_downlink_dtx_flag
gsm0808_downlink_dtx_flag
Definition: gsm0808_utils.h:139
gsm0808_create_vgcs_vbs_setup_refuse
struct msgb * gsm0808_create_vgcs_vbs_setup_refuse(enum gsm0808_cause cause)
3GPP TS 48.008 §3.2.1.52 VGCS/VBS SETUP REFUSE
Definition: gsm0808.c:1574
gsm0808_create_handover_required_reject
struct msgb * gsm0808_create_handover_required_reject(const struct gsm0808_handover_required_reject *params)
Create BSSMAP HANDOVER REQUIRED REJECT message.
Definition: gsm0808.c:922
gsm0808_create_uplink_reject_cmd
struct msgb * gsm0808_create_uplink_reject_cmd(const struct gsm0808_uplink_reject_cmd *params)
Create BSSMAP (VGCS) UPLINK REJECT COMMAND message, 3GPP TS 48.008 3.2.1.61.
Definition: gsm0808.c:1950
gsm0808_create_cipher_complete
struct msgb * gsm0808_create_cipher_complete(struct msgb *layer3, uint8_t alg_id)
Create BSSMAP Cipher Mode Complete message.
Definition: gsm0808.c:290
gsm0808_assignment_requirement
gsm0808_assignment_requirement
Definition: gsm0808_utils.h:97
gsm0808_create_clear_complete
struct msgb * gsm0808_create_clear_complete(void)
Create BSSMAP Clear Complete message.
Definition: gsm0808.c:179
gsm0808_create_assignment_completed
struct msgb * gsm0808_create_assignment_completed(uint8_t rr_cause, uint8_t chosen_channel, uint8_t encr_alg_id, uint8_t speech_mode)
Create BSSMAP Assignment Completed message.
Definition: gsm0808.c:684
gsm0808_create_ass
struct msgb * gsm0808_create_ass(const struct gsm0808_channel_type *ct, const uint16_t *cic, const struct sockaddr_storage *ss, const struct gsm0808_speech_codec_list *scl, const uint32_t *ci)
Create BSSMAP Assignment Request message, 3GPP TS 48.008 §3.2.1.1.
Definition: gsm0808.c:578
gsm0808_create_layer3_2
struct msgb * gsm0808_create_layer3_2(const struct msgb *msg_l3, const struct osmo_cell_global_id *cell, const struct gsm0808_speech_codec_list *scl)
Create "Complete L3 Info" for AoIP.
Definition: gsm0808.c:75
gsm0808_create_uplink_request
struct msgb * gsm0808_create_uplink_request(const struct gsm0808_uplink_request *params)
Create BSSMAP (VGCS) UPLINK REQUEST message, 3GPP TS 48.008 3.2.1.57.
Definition: gsm0808.c:1793
gsm0808_lcls_status_names
const struct value_string gsm0808_lcls_status_names[]
Definition: gsm0808.c:2685
gsm0808_create_cipher
struct msgb * gsm0808_create_cipher(const struct gsm0808_encrypt_info *ei, const uint8_t *cipher_response_mode)
Superseded by gsm0808_create_cipher2() to include Kc128.
Definition: gsm0808.c:241
gsm0808_create_lcls_notification
struct msgb * gsm0808_create_lcls_notification(enum gsm0808_lcls_status status, bool break_req)
Create BSSMAP LCLS NOTIFICATION message (TS 48.008 3.2.1.93).
Definition: gsm0808.c:411
gsm0808_create_lcls_conn_ctrl_ack
struct msgb * gsm0808_create_lcls_conn_ctrl_ack(enum gsm0808_lcls_status status)
Create BSSMAP LCLS CONNECT CONTROL ACK message (TS 48.008 3.2.1.92).
Definition: gsm0808.c:393
gsm0808_create_dtap
struct msgb * gsm0808_create_dtap(struct msgb *msg, uint8_t link_id)
Create BSSMAP DTAP message.
Definition: gsm0808.c:1396
gsm0808_create_clear_command
struct msgb * gsm0808_create_clear_command(uint8_t cause)
Create BSSMAP Clear Command message with BSSAP header before l3h and BSSMAP in l3h.
Definition: gsm0808.c:199
gsm0808_create_reset_ack
struct msgb * gsm0808_create_reset_ack(void)
Create BSSMAP RESET ACK message.
Definition: gsm0808.c:164
OSMO_DEPRECATED
#define OSMO_DEPRECATED(text)
get_value_string
const char * get_value_string(const struct value_string *vs, uint32_t val)
gsm0808_utils.h
gsm23003.h
cause
uint8_t cause
Definition: gsm_04_08.h:2
cm2_len
uint8_t cm2_len
Definition: gsm_04_08.h:0
lac
uint16_t lac
Definition: gsm_04_08.h:1
cm2
struct gsm48_classmark2 cm2
Definition: gsm_04_08.h:1
rr_cause
uint8_t rr_cause
Definition: gsm_04_08.h:0
msg_type
uint8_t msg_type
Definition: gsm_04_08.h:2
gsm_08_08.h
gsm0808_cause
gsm0808_cause
Definition: gsm_08_08.h:367
msg
uint8_t msg[0]
Definition: gsm_08_08.h:8
gsm0808_lcls_status
gsm0808_lcls_status
Definition: gsm_08_08.h:803
gsm0808_cause_class
gsm0808_cause_class
Definition: gsm_08_08.h:434
gsm0808_lcls_control
gsm0808_lcls_control
Definition: gsm_08_08.h:793
gsm0808_lcls_config
gsm0808_lcls_config
Definition: gsm_08_08.h:782
gsm0808_permitted_speech
gsm0808_permitted_speech
GSM 08.08 3.2.2.11 Channel Type (see also 3GPP TS 48.008, section 3.2.2.11)
Definition: gsm_08_08.h:494
link_id
uint8_t link_id
Definition: gsm_08_08.h:2
params
uint8_t params[0]
Definition: gsm_08_58.h:6
gsm_23_003.h
instead
_parse instead
Definition: ipa.h:30
socket_compat.h
gsm0808_application_data
Definition: gsm0808_utils.h:196
gsm0808_cell_id_list2
Parsed representation of a Cell Identifier List IE (3GPP TS 48.008 3.2.2.27).
Definition: gsm0808_utils.h:61
gsm0808_cell_id_list_segment
Parsed representation of a Cell Identifier List Segment IE (3GPP TS 48.008 3.2.2.27a)
Definition: gsm0808_utils.h:145
gsm0808_cell_id_list
DEPRECATED: This definition of the cell identifier list is insufficient.
Definition: gsm_08_08.h:775
gsm0808_cell_id
Parsed representation of Cell Identifier IE (3GPP TS 48.008 3.2.2.17)
Definition: gsm0808_utils.h:55
gsm0808_channel_type
Definition: gsm_08_08.h:741
gsm0808_cipher_mode_command
Definition: gsm0808.h:54
gsm0808_cipher_mode_command::cipher_response_mode_present
bool cipher_response_mode_present
3GPP TS 48.008 3.2.2.34 Cipher Response Mode, optional IE
Definition: gsm0808.h:58
gsm0808_cipher_mode_command::cipher_response_mode
uint8_t cipher_response_mode
3GPP TS 48.008 3.2.2.34 Cipher Response Mode: 0 - IMEISV must not be included by the Mobile Station; ...
Definition: gsm0808.h:63
gsm0808_cipher_mode_command::kc128_present
bool kc128_present
Definition: gsm0808.h:65
gsm0808_cipher_mode_command::more_items
bool more_items
Definition: gsm0808.h:69
gsm0808_circuit_pool_list
Definition: gsm0808_utils.h:153
gsm0808_data_identity
Definition: gsm0808_utils.h:211
gsm0808_encrypt_info
Definition: gsm_08_08.h:761
gsm0808_group_callref
Packed representation of a Group Call Reference IE (3GPP TS 48.008 3.2.2.55)
Definition: gsm0808_utils.h:121
gsm0808_handover_command
Definition: gsm0808.h:258
gsm0808_handover_command::new_bss_to_old_bss_info_raw
const uint8_t * new_bss_to_old_bss_info_raw
Definition: gsm0808.h:264
gsm0808_handover_command::more_items
bool more_items
always set this to false
Definition: gsm0808.h:268
gsm0808_handover_command::l3_info_len
uint8_t l3_info_len
Definition: gsm0808.h:260
gsm0808_handover_command::l3_info
const uint8_t * l3_info
Definition: gsm0808.h:259
gsm0808_handover_command::new_bss_to_old_bss_info_raw_len
size_t new_bss_to_old_bss_info_raw_len
Definition: gsm0808.h:265
gsm0808_handover_command::cell_identifier
struct gsm0808_cell_id cell_identifier
Definition: gsm0808.h:262
gsm0808_handover_complete
Definition: gsm0808.h:275
gsm0808_handover_complete::rr_cause
uint8_t rr_cause
Definition: gsm0808.h:277
gsm0808_handover_complete::lcls_bss_status_present
bool lcls_bss_status_present
Definition: gsm0808.h:290
gsm0808_handover_complete::lcls_bss_status
enum gsm0808_lcls_status lcls_bss_status
Definition: gsm0808.h:291
gsm0808_handover_complete::rr_cause_present
bool rr_cause_present
Definition: gsm0808.h:276
gsm0808_handover_complete::chosen_encr_alg
uint8_t chosen_encr_alg
Definition: gsm0808.h:285
gsm0808_handover_complete::speech_codec_chosen
struct gsm0808_speech_codec speech_codec_chosen
Definition: gsm0808.h:280
gsm0808_handover_complete::codec_list_bss_supported
struct gsm0808_speech_codec_list codec_list_bss_supported
Definition: gsm0808.h:282
gsm0808_handover_complete::chosen_channel
uint8_t chosen_channel
Definition: gsm0808.h:288
gsm0808_handover_complete::chosen_channel_present
bool chosen_channel_present
Definition: gsm0808.h:287
gsm0808_handover_complete::speech_codec_chosen_present
bool speech_codec_chosen_present
Definition: gsm0808.h:279
gsm0808_handover_complete::more_items
bool more_items
Definition: gsm0808.h:294
gsm0808_handover_complete::chosen_encr_alg_present
bool chosen_encr_alg_present
Definition: gsm0808.h:284
gsm0808_handover_failure
Definition: gsm0808.h:298
gsm0808_handover_failure::rr_cause_present
bool rr_cause_present
Definition: gsm0808.h:301
gsm0808_handover_failure::codec_list_bss_supported
struct gsm0808_speech_codec_list codec_list_bss_supported
Definition: gsm0808.h:304
gsm0808_handover_failure::more_items
bool more_items
Definition: gsm0808.h:307
gsm0808_handover_failure::cause
uint16_t cause
Definition: gsm0808.h:299
gsm0808_handover_failure::rr_cause
uint8_t rr_cause
Definition: gsm0808.h:302
gsm0808_handover_performed
Definition: gsm0808.h:311
gsm0808_handover_performed::speech_version_chosen
enum gsm0808_permitted_speech speech_version_chosen
Definition: gsm0808.h:322
gsm0808_handover_performed::chosen_encr_alg_present
bool chosen_encr_alg_present
Definition: gsm0808.h:318
gsm0808_handover_performed::speech_codec_chosen
struct gsm0808_speech_codec speech_codec_chosen
Definition: gsm0808.h:325
gsm0808_handover_performed::cause
uint16_t cause
Definition: gsm0808.h:312
gsm0808_handover_performed::lcls_bss_status
enum gsm0808_lcls_status lcls_bss_status
Definition: gsm0808.h:328
gsm0808_handover_performed::speech_codec_chosen_present
bool speech_codec_chosen_present
Definition: gsm0808.h:324
gsm0808_handover_performed::speech_version_chosen_present
bool speech_version_chosen_present
Definition: gsm0808.h:321
gsm0808_handover_performed::chosen_encr_alg
uint8_t chosen_encr_alg
Definition: gsm0808.h:319
gsm0808_handover_performed::lcls_bss_status_present
bool lcls_bss_status_present
Definition: gsm0808.h:327
gsm0808_handover_performed::cell_id
struct gsm0808_cell_id cell_id
Definition: gsm0808.h:313
gsm0808_handover_performed::chosen_channel
uint8_t chosen_channel
Definition: gsm0808.h:316
gsm0808_handover_performed::chosen_channel_present
bool chosen_channel_present
Definition: gsm0808.h:315
gsm0808_handover_performed::more_items
bool more_items
Definition: gsm0808.h:331
gsm0808_handover_request_ack
Definition: gsm0808.h:230
gsm0808_handover_request_ack::l3_info_len
uint8_t l3_info_len
Definition: gsm0808.h:232
gsm0808_handover_request_ack::speech_codec_chosen_present
bool speech_codec_chosen_present
Definition: gsm0808.h:244
gsm0808_handover_request_ack::more_items2
bool more_items2
always set this to false
Definition: gsm0808.h:254
gsm0808_handover_request_ack::codec_list_bss_supported
struct gsm0808_speech_codec_list codec_list_bss_supported
Definition: gsm0808.h:251
gsm0808_handover_request_ack::chosen_speech_version
enum gsm0808_permitted_speech chosen_speech_version
Definition: gsm0808.h:242
gsm0808_handover_request_ack::more_items
bool more_items
set this to true iff any fields below are used
Definition: gsm0808.h:249
gsm0808_handover_request_ack::speech_codec_chosen
struct gsm0808_speech_codec speech_codec_chosen
Definition: gsm0808.h:245
gsm0808_handover_request_ack::aoip_transport_layer
const struct sockaddr_storage * aoip_transport_layer
Definition: gsm0808.h:247
gsm0808_handover_request_ack::chosen_channel
uint8_t chosen_channel
Definition: gsm0808.h:235
gsm0808_handover_request_ack::l3_info
const uint8_t * l3_info
Definition: gsm0808.h:231
gsm0808_handover_request_ack::chosen_channel_present
bool chosen_channel_present
Definition: gsm0808.h:234
gsm0808_handover_request_ack::chosen_encr_alg
uint8_t chosen_encr_alg
For A5/N set chosen_encr_alg = N+1, e.g.
Definition: gsm0808.h:239
gsm0808_handover_request
3GPP TS 48.008 §3.2.1.8 HANDOVER REQUEST
Definition: gsm0808.h:181
gsm0808_handover_request::current_channel_type_1
uint8_t current_channel_type_1
Definition: gsm0808.h:190
gsm0808_handover_request::cell_identifier_serving
struct gsm0808_cell_id cell_identifier_serving
Definition: gsm0808.h:185
gsm0808_handover_request::more_items2
bool more_items2
always set this to false
Definition: gsm0808.h:222
gsm0808_handover_request::current_channel_type_1_present
bool current_channel_type_1_present
Definition: gsm0808.h:189
gsm0808_handover_request::old_bss_to_new_bss_info_raw_len
uint8_t old_bss_to_new_bss_info_raw_len
Definition: gsm0808.h:202
gsm0808_handover_request::global_call_reference_len
uint8_t global_call_reference_len
Definition: gsm0808.h:214
gsm0808_handover_request::old_bss_to_new_bss_info_present
bool old_bss_to_new_bss_info_present
Pass either old_bss_to_new_bss_info or old_bss_to_new_bss_info_raw.
Definition: gsm0808.h:197
gsm0808_handover_request::chosen_encryption_algorithm_serving
uint8_t chosen_encryption_algorithm_serving
Definition: gsm0808.h:194
gsm0808_handover_request::imsi
const char * imsi
Definition: gsm0808.h:204
gsm0808_handover_request::cell_identifier_target
struct gsm0808_cell_id cell_identifier_target
Definition: gsm0808.h:186
gsm0808_handover_request::cause
enum gsm0808_cause cause
Definition: gsm0808.h:187
gsm0808_handover_request::aoip_transport_layer
const struct sockaddr_storage * aoip_transport_layer
Definition: gsm0808.h:206
gsm0808_handover_request::speech_version_used
enum gsm0808_permitted_speech speech_version_used
Definition: gsm0808.h:192
gsm0808_handover_request::global_call_reference
const uint8_t * global_call_reference
Definition: gsm0808.h:213
gsm0808_handover_request::channel_type
struct gsm0808_channel_type channel_type
Definition: gsm0808.h:182
gsm0808_handover_request::codec_list_msc_preferred
const struct gsm0808_speech_codec_list * codec_list_msc_preferred
Definition: gsm0808.h:208
gsm0808_handover_request::encryption_information
struct gsm0808_encrypt_info encryption_information
Definition: gsm0808.h:183
gsm0808_handover_request::kc128
uint8_t kc128[16]
Definition: gsm0808.h:220
gsm0808_handover_request::old_bss_to_new_bss_info_raw
const uint8_t * old_bss_to_new_bss_info_raw
To feed the Old BSS to New BSS Information IE unchanged from the Handover Required message without ha...
Definition: gsm0808.h:201
gsm0808_handover_request::old_bss_to_new_bss_info
struct gsm0808_old_bss_to_new_bss_info old_bss_to_new_bss_info
Definition: gsm0808.h:198
gsm0808_handover_request::classmark_information
struct osmo_gsm48_classmark classmark_information
Definition: gsm0808.h:184
gsm0808_handover_request::kc128_present
bool kc128_present
Definition: gsm0808.h:219
gsm0808_handover_request::call_id
uint32_t call_id
Definition: gsm0808.h:211
gsm0808_handover_request::more_items
bool more_items
set this to true iff any fields below are used
Definition: gsm0808.h:217
gsm0808_handover_request::call_id_present
bool call_id_present
Definition: gsm0808.h:210
gsm0808_handover_required_reject
3GPP TS 48.008 §3.2.1.37 HANDOVER REQUIRED REJECT
Definition: gsm0808.h:172
gsm0808_handover_required_reject::more_items
bool more_items
Definition: gsm0808.h:176
gsm0808_handover_required_reject::cause
uint16_t cause
Definition: gsm0808.h:173
gsm0808_handover_required
3GPP TS 48.008 §3.2.1.9 HANDOVER REQUIRED
Definition: gsm0808.h:153
gsm0808_handover_required::cil
struct gsm0808_cell_id_list2 cil
Definition: gsm0808.h:155
gsm0808_handover_required::more_items
bool more_items
Definition: gsm0808.h:167
gsm0808_handover_required::cause
uint16_t cause
Definition: gsm0808.h:154
gsm0808_handover_required::current_channel_type_1_present
bool current_channel_type_1_present
Definition: gsm0808.h:157
gsm0808_handover_required::speech_version_used_present
bool speech_version_used_present
Definition: gsm0808.h:160
gsm0808_handover_required::old_bss_to_new_bss_info_present
bool old_bss_to_new_bss_info_present
Definition: gsm0808.h:163
gsm0808_handover_required::current_channel_type_1
uint8_t current_channel_type_1
Definition: gsm0808.h:158
gsm0808_handover_required::old_bss_to_new_bss_info
struct gsm0808_old_bss_to_new_bss_info old_bss_to_new_bss_info
Definition: gsm0808.h:164
gsm0808_handover_required::speech_version_used
enum gsm0808_permitted_speech speech_version_used
Definition: gsm0808.h:161
gsm0808_layer_3_information
Definition: gsm0808_utils.h:167
gsm0808_notification_data
3GPP TS 48.008 §3.2.1.82 (VGCS/VBS) NOTIFICATION DATA
Definition: gsm0808.h:563
gsm0808_notification_data::data_ident
struct gsm0808_data_identity data_ident
Definition: gsm0808.h:565
gsm0808_notification_data::msisdn
char msisdn[MSISDN_MAXLEN+1]
Definition: gsm0808.h:568
gsm0808_notification_data::app_data
struct gsm0808_application_data app_data
Definition: gsm0808.h:564
gsm0808_notification_data::msisdn_present
bool msisdn_present
Definition: gsm0808.h:567
gsm0808_old_bss_to_new_bss_info
3GPP TS 48.008 §3.2.2.5.8 Old BSS to New BSS information
Definition: gsm0808.h:131
gsm0808_old_bss_to_new_bss_info::extra_information_present
bool extra_information_present
Definition: gsm0808.h:132
gsm0808_old_bss_to_new_bss_info::last_eutran_plmn_id_present
bool last_eutran_plmn_id_present
Definition: gsm0808.h:145
gsm0808_old_bss_to_new_bss_info::current_channel_type_2
struct gsm0808_old_bss_to_new_bss_info::@7 current_channel_type_2
gsm0808_old_bss_to_new_bss_info::field
uint8_t field
Definition: gsm0808.h:142
gsm0808_old_bss_to_new_bss_info::current_channel_type_2_present
bool current_channel_type_2_present
Definition: gsm0808.h:139
gsm0808_old_bss_to_new_bss_info::mode
uint8_t mode
Definition: gsm0808.h:141
gsm0808_old_bss_to_new_bss_info::extra_information
struct gsm0808_old_bss_to_new_bss_info::@6 extra_information
gsm0808_old_bss_to_new_bss_info::last_eutran_plmn_id
struct osmo_plmn_id last_eutran_plmn_id
Definition: gsm0808.h:146
gsm0808_old_bss_to_new_bss_info::lcs
bool lcs
Definition: gsm0808.h:135
gsm0808_old_bss_to_new_bss_info::ue_prob
bool ue_prob
Definition: gsm0808.h:136
gsm0808_old_bss_to_new_bss_info::prec
bool prec
Definition: gsm0808.h:134
gsm0808_old_bss_to_new_bss_info::more_items
bool more_items
Definition: gsm0808.h:149
gsm0808_priority
Packed representation of a Priority IE (GGPP TS 48.008 3.2.2.18)
Definition: gsm0808_utils.h:68
gsm0808_sms_to_vgcs
Definition: gsm0808_utils.h:189
gsm0808_speech_codec_list
Definition: gsm_08_08.h:725
gsm0808_speech_codec
3GPP TS 48.008 3.2.2.104 Speech Codec.
Definition: gsm_08_08.h:593
gsm0808_talker_identity
Definition: gsm0808_utils.h:174
gsm0808_uplink_app_data
3GPP TS 48.008 §3.2.1.59a (VGCS) UPLINK APPLICATION DATA
Definition: gsm0808.h:477
gsm0808_uplink_app_data::cell_identifier
struct gsm0808_cell_id cell_identifier
Definition: gsm0808.h:478
gsm0808_uplink_app_data::l3
struct gsm0808_layer_3_information l3
Definition: gsm0808.h:479
gsm0808_uplink_app_data::bt_ind
bool bt_ind
Definition: gsm0808.h:480
gsm0808_uplink_reject_cmd
3GPP TS 48.008 §3.2.1.61 (VGCS) UPLINK REJECT COMMAND
Definition: gsm0808.h:494
gsm0808_uplink_reject_cmd::cause
enum gsm0808_cause cause
Definition: gsm0808.h:495
gsm0808_uplink_reject_cmd::talker_identity_present
bool talker_identity_present
Definition: gsm0808.h:502
gsm0808_uplink_reject_cmd::talker_identity
struct gsm0808_talker_identity talker_identity
Definition: gsm0808.h:503
gsm0808_uplink_reject_cmd::rejected_talker_priority
enum gsm0808_talker_priority rejected_talker_priority
Definition: gsm0808.h:500
gsm0808_uplink_reject_cmd::current_talker_priority
enum gsm0808_talker_priority current_talker_priority
Definition: gsm0808.h:498
gsm0808_uplink_reject_cmd::current_talker_priority_present
bool current_talker_priority_present
Definition: gsm0808.h:497
gsm0808_uplink_reject_cmd::rejected_talker_priority_present
bool rejected_talker_priority_present
Definition: gsm0808.h:499
gsm0808_uplink_release_ind
3GPP TS 48.008 §3.2.1.60 (VGCS) UPLINK RELEASE INDICATION
Definition: gsm0808.h:485
gsm0808_uplink_release_ind::cause
enum gsm0808_cause cause
Definition: gsm0808.h:486
gsm0808_uplink_release_ind::talker_priority
enum gsm0808_talker_priority talker_priority
Definition: gsm0808.h:489
gsm0808_uplink_release_ind::talker_priority_present
bool talker_priority_present
Definition: gsm0808.h:488
gsm0808_uplink_request_ack
3GPP TS 48.008 §3.2.1.58 (VGCS) UPLINK REQUEST ACKNOWLEDGE
Definition: gsm0808.h:453
gsm0808_uplink_request_ack::emerg_set_ind_present
bool emerg_set_ind_present
Definition: gsm0808.h:457
gsm0808_uplink_request_ack::talker_identity_present
bool talker_identity_present
Definition: gsm0808.h:459
gsm0808_uplink_request_ack::talker_identity
struct gsm0808_talker_identity talker_identity
Definition: gsm0808.h:460
gsm0808_uplink_request_ack::talker_priority
enum gsm0808_talker_priority talker_priority
Definition: gsm0808.h:455
gsm0808_uplink_request_ack::talker_priority_present
bool talker_priority_present
Definition: gsm0808.h:454
gsm0808_uplink_request_cnf
3GPP TS 48.008 §3.2.1.59 (VGCS) UPLINK REQUEST CONFIRM
Definition: gsm0808.h:465
gsm0808_uplink_request_cnf::talker_identity
struct gsm0808_talker_identity talker_identity
Definition: gsm0808.h:469
gsm0808_uplink_request_cnf::cell_identifier
struct gsm0808_cell_id cell_identifier
Definition: gsm0808.h:466
gsm0808_uplink_request_cnf::l3
struct gsm0808_layer_3_information l3
Definition: gsm0808.h:472
gsm0808_uplink_request_cnf::talker_identity_present
bool talker_identity_present
Definition: gsm0808.h:468
gsm0808_uplink_request
3GPP TS 48.008 §3.2.1.57 (VGCS) UPLINK REQUEST
Definition: gsm0808.h:437
gsm0808_uplink_request::talker_priority_present
bool talker_priority_present
Definition: gsm0808.h:438
gsm0808_uplink_request::l3_present
bool l3_present
Definition: gsm0808.h:444
gsm0808_uplink_request::mi
struct osmo_mobile_identity mi
Definition: gsm0808.h:448
gsm0808_uplink_request::mi_present
bool mi_present
Definition: gsm0808.h:447
gsm0808_uplink_request::cell_identifier_present
bool cell_identifier_present
Definition: gsm0808.h:441
gsm0808_uplink_request::talker_priority
enum gsm0808_talker_priority talker_priority
Definition: gsm0808.h:439
gsm0808_uplink_request::cell_identifier
struct gsm0808_cell_id cell_identifier
Definition: gsm0808.h:442
gsm0808_uplink_request::l3
struct gsm0808_layer_3_information l3
Definition: gsm0808.h:445
gsm0808_uplink_seized_cmd
3GPP TS 48.008 §3.2.1.63 (VGCS) UPLINK SEIZED COMMAND
Definition: gsm0808.h:511
gsm0808_uplink_seized_cmd::emerg_set_ind_present
bool emerg_set_ind_present
Definition: gsm0808.h:517
gsm0808_uplink_seized_cmd::talker_identity
struct gsm0808_talker_identity talker_identity
Definition: gsm0808.h:520
gsm0808_uplink_seized_cmd::cause
enum gsm0808_cause cause
Definition: gsm0808.h:512
gsm0808_uplink_seized_cmd::talker_identity_present
bool talker_identity_present
Definition: gsm0808.h:519
gsm0808_uplink_seized_cmd::talker_priority_present
bool talker_priority_present
Definition: gsm0808.h:514
gsm0808_uplink_seized_cmd::talker_priority
enum gsm0808_talker_priority talker_priority
Definition: gsm0808.h:515
gsm0808_vgcs_feature_flags
Packed representation of a VGCS Feature Flags IE (3GPP TS 48.008 3.2.2.88)
Definition: gsm0808_utils.h:82
gsm0808_vgcs_vbs_area_cell_info
3GPP TS 48.008 §3.2.1.79 VGCS/VBS AREA CELL INFO
Definition: gsm0808.h:528
gsm0808_vgcs_vbs_area_cell_info::ass_req
enum gsm0808_assignment_requirement ass_req
Definition: gsm0808.h:532
gsm0808_vgcs_vbs_area_cell_info::cils
struct gsm0808_cell_id_list_segment cils
Definition: gsm0808.h:529
gsm0808_vgcs_vbs_area_cell_info::ass_req_present
bool ass_req_present
Definition: gsm0808.h:531
gsm0808_vgcs_vbs_assign_fail
3GPP TS 48.008 §3.2.1.55 VGCS/VBS ASSIGNMENT FAILURE
Definition: gsm0808.h:422
gsm0808_vgcs_vbs_assign_fail::cpl
struct gsm0808_circuit_pool_list cpl
Definition: gsm0808.h:429
gsm0808_vgcs_vbs_assign_fail::codec_list_bss_supported
struct gsm0808_speech_codec_list codec_list_bss_supported
Definition: gsm0808.h:432
gsm0808_vgcs_vbs_assign_fail::cpl_present
bool cpl_present
Definition: gsm0808.h:428
gsm0808_vgcs_vbs_assign_fail::circuit_pool
uint8_t circuit_pool
Definition: gsm0808.h:426
gsm0808_vgcs_vbs_assign_fail::codec_list_present
bool codec_list_present
Definition: gsm0808.h:431
gsm0808_vgcs_vbs_assign_fail::circuit_pool_present
bool circuit_pool_present
Definition: gsm0808.h:425
gsm0808_vgcs_vbs_assign_fail::cause
enum gsm0808_cause cause
Definition: gsm0808.h:423
gsm0808_vgcs_vbs_assign_req
3GPP TS 48.008 §3.2.1.53 VGCS/VBS ASSIGNMENT REQUEST
Definition: gsm0808.h:358
gsm0808_vgcs_vbs_assign_req::encryption_information
struct gsm0808_encrypt_info encryption_information
Definition: gsm0808.h:374
gsm0808_vgcs_vbs_assign_req::aoip_transport_layer
struct sockaddr_storage aoip_transport_layer
Definition: gsm0808.h:386
gsm0808_vgcs_vbs_assign_req::encryption_information_present
bool encryption_information_present
Definition: gsm0808.h:373
gsm0808_vgcs_vbs_assign_req::vstk_rand_present
bool vstk_rand_present
Definition: gsm0808.h:376
gsm0808_vgcs_vbs_assign_req::channel_type
struct gsm0808_channel_type channel_type
Definition: gsm0808.h:359
gsm0808_vgcs_vbs_assign_req::aoip_transport_layer_present
bool aoip_transport_layer_present
Definition: gsm0808.h:385
gsm0808_vgcs_vbs_assign_req::priority
struct gsm0808_priority priority
Definition: gsm0808.h:365
gsm0808_vgcs_vbs_assign_req::callref
struct gsm0808_group_callref callref
Definition: gsm0808.h:362
gsm0808_vgcs_vbs_assign_req::ass_req
enum gsm0808_assignment_requirement ass_req
Definition: gsm0808.h:360
gsm0808_vgcs_vbs_assign_req::cils_present
bool cils_present
Definition: gsm0808.h:382
gsm0808_vgcs_vbs_assign_req::cell_identifier
struct gsm0808_cell_id cell_identifier
Definition: gsm0808.h:361
gsm0808_vgcs_vbs_assign_req::cic_present
bool cic_present
Definition: gsm0808.h:367
gsm0808_vgcs_vbs_assign_req::cic
uint16_t cic
Definition: gsm0808.h:368
gsm0808_vgcs_vbs_assign_req::vstk_present
bool vstk_present
Definition: gsm0808.h:379
gsm0808_vgcs_vbs_assign_req::cils
struct gsm0808_cell_id_list_segment cils
Definition: gsm0808.h:383
gsm0808_vgcs_vbs_assign_req::downlink_dtx_flag_present
bool downlink_dtx_flag_present
Definition: gsm0808.h:370
gsm0808_vgcs_vbs_assign_req::priority_present
bool priority_present
Definition: gsm0808.h:364
gsm0808_vgcs_vbs_assign_req::call_id_present
bool call_id_present
Definition: gsm0808.h:388
gsm0808_vgcs_vbs_assign_req::codec_list_msc_preferred
struct gsm0808_speech_codec_list codec_list_msc_preferred
Definition: gsm0808.h:392
gsm0808_vgcs_vbs_assign_req::vstk_rand
uint8_t vstk_rand[5]
Definition: gsm0808.h:377
gsm0808_vgcs_vbs_assign_req::call_id
uint32_t call_id
Definition: gsm0808.h:389
gsm0808_vgcs_vbs_assign_req::vstk
uint8_t vstk[16]
Definition: gsm0808.h:380
gsm0808_vgcs_vbs_assign_req::codec_list_present
bool codec_list_present
Definition: gsm0808.h:391
gsm0808_vgcs_vbs_assign_req::downlink_dtx_flag
enum gsm0808_downlink_dtx_flag downlink_dtx_flag
Definition: gsm0808.h:371
gsm0808_vgcs_vbs_assign_res
3GPP TS 48.008 §3.2.1.54 VGCS/VBS ASSIGNMENT RESULT
Definition: gsm0808.h:397
gsm0808_vgcs_vbs_assign_res::cic_present
bool cic_present
Definition: gsm0808.h:404
gsm0808_vgcs_vbs_assign_res::channel_type
struct gsm0808_channel_type channel_type
Definition: gsm0808.h:398
gsm0808_vgcs_vbs_assign_res::call_id_present
bool call_id_present
Definition: gsm0808.h:416
gsm0808_vgcs_vbs_assign_res::codec_present
bool codec_present
Definition: gsm0808.h:413
gsm0808_vgcs_vbs_assign_res::aoip_transport_layer
struct sockaddr_storage aoip_transport_layer
Definition: gsm0808.h:411
gsm0808_vgcs_vbs_assign_res::codec_msc_chosen
struct gsm0808_speech_codec codec_msc_chosen
Definition: gsm0808.h:414
gsm0808_vgcs_vbs_assign_res::circuit_pool
uint8_t circuit_pool
Definition: gsm0808.h:408
gsm0808_vgcs_vbs_assign_res::aoip_transport_layer_present
bool aoip_transport_layer_present
Definition: gsm0808.h:410
gsm0808_vgcs_vbs_assign_res::chosen_channel_present
bool chosen_channel_present
Definition: gsm0808.h:401
gsm0808_vgcs_vbs_assign_res::circuit_pool_present
bool circuit_pool_present
Definition: gsm0808.h:407
gsm0808_vgcs_vbs_assign_res::chosen_channel
uint8_t chosen_channel
Definition: gsm0808.h:402
gsm0808_vgcs_vbs_assign_res::cic
uint16_t cic
Definition: gsm0808.h:405
gsm0808_vgcs_vbs_assign_res::cell_identifier
struct gsm0808_cell_id cell_identifier
Definition: gsm0808.h:399
gsm0808_vgcs_vbs_assign_res::call_id
uint32_t call_id
Definition: gsm0808.h:417
gsm0808_vgcs_vbs_assign_stat
3GPP TS 48.008 §3.2.1.80 VGCS/VBS ASSIGNMENT STATUS
Definition: gsm0808.h:537
gsm0808_vgcs_vbs_assign_stat::cils_est_present
bool cils_est_present
Definition: gsm0808.h:539
gsm0808_vgcs_vbs_assign_stat::cils_rel_present
bool cils_rel_present
Definition: gsm0808.h:547
gsm0808_vgcs_vbs_assign_stat::cell_status
enum gsm0808_vgcs_vbs_cell_status cell_status
Definition: gsm0808.h:555
gsm0808_vgcs_vbs_assign_stat::cils_rel
struct gsm0808_cell_id_list_segment cils_rel
Definition: gsm0808.h:548
gsm0808_vgcs_vbs_assign_stat::cils_tbe_present
bool cils_tbe_present
Definition: gsm0808.h:543
gsm0808_vgcs_vbs_assign_stat::cils_est
struct gsm0808_cell_id_list_segment cils_est
Definition: gsm0808.h:540
gsm0808_vgcs_vbs_assign_stat::cell_status_present
bool cell_status_present
Definition: gsm0808.h:554
gsm0808_vgcs_vbs_assign_stat::cils_ne_present
bool cils_ne_present
Definition: gsm0808.h:551
gsm0808_vgcs_vbs_assign_stat::cils_ne
struct gsm0808_cell_id_list_segment cils_ne
Definition: gsm0808.h:552
gsm0808_vgcs_vbs_assign_stat::cils_tbe
struct gsm0808_cell_id_list_segment cils_tbe
Definition: gsm0808.h:544
gsm0808_vgcs_vbs_setup_ack
3GPP TS 48.008 §3.2.1.51 VGCS/VBS SETUP ACK
Definition: gsm0808.h:348
gsm0808_vgcs_vbs_setup_ack::vgcs_feature_flags_present
bool vgcs_feature_flags_present
Definition: gsm0808.h:349
gsm0808_vgcs_vbs_setup_ack::flags
struct gsm0808_vgcs_feature_flags flags
Definition: gsm0808.h:350
gsm0808_vgcs_vbs_setup
3GPP TS 48.008 §3.2.1.50 VGCS/VBS SETUP
Definition: gsm0808.h:336
gsm0808_vgcs_vbs_setup::priority
struct gsm0808_priority priority
Definition: gsm0808.h:340
gsm0808_vgcs_vbs_setup::callref
struct gsm0808_group_callref callref
Definition: gsm0808.h:337
gsm0808_vgcs_vbs_setup::flags
struct gsm0808_vgcs_feature_flags flags
Definition: gsm0808.h:343
gsm0808_vgcs_vbs_setup::vgcs_feature_flags_present
bool vgcs_feature_flags_present
Definition: gsm0808.h:342
gsm0808_vgcs_vbs_setup::priority_present
bool priority_present
Definition: gsm0808.h:339
msgb
osmo_cell_global_id
Definition: gsm23003.h:29
osmo_gsm48_classmark
Definition: gsm_04_08.h:230
osmo_lcls
LCLS-related parameters from 3GPP TS 48.008.
Definition: gsm0808_utils.h:226
osmo_plmn_id
Definition: gsm23003.h:10
tlv_definition
Definition of All 256 IE / TLV.
Definition: tlv.h:527
tlv_parsed
result of the TLV parser
Definition: tlv.h:532
value_string
tlv.h
utils.h