libosmogb 1.13.1.1-afb4 Osmocom Gb library

Macros | Functions
gprs_bssgp_bss.c File Reference

GPRS BSSGP protocol implementation as per 3GPP TS 08.18. More...

`#include <errno.h>`
`#include <stdint.h>`
`#include <osmocom/core/msgb.h>`
`#include <osmocom/core/byteswap.h>`
`#include <osmocom/core/rate_ctr.h>`
`#include <osmocom/gsm/tlv.h>`
`#include <osmocom/core/talloc.h>`
`#include <osmocom/gprs/gprs_bssgp.h>`
`#include <osmocom/gprs/gprs_bssgp_bss.h>`
`#include <osmocom/gprs/gprs_ns.h>`
`#include "gprs_bssgp_internal.h"`

## Macros
#define | GSM_IMSI_LENGTH 17

## Functions
uint8_t * | bssgp_msgb_tlli_put (struct msgb *msg, uint32_t tlli)
uint8_t * | bssgp_msgb_ra_put (struct msgb *msg, const struct gprs_ra_id *ra_id)
int | bssgp_tx_suspend (uint16_t nsei, uint32_t tlli, const struct gprs_ra_id *ra_id)
| GMM-SUSPEND.req (Chapter 10.3.6) More...
int | bssgp_tx_resume (uint16_t nsei, uint32_t tlli, const struct gprs_ra_id *ra_id, uint8_t suspend_ref)
| GMM-RESUME.req (Chapter 10.3.9) More...
int | bssgp_tx_ra_capa_upd (struct bssgp_bvc_ctx *bctx, uint32_t tlli, uint8_t tag)
| Transmit RA-CAPABILITY-UPDATE (10.3.3) More...
static struct msgb * | common_tx_radio_status (struct bssgp_bvc_ctx *bctx)
static int | common_tx_radio_status2 (struct msgb *msg, uint8_t cause)
int | bssgp_tx_radio_status_tlli (struct bssgp_bvc_ctx *bctx, uint8_t cause, uint32_t tlli)
| Transmit RADIO-STATUS for TLLI (10.3.5) More...
int | bssgp_tx_radio_status_tmsi (struct bssgp_bvc_ctx *bctx, uint8_t cause, uint32_t tmsi)
| Transmit RADIO-STATUS for TMSI (10.3.5) More...
int | bssgp_tx_radio_status_imsi (struct bssgp_bvc_ctx *bctx, uint8_t cause, const char *imsi)
| Transmit RADIO-STATUS for IMSI (10.3.5) More...
int | bssgp_tx_flush_ll_ack (struct bssgp_bvc_ctx *bctx, uint32_t tlli, uint8_t action, uint16_t bvci_new, uint32_t num_octets)
| Transmit FLUSH-LL-ACK (Chapter 10.4.2) More...
int | bssgp_tx_llc_discarded (struct bssgp_bvc_ctx *bctx, uint32_t tlli, uint8_t num_frames, uint32_t num_octets)
| Transmit LLC-DISCARDED (Chapter 10.4.3) More...
int | bssgp_tx_bvc_block (struct bssgp_bvc_ctx *bctx, uint8_t cause)
| Transmit a BVC-BLOCK message (Chapter 10.4.8) More...
int | bssgp_tx_bvc_unblock (struct bssgp_bvc_ctx *bctx)
| Transmit a BVC-UNBLOCK message (Chapter 10.4.10) More...
int | bssgp_tx_bvc_reset2 (struct bssgp_bvc_ctx *bctx, uint16_t bvci, uint8_t cause, bool add_cell_id)
| Transmit a BVC-RESET message (Chapter 10.4.12) More...
int | bssgp_tx_bvc_reset (struct bssgp_bvc_ctx *bctx, uint16_t bvci, uint8_t cause)
int | bssgp_tx_fc_bvc (struct bssgp_bvc_ctx *bctx, uint8_t tag, uint32_t bucket_size, uint32_t bucket_leak_rate, uint32_t bmax_default_ms, uint32_t r_default_ms, uint8_t *bucket_full_ratio, uint32_t *queue_delay_ms)
| Transmit a FLOW_CONTROL-BVC (Chapter 10.4.4) More...
int | bssgp_tx_fc_ms (struct bssgp_bvc_ctx *bctx, uint32_t tlli, uint8_t tag, uint32_t ms_bucket_size, uint32_t bucket_leak_rate, uint8_t *bucket_full_ratio)
| Transmit a FLOW_CONTROL-MS (Chapter 10.4.6) More...
int | bssgp_tx_ul_ud (struct bssgp_bvc_ctx *bctx, uint32_t tlli, const uint8_t *qos_profile, struct msgb *llc_pdu)
| RL-UL-UNITDATA.req (Chapter 10.2.2) More...
int | bssgp_rx_paging (struct bssgp_paging_info *pinfo, struct msgb *msg)

## Detailed Description

GPRS BSSGP protocol implementation as per 3GPP TS 08.18.

## Macro Definition Documentation

## ◆ GSM_IMSI_LENGTH

#define GSM_IMSI_LENGTH 17

## Function Documentation

## ◆ bssgp_msgb_ra_put()

uint8_t * bssgp_msgb_ra_put | ( | struct msgb * | msg,
|  | const struct gprs_ra_id * | ra_id
| ) |  |

References BSSGP_IE_ROUTEING_AREA, gsm48_encode_ra(), msg, msgb_tvlv_put(), and ra_id.

Referenced by bssgp_tx_paging(), bssgp_tx_resume(), bssgp_tx_resume_ack(), bssgp_tx_resume_nack(), bssgp_tx_suspend(), bssgp_tx_suspend_ack(), and bssgp_tx_suspend_nack().

## ◆ bssgp_msgb_tlli_put()

uint8_t * bssgp_msgb_tlli_put | ( | struct msgb * | msg,
|  | uint32_t | tlli
| ) |  |

References BSSGP_IE_TLLI, msg, msgb_tvlv_put(), osmo_htonl, and tlli.

Referenced by bssgp_tx_fc_ms(), bssgp_tx_flush_ll_ack(), bssgp_tx_llc_discarded(), bssgp_tx_ra_capa_upd(), bssgp_tx_radio_status_tlli(), bssgp_tx_resume(), bssgp_tx_resume_ack(), bssgp_tx_resume_nack(), bssgp_tx_suspend(), bssgp_tx_suspend_ack(), and bssgp_tx_suspend_nack().

## ◆ bssgp_rx_paging()

int bssgp_rx_paging | ( | struct bssgp_paging_info * | pinfo,
|  | struct msgb * | msg
| ) |  |

References BSSGP_IE_BSS_AREA_ID, BSSGP_IE_BVCI, BSSGP_IE_DRX_PARAMS, BSSGP_IE_IMSI, BSSGP_IE_LOCATION_AREA, BSSGP_IE_QOS_PROFILE, BSSGP_IE_ROUTEING_AREA, BSSGP_IE_TMSI, BSSGP_PAGING_BSS_AREA, BSSGP_PAGING_BVCI, BSSGP_PAGING_CS, BSSGP_PAGING_LOCATION_AREA, BSSGP_PAGING_PS, BSSGP_PAGING_ROUTEING_AREA, BSSGP_PDUT_PAGING_CS, BSSGP_PDUT_PAGING_PS, bssgp_tlv_parse(), bssgp_paging_info::bvci, bssgp_normal_hdr::data, bssgp_paging_info::drx_params, gsm48_mi_to_string(), gsm48_parse_ra(), GSM_IMSI_LENGTH, bssgp_paging_info::imsi, bssgp_paging_info::mode, msg, msgb_bssgp_len, msgb_bssgph, bssgp_normal_hdr::pdu_type, bssgp_paging_info::ptmsi, bssgp_paging_info::qos, bssgp_paging_info::raid, bssgp_paging_info::scope, TLVP_LEN, TLVP_PRES_LEN, TLVP_PRESENT, TLVP_VAL, and tlvp_val16be().

## ◆ bssgp_tx_bvc_block()

int bssgp_tx_bvc_block | ( | struct bssgp_bvc_ctx * | bctx,
|  | uint8_t | cause
| ) |  |

Transmit a BVC-BLOCK message (Chapter 10.4.8)

References bssgp_cause_str(), BSSGP_IE_BVCI, BSSGP_IE_CAUSE, bssgp_msgb_alloc(), bssgp_ns_send, bssgp_ns_send_data, BSSGP_PDUT_BVC_BLOCK, bssgp_bvc_ctx::bvci, cause, DLBSSGP, LOGL_NOTICE, LOGP, msg, msgb_bvci, msgb_nsei, msgb_put(), msgb_tvlv_put(), bssgp_bvc_ctx::nsei, osmo_htons, and bssgp_normal_hdr::pdu_type.

## ◆ bssgp_tx_bvc_reset()

int bssgp_tx_bvc_reset | ( | struct bssgp_bvc_ctx * | bctx,
|  | uint16_t | bvci,
|  | uint8_t | cause
| ) |  |

References bssgp_tx_bvc_reset2(), bvci, BVCI_PTM, BVCI_SIGNALLING, and cause.

Referenced by bssgp_tx_bvc_ptp_reset(), and DEFUN().

## ◆ bssgp_tx_bvc_reset2()

int bssgp_tx_bvc_reset2 | ( | struct bssgp_bvc_ctx * | bctx,
|  | uint16_t | bvci,
|  | uint8_t | cause,
|  | bool | add_cell_id
| ) |  |

Transmit a BVC-RESET message (Chapter 10.4.12)

References bssgp_tx_bvc_reset_nsei_bvci(), bvci, cause, bssgp_bvc_ctx::cell_id, bssgp_bvc_ctx::nsei, and bssgp_bvc_ctx::ra_id.

Referenced by bssgp_tx_bvc_reset().

## ◆ bssgp_tx_bvc_unblock()

int bssgp_tx_bvc_unblock | ( | struct bssgp_bvc_ctx * | bctx | ) |

Transmit a BVC-UNBLOCK message (Chapter 10.4.10)

References BSSGP_IE_BVCI, bssgp_msgb_alloc(), bssgp_ns_send, bssgp_ns_send_data, BSSGP_PDUT_BVC_UNBLOCK, bssgp_bvc_ctx::bvci, DLBSSGP, LOGL_NOTICE, LOGP, msg, msgb_bvci, msgb_nsei, msgb_put(), msgb_tvlv_put(), bssgp_bvc_ctx::nsei, osmo_htons, and bssgp_normal_hdr::pdu_type.

## ◆ bssgp_tx_fc_bvc()

int bssgp_tx_fc_bvc | ( | struct bssgp_bvc_ctx * | bctx,
|  | uint8_t | tag,
|  | uint32_t | bucket_size,
|  | uint32_t | bucket_leak_rate,
|  | uint32_t | bmax_default_ms,
|  | uint32_t | r_default_ms,
|  | uint8_t * | bucket_full_ratio,
|  | uint32_t * | queue_delay_ms
| ) |  |

Transmit a FLOW_CONTROL-BVC (Chapter 10.4.4)

Parameters

  [in] | bctx | BVC Context
  [in] | tag | Additional tag to identify acknowledge
  [in] | bucket_size | Maximum bucket size in octets
  [in] | bucket_leak_rate | Bucket leak rate in octets/sec
  [in] | bmax_default_ms | Maximum bucket size default for MS
  [in] | r_default_ms | Bucket leak rate default for MS in octets/sec
  [in] | bucket_full_ratio | Ratio (in percent) of queue filling
  [in] | queue_delay_ms | Average queuing delay in milliseconds

References BSSGP_IE_BMAX_DEFAULT_MS, BSSGP_IE_BUCKET_FULL_RATIO, BSSGP_IE_BUCKET_LEAK_RATE, BSSGP_IE_BVC_BUCKET_SIZE, BSSGP_IE_BVC_MEASUREMENT, BSSGP_IE_R_DEFAULT_MS, BSSGP_IE_TAG, bssgp_msgb_alloc(), bssgp_ns_send, bssgp_ns_send_data, BSSGP_PDUT_FLOW_CONTROL_BVC, bssgp_bvc_ctx::bvci, msg, msgb_bvci, msgb_nsei, msgb_put(), msgb_tvlv_put(), bssgp_bvc_ctx::nsei, osmo_htons, and bssgp_normal_hdr::pdu_type.

## ◆ bssgp_tx_fc_ms()

int bssgp_tx_fc_ms | ( | struct bssgp_bvc_ctx * | bctx,
|  | uint32_t | tlli,
|  | uint8_t | tag,
|  | uint32_t | ms_bucket_size,
|  | uint32_t | bucket_leak_rate,
|  | uint8_t * | bucket_full_ratio
| ) |  |

Transmit a FLOW_CONTROL-MS (Chapter 10.4.6)

Parameters

  [in] | bctx | BVC Context
  [in] | tlli | TLLI to identify MS
  [in] | tag | Additional tag to identify acknowledge
  [in] | ms_bucket_size | Maximum bucket size in octets
  [in] | bucket_leak_rate | Bucket leak rate in octets/sec
  [in] | bucket_full_ratio | Ratio (in percent) of queue filling

References BSSGP_IE_BUCKET_FULL_RATIO, BSSGP_IE_BUCKET_LEAK_RATE, BSSGP_IE_MS_BUCKET_SIZE, BSSGP_IE_TAG, bssgp_msgb_alloc(), bssgp_msgb_tlli_put(), bssgp_ns_send, bssgp_ns_send_data, BSSGP_PDUT_FLOW_CONTROL_MS, bssgp_bvc_ctx::bvci, msg, msgb_bvci, msgb_nsei, msgb_put(), msgb_tvlv_put(), bssgp_bvc_ctx::nsei, bssgp_normal_hdr::pdu_type, and tlli.

## ◆ bssgp_tx_flush_ll_ack()

int bssgp_tx_flush_ll_ack | ( | struct bssgp_bvc_ctx * | bctx,
|  | uint32_t | tlli,
|  | uint8_t | action,
|  | uint16_t | bvci_new,
|  | uint32_t | num_octets
| ) |  |

Transmit FLUSH-LL-ACK (Chapter 10.4.2)

References BSSGP_IE_BVCI, BSSGP_IE_FLUSH_ACTION, BSSGP_IE_NUM_OCT_AFF, bssgp_msgb_alloc(), bssgp_msgb_tlli_put(), bssgp_ns_send, bssgp_ns_send_data, BSSGP_PDUT_FLUSH_LL_ACK, msg, msgb_bvci, msgb_nsei, msgb_put(), msgb_tvlv_put(), bssgp_bvc_ctx::nsei, osmo_htonl, osmo_htons, bssgp_normal_hdr::pdu_type, and tlli.

## ◆ bssgp_tx_llc_discarded()

int bssgp_tx_llc_discarded | ( | struct bssgp_bvc_ctx * | bctx,
|  | uint32_t | tlli,
|  | uint8_t | num_frames,
|  | uint32_t | num_octets
| ) |  |

Transmit LLC-DISCARDED (Chapter 10.4.3)

References BSSGP_IE_BVCI, BSSGP_IE_LLC_FRAMES_DISCARDED, BSSGP_IE_NUM_OCT_AFF, bssgp_msgb_alloc(), bssgp_msgb_tlli_put(), bssgp_ns_send, bssgp_ns_send_data, BSSGP_PDUT_LLC_DISCARD, bssgp_bvc_ctx::bvci, DLBSSGP, LOGL_NOTICE, LOGP, msg, msgb_bvci, msgb_nsei, msgb_put(), msgb_tvlv_put(), bssgp_bvc_ctx::nsei, osmo_htonl, osmo_htons, bssgp_normal_hdr::pdu_type, and tlli.

## ◆ bssgp_tx_ra_capa_upd()

int bssgp_tx_ra_capa_upd | ( | struct bssgp_bvc_ctx * | bctx,
|  | uint32_t | tlli,
|  | uint8_t | tag
| ) |  |

Transmit RA-CAPABILITY-UPDATE (10.3.3)

References BSSGP_IE_TAG, bssgp_msgb_alloc(), bssgp_msgb_tlli_put(), bssgp_ns_send, bssgp_ns_send_data, BSSGP_PDUT_RA_CAPA_UDPATE, bssgp_bvc_ctx::bvci, DLBSSGP, LOGL_NOTICE, LOGP, msg, msgb_bvci, msgb_nsei, msgb_put(), msgb_tvlv_put(), bssgp_bvc_ctx::nsei, bssgp_normal_hdr::pdu_type, and tlli.

## ◆ bssgp_tx_radio_status_imsi()

int bssgp_tx_radio_status_imsi | ( | struct bssgp_bvc_ctx * | bctx,
|  | uint8_t | cause,
|  | const char * | imsi
| ) |  |

Transmit RADIO-STATUS for IMSI (10.3.5)

References BSSGP_IE_IMSI, cause, common_tx_radio_status(), common_tx_radio_status2(), DLBSSGP, gsm48_generate_mid_from_imsi(), GSM48_MID_MAX_SIZE, LOGL_NOTICE, LOGPC, mi, msg, msgb_tvlv_put(), and OSMO_ASSERT.

## ◆ bssgp_tx_radio_status_tlli()

int bssgp_tx_radio_status_tlli | ( | struct bssgp_bvc_ctx * | bctx,
|  | uint8_t | cause,
|  | uint32_t | tlli
| ) |  |

Transmit RADIO-STATUS for TLLI (10.3.5)

References bssgp_msgb_tlli_put(), cause, common_tx_radio_status(), common_tx_radio_status2(), DLBSSGP, LOGL_NOTICE, LOGPC, msg, and tlli.

## ◆ bssgp_tx_radio_status_tmsi()

int bssgp_tx_radio_status_tmsi | ( | struct bssgp_bvc_ctx * | bctx,
|  | uint8_t | cause,
|  | uint32_t | tmsi
| ) |  |

Transmit RADIO-STATUS for TMSI (10.3.5)

References BSSGP_IE_TMSI, cause, common_tx_radio_status(), common_tx_radio_status2(), DLBSSGP, LOGL_NOTICE, LOGPC, msg, msgb_tvlv_put(), and osmo_htonl.

## ◆ bssgp_tx_resume()

int bssgp_tx_resume | ( | uint16_t | nsei,
|  | uint32_t | tlli,
|  | const struct gprs_ra_id * | ra_id,
|  | uint8_t | suspend_ref
| ) |  |

GMM-RESUME.req (Chapter 10.3.9)

References BSSGP_IE_SUSPEND_REF_NR, bssgp_msgb_alloc(), bssgp_msgb_ra_put(), bssgp_msgb_tlli_put(), bssgp_ns_send, bssgp_ns_send_data, BSSGP_PDUT_RESUME, DLBSSGP, LOGL_NOTICE, LOGP, msg, msgb_bvci, msgb_nsei, msgb_put(), msgb_tvlv_put(), nsei, bssgp_normal_hdr::pdu_type, ra_id, and tlli.

## ◆ bssgp_tx_suspend()

int bssgp_tx_suspend | ( | uint16_t | nsei,
|  | uint32_t | tlli,
|  | const struct gprs_ra_id * | ra_id
| ) |  |

GMM-SUSPEND.req (Chapter 10.3.6)

References bssgp_msgb_alloc(), bssgp_msgb_ra_put(), bssgp_msgb_tlli_put(), bssgp_ns_send, bssgp_ns_send_data, BSSGP_PDUT_SUSPEND, DLBSSGP, LOGL_NOTICE, LOGP, msg, msgb_bvci, msgb_nsei, msgb_put(), nsei, bssgp_normal_hdr::pdu_type, ra_id, and tlli.

## ◆ bssgp_tx_ul_ud()

int bssgp_tx_ul_ud | ( | struct bssgp_bvc_ctx * | bctx,
|  | uint32_t | tlli,
|  | const uint8_t * | qos_profile,
|  | struct msgb * | llc_pdu
| ) |  |

RL-UL-UNITDATA.req (Chapter 10.2.2)

Parameters

  [in] | bctx | BVC Context
  [in] | tlli | TLLI to identify MS
  [in] | qos_profile | Pointer to three octests of QoS profile
  [in] | llc_pdu | msgb pointer containing UL Unitdata IE payload

References bssgp_create_cell_id(), BSSGP_CTR_BYTES_OUT, BSSGP_CTR_PKTS_OUT, BSSGP_IE_ALIGNMENT, BSSGP_IE_CELL_ID, bssgp_ns_send, bssgp_ns_send_data, BSSGP_PDUT_UL_UNITDATA, bssgp_bvc_ctx::bvci, bssgp_bvc_ctx::cell_id, bssgp_bvc_ctx::ctrg, msg, msgb_bvci, msgb_nsei, msgb_push(), msgb_tvlv_push(), bssgp_bvc_ctx::nsei, osmo_htonl, bssgp_ud_hdr::pdu_type, qos_profile, bssgp_ud_hdr::qos_profile, bssgp_bvc_ctx::ra_id, rate_ctr_add(), rate_ctr_group_get_ctr(), rate_ctr_inc(), tlli, and bssgp_ud_hdr::tlli.

## ◆ common_tx_radio_status()

static struct msgb * common_tx_radio_status | ( | struct bssgp_bvc_ctx * | bctx | ) |
| static

References bssgp_msgb_alloc(), BSSGP_PDUT_RADIO_STATUS, bssgp_bvc_ctx::bvci, DLBSSGP, LOGL_NOTICE, LOGP, msg, msgb_bvci, msgb_nsei, msgb_put(), bssgp_bvc_ctx::nsei, and bssgp_normal_hdr::pdu_type.

Referenced by bssgp_tx_radio_status_imsi(), bssgp_tx_radio_status_tlli(), and bssgp_tx_radio_status_tmsi().

## ◆ common_tx_radio_status2()

static int common_tx_radio_status2 | ( | struct msgb * | msg,
|  | uint8_t | cause
| ) |  |
| static

References bssgp_cause_str(), BSSGP_IE_CAUSE, bssgp_ns_send, bssgp_ns_send_data, cause, DLBSSGP, LOGL_NOTICE, LOGPC, msg, and msgb_tvlv_put().

Referenced by bssgp_tx_radio_status_imsi(), bssgp_tx_radio_status_tlli(), and bssgp_tx_radio_status_tmsi().