libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Fields
bsslap_pdu Struct Reference
3GPP TS 48.071 BSS LCS Assistance Protocol (BSSLAP).

`#include <gsm_48_071.h>`

## Data Fields
enum bsslap_msgt | msg_type
union {
struct bsslap_ta_response ta_response
enum bsslap_cause reject
struct bsslap_reset reset
enum bsslap_cause abort
struct bsslap_ta_layer3 ta_layer3
}; |

## Field Documentation

## ◆

union { ... } bsslap_pdu::@120

## ◆ abort

enum bsslap_cause bsslap_pdu::abort

Referenced by osmo_bsslap_dec(), and osmo_bsslap_enc().

## ◆ msg_type

enum bsslap_msgt bsslap_pdu::msg_type

Referenced by osmo_bssap_le_pdu_to_str_buf(), osmo_bsslap_dec(), and osmo_bsslap_enc().

## ◆ reject

enum bsslap_cause bsslap_pdu::reject

Referenced by osmo_bsslap_dec(), and osmo_bsslap_enc().

## ◆ reset

struct bsslap_reset bsslap_pdu::reset

Referenced by osmo_bsslap_dec(), and osmo_bsslap_enc().

## ◆ ta_layer3

struct bsslap_ta_layer3 bsslap_pdu::ta_layer3

Referenced by osmo_bsslap_dec(), and osmo_bsslap_enc().

## ◆ ta_response

struct bsslap_ta_response bsslap_pdu::ta_response

Referenced by osmo_bsslap_dec(), and osmo_bsslap_enc().

The documentation for this struct was generated from the following file:

- include/osmocom/gsm/protocol/gsm_48_071.h