libosmogsm 1.13.1.1-afb4 Osmocom GSM library

### - c -

- c : abis_rsl_cchan_hdr, abis_rsl_dchan_hdr, abis_rsl_rll_hdr
- c_i_cb : info_meas_ind_param
- c_r : osmo_rlp_frame_decoded
- call_id : gsm0808_handover_request, gsm0808_vgcs_vbs_assign_req, gsm0808_vgcs_vbs_assign_res
- call_id_present : gsm0808_handover_request, gsm0808_vgcs_vbs_assign_req, gsm0808_vgcs_vbs_assign_res
- call_priority : osmo_gsm48_si_pch_nch_info
- call_priority_present : osmo_gsm48_si_pch_nch_info
- callref : gsm0808_vgcs_vbs_assign_req, gsm0808_vgcs_vbs_setup
- cancel_type : osmo_gsup_message
- category : osmo_cbsp_write_replace
- cause : bsslap_reset, gsm0808_handover_failure, gsm0808_handover_performed, gsm0808_handover_request, gsm0808_handover_required, gsm0808_handover_required_reject, gsm0808_uplink_reject_cmd, gsm0808_uplink_release_ind, gsm0808_uplink_seized_cmd, gsm0808_vgcs_vbs_assign_fail, gsm48_gprs_susp_req, info_act_cnf_param, osmo_bsslap_err, osmo_bssmap_le_err, osmo_cbsp_error_ind, osmo_cbsp_fail_ent, osmo_gsup_message, osmo_iuup_rnl_status, osmo_oap_message
- cause_bssap : osmo_gsup_message
- cause_bssap_set : osmo_gsup_message
- cause_rr : osmo_gsup_message
- cause_rr_set : osmo_gsup_message
- cause_sm : osmo_gsup_message
- cause_val : lcs_cause_ie
- cbq : osmo_gsm48_si_selection_params
- cbs : osmo_cbsp_write_replace
- ccn_active : osmo_gprs_cell_options
- cdma200_rat_cap : gsm48_classmark3
- cell_channel_description : gsm48_system_information_type_1
- cell_desc : gsm48_ho_cmd
- cell_id : bsslap_reset, bsslap_ta_response, bssmap_le_perform_loc_req, gsm0808_handover_performed, osmo_cbsp_cell_ent, osmo_cbsp_fail_ent, osmo_cbsp_loading_ent, osmo_cbsp_num_compl_ent, osmo_gsm48_si_ro_info
- cell_identifier : gsm0808_handover_command, gsm0808_uplink_app_data, gsm0808_uplink_request, gsm0808_uplink_request_cnf, gsm0808_vgcs_vbs_assign_req, gsm0808_vgcs_vbs_assign_res
- cell_identifier_present : gsm0808_uplink_request
- cell_identifier_serving : gsm0808_handover_request
- cell_identifier_target : gsm0808_handover_request
- cell_identity : gsm48_system_information_type_3, osmo_cell_global_id, osmo_cell_global_id_ps
- cell_list : osmo_cbsp_kill, osmo_cbsp_kill_complete, osmo_cbsp_kill_failure, osmo_cbsp_load_query, osmo_cbsp_msg_status_query, osmo_cbsp_reset, osmo_cbsp_reset_complete, osmo_cbsp_reset_failure, osmo_cbsp_restart, osmo_cbsp_write_replace, osmo_cbsp_write_replace_complete, osmo_cbsp_write_replace_failure
- cell_options : gsm48_system_information_type_3
- cell_opts : osmo_gsm48_si13_info
- cell_resel_off : osmo_gsm48_si_selection_params
- cell_sel_par : gsm48_system_information_type_3, gsm48_system_information_type_4
- cell_status : gsm0808_vgcs_vbs_assign_stat
- cell_status_present : gsm0808_vgcs_vbs_assign_stat
- cfg : gsm0808_speech_codec
- ch_indctr : gsm0808_channel_type
- ch_rate_type : gsm0808_channel_type
- chan_desc : bsslap_reset, gsm48_add_ass, gsm48_ass_cmd, gsm48_chan_mode_modify, gsm48_frq_redef, gsm48_ho_cmd, gsm48_imm_ass, rsl_ie_chan_ident
- chan_desc1 : gsm48_imm_ass_ext
- chan_desc2 : gsm48_imm_ass_ext
- chan_nr : abis_rsl_cchan_hdr, abis_rsl_chan_nr, abis_rsl_dchan_hdr, abis_rsl_rll_hdr, gsm48_chan_desc, info_act_cnf_param, info_act_req_param, info_ciph_req_param, info_meas_ind_param, info_ulacc_req_param, lapdm_msg_ctx, ph_data_param, ph_rach_ind_param, ph_tch_param, rsl_ie_chan_ident
- chan_nr_fields : abis_rsl_cchan_hdr, abis_rsl_dchan_hdr, abis_rsl_rll_hdr
- chan_rate : rsl_ie_chan_mode
- chan_rt : rsl_ie_chan_mode
- channel_ind : osmo_cbsp_error_ind, osmo_cbsp_kill, osmo_cbsp_kill_complete, osmo_cbsp_kill_failure, osmo_cbsp_load_query, osmo_cbsp_load_query_complete, osmo_cbsp_load_query_failure, osmo_cbsp_msg_status_query, osmo_cbsp_msg_status_query_complete, osmo_cbsp_msg_status_query_failure, osmo_cbsp_write_replace, osmo_cbsp_write_replace_complete, osmo_cbsp_write_replace_failure
- channel_type : gsm0808_handover_request, gsm0808_vgcs_vbs_assign_req, gsm0808_vgcs_vbs_assign_res
- chosen_channel : gsm0808_handover_complete, gsm0808_handover_performed, gsm0808_handover_request_ack, gsm0808_vgcs_vbs_assign_res
- chosen_channel_present : gsm0808_handover_complete, gsm0808_handover_performed, gsm0808_handover_request_ack, gsm0808_vgcs_vbs_assign_res
- chosen_encr_alg : gsm0808_handover_complete, gsm0808_handover_performed, gsm0808_handover_request_ack
- chosen_encr_alg_present : gsm0808_handover_complete, gsm0808_handover_performed
- chosen_encryption_algorithm_serving : gsm0808_handover_request
- chosen_speech_version : gsm0808_handover_request_ack
- ci : gsm0808_cell_id_u, osmo_lac_and_ci_id
- ci_amr_fr : osmo_preproc_ave_cfg, osmo_preproc_pc_comp
- ci_amr_hr : osmo_preproc_ave_cfg, osmo_preproc_pc_comp
- ci_fr : osmo_preproc_ave_cfg, osmo_preproc_pc_comp
- ci_gprs : osmo_preproc_ave_cfg, osmo_preproc_pc_comp
- ci_hr : osmo_preproc_ave_cfg, osmo_preproc_pc_comp
- ci_sdcch : osmo_preproc_ave_cfg, osmo_preproc_pc_comp
- cic : gsm0808_vgcs_vbs_assign_req, gsm0808_vgcs_vbs_assign_res
- cic_present : gsm0808_vgcs_vbs_assign_req, gsm0808_vgcs_vbs_assign_res
- cil : gsm0808_cell_id_list_segment, gsm0808_handover_required
- cils : gsm0808_vgcs_vbs_area_cell_info, gsm0808_vgcs_vbs_assign_req
- cils_est : gsm0808_vgcs_vbs_assign_stat
- cils_est_present : gsm0808_vgcs_vbs_assign_stat
- cils_ne : gsm0808_vgcs_vbs_assign_stat
- cils_ne_present : gsm0808_vgcs_vbs_assign_stat
- cils_present : gsm0808_vgcs_vbs_assign_req
- cils_rel : gsm0808_vgcs_vbs_assign_stat
- cils_rel_present : gsm0808_vgcs_vbs_assign_stat
- cils_tbe : gsm0808_vgcs_vbs_assign_stat
- cils_tbe_present : gsm0808_vgcs_vbs_assign_stat
- ciph_req : mph_info_param
- cipher_response_mode : gsm0808_cipher_mode_command
- cipher_response_mode_present : gsm0808_cipher_mode_command
- ciphering_mode_setting_cap : gsm48_classmark3
- circuit_pool : gsm0808_vgcs_vbs_assign_fail, gsm0808_vgcs_vbs_assign_res
- circuit_pool_present : gsm0808_vgcs_vbs_assign_fail, gsm0808_vgcs_vbs_assign_res
- ck : osmo_auth_vector
- classmark1 : gsm48_imsi_detach_ind, osmo_gsm48_classmark
- classmark1_set : osmo_gsm48_classmark
- classmark2 : osmo_gsm48_classmark
- classmark2_len : osmo_gsm48_classmark
- classmark3 : osmo_gsm48_classmark
- classmark3_len : osmo_gsm48_classmark
- classmark_information : gsm0808_handover_request
- client_id : osmo_oap_client_config, osmo_oap_client_state, osmo_oap_message
- cm2 : gsm48_cm_change, gsm48_talker_indication
- cm2_len : gsm48_cm_change, gsm48_talker_indication
- cn_domain : osmo_gsup_message
- code : osmo_mme_id
- codec : gsm0808_speech_codec_list
- codec_list_bss_supported : gsm0808_handover_complete, gsm0808_handover_failure, gsm0808_handover_request_ack, gsm0808_vgcs_vbs_assign_fail
- codec_list_msc_preferred : gsm0808_handover_request, gsm0808_vgcs_vbs_assign_req
- codec_list_present : gsm0808_vgcs_vbs_assign_fail, gsm0808_vgcs_vbs_assign_req
- codec_msc_chosen : gsm0808_vgcs_vbs_assign_res
- codec_present : gsm0808_vgcs_vbs_assign_res
- coding : gsm_mncc_bearer_cap, gsm_mncc_cause, gsm_mncc_progress
- confidence : osmo_gad_ell_arc, osmo_gad_ell_point_alt_unc_ell, osmo_gad_ell_point_unc_ellipse
- config : osmo_iuup_instance, osmo_iuup_rnl_prim, osmo_lcls
- conn_ind : osmo_phsap_prim
- conn_oriented_info : bssmap_le_pdu
- content : gsm23041_msg_param_gsm, gsm23041_msg_param_umts
- context_id : osmo_gsup_pdp_info
- control : osmo_lcls
- control_channel_desc : gsm48_system_information_type_3
- corr_needed : osmo_lcls
- count : SHA1Context
- cp_max_retr : gsm411_smc_inst
- cp_msg : gsm411_smc_inst
- cp_rel : gsm411_smc_inst
- cp_retx : gsm411_smc_inst
- cp_state : gsm411_smc_inst
- cp_tc1 : gsm411_smc_inst
- cp_timer : gsm411_smc_inst
- cp_type : smcdatastate
- cpl : gsm0808_vgcs_vbs_assign_fail
- cpl_present : gsm0808_vgcs_vbs_assign_fail
- cr : osmo_gcr_parsed
- cs_ps_srvcc_geran_eutra : gsm48_classmark3
- cs_ps_srvcc_geran_utra : gsm48_classmark3
- ctrl_ack_type_use_block : osmo_gprs_cell_options
- curlen : sha256_state
- current_channel_type_1 : gsm0808_handover_request, gsm0808_handover_required
- current_channel_type_1_present : gsm0808_handover_request, gsm0808_handover_required
- current_channel_type_2 : gsm0808_old_bss_to_new_bss_info
- current_channel_type_2_present : gsm0808_old_bss_to_new_bss_info
- current_rat_type : osmo_gsup_message
- current_talker_priority : gsm0808_uplink_reject_cmd
- current_talker_priority_present : gsm0808_uplink_reject_cmd
- cycle : fn_remap_table