libosmogsm 1.13.1.1-afb4 Osmocom GSM library

aes_wrap.h
Go to the documentation of this file.
1
10/*
11 * Copyright (c) 2003-2007, Jouni Malinen <j@w1.fi>
12 *
13 * This program is free software; you can redistribute it and/or modify
14 * it under the terms of the GNU General Public License version 2 as
15 * published by the Free Software Foundation.
16 *
17 * Alternatively, this software may be distributed under the terms of BSD
18 * license.
19 *
20 * SPDX-License-Identifier: GPL-2.0 OR BSD-3-Clause
21 *
22 * See README and COPYING for more details.
23 */
24
25#pragma once
26
27 int __must_check aes_wrap(const u8 *kek, int n, const u8 *plain, u8 *cipher);
28 int __must_check aes_unwrap(const u8 *kek, int n, const u8 *cipher, u8 *plain);
29 int __must_check omac1_aes_128_vector(const u8 *key, size_t num_elem,
30 const u8 *addr[], const size_t *len,
31 u8 *mac);
32 int __must_check omac1_aes_128(const u8 *key, const u8 *data, size_t data_len,
33 u8 *mac);
34 int __must_check aes_128_encrypt_block(const u8 *key, const u8 *in, u8 *out);
35 int __must_check aes_128_ctr_encrypt(const u8 *key, const u8 *nonce,
36 u8 *data, size_t data_len);
37 int __must_check aes_128_eax_encrypt(const u8 *key,
38 const u8 *nonce, size_t nonce_len,
39 const u8 *hdr, size_t hdr_len,
40 u8 *data, size_t data_len, u8 *tag);
41 int __must_check aes_128_eax_decrypt(const u8 *key,
42 const u8 *nonce, size_t nonce_len,
43 const u8 *hdr, size_t hdr_len,
44 u8 *data, size_t data_len, const u8 *tag);
45 int __must_check aes_128_cbc_encrypt(const u8 *key, const u8 *iv, u8 *data,
46 size_t data_len);
47 int __must_check aes_128_cbc_decrypt(const u8 *key, const u8 *iv, u8 *data,
48 size_t data_len);
aes_wrap
int __must_check aes_wrap(const u8 *kek, int n, const u8 *plain, u8 *cipher)
aes_unwrap
int __must_check aes_unwrap(const u8 *kek, int n, const u8 *cipher, u8 *plain)
aes_128_encrypt_block
int __must_check aes_128_encrypt_block(const u8 *key, const u8 *in, u8 *out)
aes_128_encrypt_block - Perform one AES 128-bit block operation @key: Key for AES @in: Input data (16...
Definition: aes-encblock.c:31
omac1_aes_128
int __must_check omac1_aes_128(const u8 *key, const u8 *data, size_t data_len, u8 *mac)
aes_128_cbc_decrypt
int __must_check aes_128_cbc_decrypt(const u8 *key, const u8 *iv, u8 *data, size_t data_len)
aes_128_cbc_encrypt
int __must_check aes_128_cbc_encrypt(const u8 *key, const u8 *iv, u8 *data, size_t data_len)
omac1_aes_128_vector
int __must_check omac1_aes_128_vector(const u8 *key, size_t num_elem, const u8 *addr[], const size_t *len, u8 *mac)
aes_128_ctr_encrypt
int __must_check aes_128_ctr_encrypt(const u8 *key, const u8 *nonce, u8 *data, size_t data_len)
aes_128_eax_encrypt
int __must_check aes_128_eax_encrypt(const u8 *key, const u8 *nonce, size_t nonce_len, const u8 *hdr, size_t hdr_len, u8 *data, size_t data_len, u8 *tag)
aes_128_eax_decrypt
int __must_check aes_128_eax_decrypt(const u8 *key, const u8 *nonce, size_t nonce_len, const u8 *hdr, size_t hdr_len, u8 *data, size_t data_len, const u8 *tag)
n
write Write running configuration to or terminal n Write configuration to the copy running config startup Copy configuration n Copy running config to n Copy running config to startup write Write running configuration to or terminal n Write to terminal n
data
uint8_t data[0]
hdr
struct gsm48_hdr hdr
Definition: gsm_04_08.h:0
len
uint8_t len
Definition: gsm_04_11.h:0
u8
uint8_t u8
Definition: common.h:27
__must_check
#define __must_check
Definition: common.h:101