libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Structures | Macros | Functions | Variables
gsm0502.c File Reference

Paging helper code. More...

`#include <stdint.h>`
`#include <osmocom/gsm/protocol/gsm_04_08.h>`
`#include <osmocom/gsm/gsm0502.h>`
`#include <osmocom/gsm/gsm48.h>`
`#include <osmocom/gsm/rsl.h>`
`#include <osmocom/gsm/gsm_utils.h>`
`#include <osmocom/core/logging.h>`
`#include <inttypes.h>`

## Data Structures
struct | fn_remap_table

## Macros
#define | TCH_REPEAT_LENGTH 13
#define | FACCH_F_REPEAT_LENGTH 13
#define | FACCH_H_REPEAT_LENGTH 26
#define | fn_remap_table_from_traffic_block_map(table, map, rows, cols, repeat)
#define | CB_FCCH -1
#define | CB_SCH -2
#define | CB_BCCH -3
#define | CB_IDLE -4

## Functions
unsigned int | gsm0502_calc_paging_group (const struct gsm48_control_channel_descr *chan_desc, uint64_t imsi)
static | __attribute__ ((constructor))
uint32_t | gsm0502_fn_remap (uint32_t fn, enum gsm0502_fn_remap_channel channel)
| Calculate the frame number of the beginning of a block. More...
uint16_t | gsm0502_hop_seq_gen (const struct gsm_time *t, uint8_t hsn, uint8_t maio, size_t n, const uint16_t *ma)
| Hopping sequence generation as per 3GPP TS 45.002, section 6.2.3. More...
int | gsm0502_fn2ccch_block (uint32_t fn)
| Calculate CCCH block number from the given TDMA frame number. More...

## Variables
static const uint8_t | gsm0502_tch_f_traffic_block_map [3][8]
static const uint8_t | gsm0502_tch_h0_traffic_block_map [3][4]
static const uint8_t | gsm0502_tch_h1_traffic_block_map [3][4]
static const uint8_t | gsm0502_tch_f_facch_block_map [3][8]
static const uint8_t | gsm0502_tch_h0_facch_block_map [3][6]
static const uint8_t | gsm0502_tch_h1_facch_block_map [3][6]
static struct fn_remap_table | tch_f_remap_table
static struct fn_remap_table | tch_h0_remap_table
static struct fn_remap_table | tch_h1_remap_table
static struct fn_remap_table | facch_f_remap_table
static struct fn_remap_table | facch_h0_remap_table
static struct fn_remap_table | facch_h1_remap_table
static struct fn_remap_table * | fn_remap_table_ptr [FN_REMAP_MAX]
static const uint8_t | rn_table [114]
static const int | ccch_block_table [51]

## Detailed Description

Paging helper code.

## Macro Definition Documentation

## ◆ CB_BCCH

#define CB_BCCH -3

## ◆ CB_FCCH

#define CB_FCCH -1

## ◆ CB_IDLE

#define CB_IDLE -4

## ◆ CB_SCH

#define CB_SCH -2

## ◆ FACCH_F_REPEAT_LENGTH

#define FACCH_F_REPEAT_LENGTH 13

## ◆ FACCH_H_REPEAT_LENGTH

#define FACCH_H_REPEAT_LENGTH 26

## ◆ fn_remap_table_from_traffic_block_map

#define fn_remap_table_from_traffic_block_map | ( |  | table,
|  |  | map,
|  |  | rows,
|  |  | cols,
|  |  | repeat
| ) |  |

Value:
for(i=0;i<rows;i++) { \
table.blockend[i] = map[i][cols-1]; \
if(map[i][0] <= map[i][cols-1]) \
table.distance[i] = map[i][cols-1] - map[i][0]; \
else \
table.distance[i] = repeat - map[i][0] + map[i][cols-1]; \
} \
table.cycle = repeat; \
table.len = rows;

## ◆ TCH_REPEAT_LENGTH

#define TCH_REPEAT_LENGTH 13

## Function Documentation

## ◆ __attribute__()

static __attribute__ | ( | (constructor) |  | ) |
| static

References facch_f_remap_table, FACCH_F_REPEAT_LENGTH, facch_h0_remap_table, facch_h1_remap_table, FACCH_H_REPEAT_LENGTH, FN_REMAP_FACCH_F, FN_REMAP_FACCH_H0, FN_REMAP_FACCH_H1, fn_remap_table_from_traffic_block_map, fn_remap_table_ptr, FN_REMAP_TCH_F, FN_REMAP_TCH_H0, FN_REMAP_TCH_H1, gsm0502_tch_f_facch_block_map, gsm0502_tch_f_traffic_block_map, gsm0502_tch_h0_facch_block_map, gsm0502_tch_h0_traffic_block_map, gsm0502_tch_h1_facch_block_map, gsm0502_tch_h1_traffic_block_map, tch_f_remap_table, tch_h0_remap_table, tch_h1_remap_table, and TCH_REPEAT_LENGTH.

## Variable Documentation

## ◆ ccch_block_table

const int ccch_block_table[51]
| static

Initial value:
= {
CB_FCCH, CB_SCH,
CB_BCCH, CB_BCCH, CB_BCCH, CB_BCCH,
0, 0, 0, 0,
CB_FCCH, CB_SCH,
1, 1, 1, 1,
2, 2, 2, 2,
CB_FCCH, CB_SCH,
3, 3, 3, 3,
4, 4, 4, 4,
CB_FCCH, CB_SCH,
5, 5, 5, 5,
6, 6, 6, 6,
CB_FCCH, CB_SCH,
7, 7, 7, 7,
8, 8, 8, 8,
CB_IDLE
}
CB_IDLE
#define CB_IDLE
Definition: gsm0502.c:267
CB_BCCH
#define CB_BCCH
Definition: gsm0502.c:266
CB_SCH
#define CB_SCH
Definition: gsm0502.c:265
CB_FCCH
#define CB_FCCH
Definition: gsm0502.c:264

Referenced by gsm0502_fn2ccch_block().

## ◆ facch_f_remap_table

struct fn_remap_table facch_f_remap_table
| static

Referenced by __attribute__().

## ◆ facch_h0_remap_table

struct fn_remap_table facch_h0_remap_table
| static

Referenced by __attribute__().

## ◆ facch_h1_remap_table

struct fn_remap_table facch_h1_remap_table
| static

Referenced by __attribute__().

## ◆ fn_remap_table_ptr

struct fn_remap_table* fn_remap_table_ptr[FN_REMAP_MAX]
| static

Referenced by __attribute__(), and gsm0502_fn_remap().

## ◆ gsm0502_tch_f_facch_block_map

const uint8_t gsm0502_tch_f_facch_block_map[3][8]
| static

Initial value:
= {
{0, 1, 2, 3, 4, 5, 6, 7},
{4, 5, 6, 7, 8, 9, 10, 11},
{8, 9, 10, 11, 0, 1, 2, 3}
}

Referenced by __attribute__().

## ◆ gsm0502_tch_f_traffic_block_map

const uint8_t gsm0502_tch_f_traffic_block_map[3][8]
| static

Initial value:
= {
{0, 1, 2, 3, 4, 5, 6, 7},
{4, 5, 6, 7, 8, 9, 10, 11},
{8, 9, 10, 11, 0, 1, 2, 3}
}

Referenced by __attribute__().

## ◆ gsm0502_tch_h0_facch_block_map

const uint8_t gsm0502_tch_h0_facch_block_map[3][6]
| static

Initial value:
= {
{0, 2, 4, 6, 8, 10},
{8, 10, 13, 15, 17, 19},
{17, 19, 21, 23, 0, 2}
}

Referenced by __attribute__().

## ◆ gsm0502_tch_h0_traffic_block_map

const uint8_t gsm0502_tch_h0_traffic_block_map[3][4]
| static

Initial value:
= {
{0, 2, 4, 6},
{4, 6, 8, 10},
{8, 10, 0, 2}
}

Referenced by __attribute__().

## ◆ gsm0502_tch_h1_facch_block_map

const uint8_t gsm0502_tch_h1_facch_block_map[3][6]
| static

Initial value:
= {
{1, 3, 5, 7, 9, 11},
{9, 11, 14, 16, 18, 20},
{18, 20, 22, 24, 1, 3}
}

Referenced by __attribute__().

## ◆ gsm0502_tch_h1_traffic_block_map

const uint8_t gsm0502_tch_h1_traffic_block_map[3][4]
| static

Initial value:
= {
{1, 3, 5, 7},
{5, 7, 9, 11},
{9, 11, 1, 3}
}

Referenced by __attribute__().

## ◆ rn_table

const uint8_t rn_table[114]
| static

Initial value:
= {
48, 98, 63, 1, 36, 95, 78, 102, 94, 73,
0, 64, 25, 81, 76, 59, 124, 23, 104, 100,
101, 47, 118, 85, 18, 56, 96, 86, 54, 2,
80, 34, 127, 13, 6, 89, 57, 103, 12, 74,
55, 111, 75, 38, 109, 71, 112, 29, 11, 88,
87, 19, 3, 68, 110, 26, 33, 31, 8, 45,
82, 58, 40, 107, 32, 5, 106, 92, 62, 67,
77, 108, 122, 37, 60, 66, 121, 42, 51, 126,
117, 114, 4, 90, 43, 52, 53, 113, 120, 72,
16, 49, 7, 79, 119, 61, 22, 84, 9, 97,
91, 15, 21, 24, 46, 39, 93, 105, 65, 70,
125, 99, 17, 123,
}

Referenced by gsm0502_hop_seq_gen().

## ◆ tch_f_remap_table

struct fn_remap_table tch_f_remap_table
| static

Referenced by __attribute__().

## ◆ tch_h0_remap_table

struct fn_remap_table tch_h0_remap_table
| static

Referenced by __attribute__().

## ◆ tch_h1_remap_table

struct fn_remap_table tch_h1_remap_table
| static

Referenced by __attribute__().