libosmogsm 1.13.1.1-afb4 Osmocom GSM library

gsm_08_58.h
Go to the documentation of this file.
1
4/*
5 * (C) 2008 by Harald Welte <laforge@gnumonks.org>
6 * All Rights Reserved
7 *
8 * This program is free software; you can redistribute it and/or modify
9 * it under the terms of the GNU General Public License as published by
10 * the Free Software Foundation; either version 2 of the License, or
11 * (at your option) any later version.
12 *
13 * This program is distributed in the hope that it will be useful,
14 * but WITHOUT ANY WARRANTY; without even the implied warranty of
15 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the
16 * GNU General Public License for more details.
17 *
18 */
19
20#pragma once
21
22#include <stdint.h>
23
24#include <osmocom/core/endian.h>
25
30/* Channel Number 9.3.1 */
31 union abis_rsl_chan_nr {
32 struct {
33#if OSMO_IS_BIG_ENDIAN
34 uint8_t cbits:5,
35 tn:3;
36#elif OSMO_IS_LITTLE_ENDIAN
37 uint8_t tn:3,
38 cbits:5;
39#endif
40 } __attribute__ ((packed));
41 uint8_t chan_nr;
42} __attribute__ ((packed));
43#define ABIS_RSL_CHAN_NR_CBITS_Bm_ACCHs 0x01
44#define ABIS_RSL_CHAN_NR_CBITS_Lm_ACCHs(ss) (0x02 + (ss))
45#define ABIS_RSL_CHAN_NR_CBITS_SDCCH4_ACCH(ss) (0x04 + (ss))
46#define ABIS_RSL_CHAN_NR_CBITS_SDCCH8_ACCH(ss) (0x08 + (ss))
47#define ABIS_RSL_CHAN_NR_CBITS_BCCH 0x10
48#define ABIS_RSL_CHAN_NR_CBITS_RACH 0x11
49#define ABIS_RSL_CHAN_NR_CBITS_PCH_AGCH 0x12
50#define ABIS_RSL_CHAN_NR_CBITS_OSMO_PDCH 0x18 /*< non-standard, for dyn TS */
51#define ABIS_RSL_CHAN_NR_CBITS_OSMO_CBCH4 0x19 /*< non-standard, for CBCH/SDCCH4 */
52#define ABIS_RSL_CHAN_NR_CBITS_OSMO_CBCH8 0x1a /*< non-standard, for CBCH/SDCCH8 */
53
54/* non-standard, Osmocom specific Bm/Lm equivalents for VAMOS */
55#define ABIS_RSL_CHAN_NR_CBITS_OSMO_VAMOS_Bm_ACCHs 0x1d /*< VAMOS TCH/F */
56#define ABIS_RSL_CHAN_NR_CBITS_OSMO_VAMOS_Lm_ACCHs(ss) (0x1e + (ss)) /*< VAMOS TCH/H */
57
58/* Link Identifier 9.3.2 */
59 union abis_rsl_link_id {
60 struct {
61#if OSMO_IS_BIG_ENDIAN
62 uint8_t cbits:2,
63 na:1,
64 reserved:2,
65 sapi:3;
66#elif OSMO_IS_LITTLE_ENDIAN
67 uint8_t sapi:3,
68 reserved:2,
69 na:1,
70 cbits:2;
71#endif
72 } __attribute__ ((packed));
73 uint8_t link_id;
74} __attribute__ ((packed));
75#define ABIS_RSL_LINK_ID_CBITS_FACCH_SDCCH 0x00
76#define ABIS_RSL_LINK_ID_CBITS_SACCH 0x01
77
79 struct abis_rsl_common_hdr {
80 uint8_t msg_discr;
81 uint8_t msg_type;
82 uint8_t data[0];
83} __attribute__ ((packed));
84
85/* RSL RLL header (Chapter 8.3) */
86 struct abis_rsl_rll_hdr {
87 struct abis_rsl_common_hdr c;
88 uint8_t ie_chan;
89 union {
90 uint8_t chan_nr; /* API backward compat */
91 union abis_rsl_chan_nr chan_nr_fields;
92 };
93 uint8_t ie_link_id;
94 union {
95 uint8_t link_id; /* API backward compat */
96 union abis_rsl_link_id link_id_fields;
97 };
98 uint8_t data[0];
99} __attribute__ ((packed));
100
101/* RSL Dedicated Channel header (Chapter 8.3 and 8.4) */
102 struct abis_rsl_dchan_hdr {
103 struct abis_rsl_common_hdr c;
104 uint8_t ie_chan;
105 union {
106 uint8_t chan_nr; /* API backward compat */
107 union abis_rsl_chan_nr chan_nr_fields;
108 };
109 uint8_t data[0];
110} __attribute__ ((packed));
111
112/* RSL Common Channel header (Chapter 8.5) */
113 struct abis_rsl_cchan_hdr {
114 struct abis_rsl_common_hdr c;
115 uint8_t ie_chan;
116 union {
117 uint8_t chan_nr; /* API backward compat */
118 union abis_rsl_chan_nr chan_nr_fields;
119 };
120 uint8_t data[0];
121} __attribute__ ((packed));
122
123/* Osmocom specific IE to negotiate repeated ACCH capabilities */
124 struct abis_rsl_osmo_rep_acch_cap {
125#if OSMO_IS_LITTLE_ENDIAN
126 uint8_t dl_facch_cmd:1,
127 dl_facch_all:1,
128 dl_sacch:1,
129 ul_sacch:1,
130 rxqual:3,
131 reserved:1;
132#elif OSMO_IS_BIG_ENDIAN
133/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
134 uint8_t reserved:1, rxqual:3, ul_sacch:1, dl_sacch:1, dl_facch_all:1, dl_facch_cmd:1;
135#endif
136} __attribute__ ((packed));
137
138/* Osmocom specific IE to negotiate temporary overpower of ACCH channels */
139 struct abis_rsl_osmo_temp_ovp_acch_cap {
140#if OSMO_IS_LITTLE_ENDIAN
141 uint8_t overpower_db:3,
142 rxqual:3,
143 facch_enable:1,
144 sacch_enable:1;
145#elif OSMO_IS_BIG_ENDIAN
146/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
147 uint8_t sacch_enable:1, facch_enable:1, rxqual:3, overpower_db:3;
148#endif
149} __attribute__ ((packed));
150
151/* Chapter 9.1 */
152/* RSL Message Discriminator: RLL */
153#define ABIS_RSL_MDISC_RLL 0x02
154/* RSL Message Discriminator: Dedicated Channel */
155#define ABIS_RSL_MDISC_DED_CHAN 0x08
156/* RSL Message Discriminator: Common Channel */
157#define ABIS_RSL_MDISC_COM_CHAN 0x0c
158/* RSL Message Discriminator: TRX Management */
159#define ABIS_RSL_MDISC_TRX 0x10
160/* RSL Message Discriminator: Location Service */
161#define ABIS_RSL_MDISC_LOC 0x20
162/* RSL Message Discriminator: ip.access */
163#define ABIS_RSL_MDISC_IPACCESS 0x7e
164#define ABIS_RSL_MDISC_TRANSP 0x01
165
166/* Check if given RSL message discriminator is transparent */
167#define ABIS_RSL_MDISC_IS_TRANSP(x) (x & 0x01)
168
169/* RSL Message Type (Chapter 9.1) */
170 enum abis_rsl_msgtype {
171 /* Radio Link Layer Management */
172 RSL_MT_DATA_REQ = 0x01,
173 RSL_MT_DATA_IND,
174 RSL_MT_ERROR_IND,
175 RSL_MT_EST_REQ,
176 RSL_MT_EST_CONF,
177 RSL_MT_EST_IND,
178 RSL_MT_REL_REQ,
179 RSL_MT_REL_CONF,
180 RSL_MT_REL_IND,
181 RSL_MT_UNIT_DATA_REQ,
182 RSL_MT_UNIT_DATA_IND, /* 0x0b */
183 RSL_MT_SUSP_REQ, /* non-standard elements */
184 RSL_MT_SUSP_CONF,
185 RSL_MT_RES_REQ,
186 RSL_MT_RECON_REQ, /* 0x0f */
187
188 /* Common Channel Management / TRX Management */
189 RSL_MT_BCCH_INFO = 0x11,
190 RSL_MT_CCCH_LOAD_IND,
191 RSL_MT_CHAN_RQD,
192 RSL_MT_DELETE_IND,
193 RSL_MT_PAGING_CMD,
194 RSL_MT_IMMEDIATE_ASSIGN_CMD,
195 RSL_MT_SMS_BC_REQ,
196 RSL_MT_CHAN_CONF, /* non-standard element */
197 /* empty */
198 RSL_MT_RF_RES_IND = 0x19,
199 RSL_MT_SACCH_FILL,
200 RSL_MT_OVERLOAD,
201 RSL_MT_ERROR_REPORT,
202 RSL_MT_SMS_BC_CMD,
203 RSL_MT_CBCH_LOAD_IND,
204 RSL_MT_NOT_CMD, /* 0x1f */
205
206 /* Dedicate Channel Management */
207 RSL_MT_CHAN_ACTIV = 0x21,
208 RSL_MT_CHAN_ACTIV_ACK,
209 RSL_MT_CHAN_ACTIV_NACK,
210 RSL_MT_CONN_FAIL,
211 RSL_MT_DEACTIVATE_SACCH,
212 RSL_MT_ENCR_CMD,
213 RSL_MT_HANDO_DET,
214 RSL_MT_MEAS_RES,
215 RSL_MT_MODE_MODIFY_REQ,
216 RSL_MT_MODE_MODIFY_ACK,
217 RSL_MT_MODE_MODIFY_NACK,
218 RSL_MT_PHY_CONTEXT_REQ,
219 RSL_MT_PHY_CONTEXT_CONF,
220 RSL_MT_RF_CHAN_REL,
221 RSL_MT_MS_POWER_CONTROL,
222 RSL_MT_BS_POWER_CONTROL, /* 0x30 */
223 RSL_MT_PREPROC_CONFIG,
224 RSL_MT_PREPROC_MEAS_RES,
225 RSL_MT_RF_CHAN_REL_ACK,
226 RSL_MT_SACCH_INFO_MODIFY,
227 RSL_MT_TALKER_DET,
228 RSL_MT_LISTENER_DET,
229 RSL_MT_REMOTE_CODEC_CONF_REP,
230 RSL_MT_RTD_REP,
231 RSL_MT_PRE_HANDO_NOTIF,
232 RSL_MT_MR_CODEC_MOD_REQ,
233 RSL_MT_MR_CODEC_MOD_ACK,
234 RSL_MT_MR_CODEC_MOD_NACK,
235 RSL_MT_MR_CODEC_MOD_PER,
236 RSL_MT_TFO_REP,
237 RSL_MT_TFO_MOD_REQ, /* 0x3f */
238 RSL_MT_LOCATION_INFO = 0x41,
239
240 /* ip.access specific RSL message types */
241 RSL_MT_IPAC_DIR_RETR_ENQ = 0x40,
242 RSL_MT_IPAC_PDCH_ACT = 0x48,
243 RSL_MT_IPAC_PDCH_ACT_ACK,
244 RSL_MT_IPAC_PDCH_ACT_NACK,
245 RSL_MT_IPAC_PDCH_DEACT = 0x4b,
246 RSL_MT_IPAC_PDCH_DEACT_ACK,
247 RSL_MT_IPAC_PDCH_DEACT_NACK,
248 RSL_MT_IPAC_CONNECT_MUX = 0x50,
249 RSL_MT_IPAC_CONNECT_MUX_ACK,
250 RSL_MT_IPAC_CONNECT_MUX_NACK,
251 RSL_MT_IPAC_BIND_MUX = 0x53,
252 RSL_MT_IPAC_BIND_MUX_ACK,
253 RSL_MT_IPAC_BIND_MUX_NACK,
254 RSL_MT_IPAC_DISC_MUX = 0x56,
255 RSL_MT_IPAC_DISC_MUX_ACK,
256 RSL_MT_IPAC_DISC_MUX_NACK,
257 RSL_MT_IPAC_MEAS_PREPROC_DFT = 0x60, /*Extented Common Channel Management */
258 RSL_MT_IPAC_HO_CAN_ENQ = 0x61,
259 RSL_MT_IPAC_HO_CAN_RES = 0x62,
260 RSL_MT_IPAC_CRCX = 0x70, /* Bind to local BTS RTP port */
261 RSL_MT_IPAC_CRCX_ACK,
262 RSL_MT_IPAC_CRCX_NACK,
263 RSL_MT_IPAC_MDCX = 0x73,
264 RSL_MT_IPAC_MDCX_ACK,
265 RSL_MT_IPAC_MDCX_NACK,
266 RSL_MT_IPAC_DLCX_IND = 0x76,
267 RSL_MT_IPAC_DLCX = 0x77,
268 RSL_MT_IPAC_DLCX_ACK,
269 RSL_MT_IPAC_DLCX_NACK,
270
271 RSL_MT_OSMO_ETWS_CMD = 0x7f,
272};
273
275 enum abis_rsl_msgtype_siemens {
276 RSL_MT_SIEMENS_MRPCI = 0x41,
277 RSL_MT_SIEMENS_INTRAC_HO_COND_IND = 0x42,
278 RSL_MT_SIEMENS_INTERC_HO_COND_IND = 0x43,
279 RSL_MT_SIEMENS_FORCED_HO_REQ = 0x44,
280 RSL_MT_SIEMENS_PREF_AREA_REQ = 0x45,
281 RSL_MT_SIEMENS_PREF_AREA = 0x46,
282 RSL_MT_SIEMENS_START_TRACE = 0x47,
283 RSL_MT_SIEMENS_START_TRACE_ACK = 0x48,
284 RSL_MT_SIEMENS_STOP_TRACE = 0x49,
285 RSL_MT_SIEMENS_TRMR = 0x4a,
286 RSL_MT_SIEMENS_HO_FAIL_IND = 0x4b,
287 RSL_MT_SIEMENS_STOP_TRACE_ACK = 0x4c,
288 RSL_MT_SIEMENS_UPLF = 0x4d,
289 RSL_MT_SIEMENS_UPLB = 0x4e,
290 RSL_MT_SIEMENS_SET_SYS_INFO_10 = 0x4f,
291 RSL_MT_SIEMENS_MODIF_COND_IND = 0x50,
292};
293
295 enum abis_rsl_msgtype_ericsson {
296 RSL_MT_ERICSSON_IMM_ASS_SENT = 0x10,
297};
298
300 enum abis_rsl_ie {
301 RSL_IE_CHAN_NR = 0x01,
302 RSL_IE_LINK_IDENT,
303 RSL_IE_ACT_TYPE,
304 RSL_IE_BS_POWER,
305 RSL_IE_CHAN_IDENT,
306 RSL_IE_CHAN_MODE,
307 RSL_IE_ENCR_INFO,
308 RSL_IE_FRAME_NUMBER,
309 RSL_IE_HANDO_REF,
310 RSL_IE_L1_INFO,
311 RSL_IE_L3_INFO,
312 RSL_IE_MS_IDENTITY,
313 RSL_IE_MS_POWER,
314 RSL_IE_PAGING_GROUP,
315 RSL_IE_PAGING_LOAD,
316 RSL_IE_PYHS_CONTEXT = 0x10,
317 RSL_IE_ACCESS_DELAY,
318 RSL_IE_RACH_LOAD,
319 RSL_IE_REQ_REFERENCE,
320 RSL_IE_RELEASE_MODE,
321 RSL_IE_RESOURCE_INFO,
322 RSL_IE_RLM_CAUSE,
323 RSL_IE_STARTNG_TIME,
324 RSL_IE_TIMING_ADVANCE,
325 RSL_IE_UPLINK_MEAS,
326 RSL_IE_CAUSE,
327 RSL_IE_MEAS_RES_NR,
328 RSL_IE_MSG_ID,
329 /* reserved */
330 RSL_IE_SYSINFO_TYPE = 0x1e,
331 RSL_IE_MS_POWER_PARAM,
332 RSL_IE_BS_POWER_PARAM,
333 RSL_IE_PREPROC_PARAM,
334 RSL_IE_PREPROC_MEAS,
335 RSL_IE_IMM_ASS_INFO, /* Phase 1 (3.6.0), later Full below */
336 RSL_IE_SMSCB_INFO = 0x24,
337 RSL_IE_MS_TIMING_OFFSET,
338 RSL_IE_ERR_MSG,
339 RSL_IE_FULL_BCCH_INFO,
340 RSL_IE_CHAN_NEEDED,
341 RSL_IE_CB_CMD_TYPE,
342 RSL_IE_SMSCB_MSG,
343 RSL_IE_FULL_IMM_ASS_INFO,
344 RSL_IE_SACCH_INFO,
345 RSL_IE_CBCH_LOAD_INFO,
346 RSL_IE_SMSCB_CHAN_INDICATOR,
347 RSL_IE_GROUP_CALL_REF,
348 RSL_IE_CHAN_DESC = 0x30,
349 RSL_IE_NCH_DRX_INFO,
350 RSL_IE_CMD_INDICATOR,
351 RSL_IE_EMLPP_PRIO,
352 RSL_IE_UIC,
353 RSL_IE_MAIN_CHAN_REF,
354 RSL_IE_MR_CONFIG,
355 RSL_IE_MR_CONTROL,
356 RSL_IE_SUP_CODEC_TYPES,
357 RSL_IE_CODEC_CONFIG,
358 RSL_IE_RTD,
359 RSL_IE_TFO_STATUS,
360 RSL_IE_LLP_APDU,
361 RSL_IE_TFO_XPAR_CONT,
362 /* Siemens vendor-specific */
363 RSL_IE_SIEMENS_MRPCI = 0x40,
364 RSL_IE_SIEMENS_PREF_AREA_TYPE = 0x43,
365 RSL_IE_SIEMENS_ININ_CELL_HO_PAR = 0x45,
366 RSL_IE_SIEMENS_TRACE_REF_NR = 0x46,
367 RSL_IE_SIEMENS_INT_TRACE_IDX = 0x47,
368 RSL_IE_SIEMENS_L2_HDR_INFO = 0x48,
369 RSL_IE_SIEMENS_HIGHEST_RATE = 0x4e,
370 RSL_IE_SIEMENS_SUGGESTED_RATE = 0x4f,
371
372 /* Osmocom specific */
373 RSL_IE_OSMO_REP_ACCH_CAP = 0x60,
374 RSL_IE_OSMO_TRAINING_SEQUENCE = 0x61,
375 RSL_IE_OSMO_TEMP_OVP_ACCH_CAP = 0x62,
376 RSL_IE_OSMO_OSMUX_CID = 0x63,
377 RSL_IE_OSMO_RTP_EXTENSIONS = 0x64,
378
379 /* ip.access */
380 RSL_IE_IPAC_SRTP_CONFIG = 0xe0,
381 RSL_IE_IPAC_PROXY_UDP = 0xe1,
382 RSL_IE_IPAC_BSCMPL_TOUT = 0xe2,
383 RSL_IE_IPAC_REMOTE_IP = 0xf0,
384 RSL_IE_IPAC_REMOTE_PORT = 0xf1,
385 RSL_IE_IPAC_RTP_PAYLOAD = 0xf2,
386 RSL_IE_IPAC_LOCAL_PORT = 0xf3,
387 RSL_IE_IPAC_SPEECH_MODE = 0xf4,
388 RSL_IE_IPAC_LOCAL_IP = 0xf5,
389 RSL_IE_IPAC_CONN_STAT = 0xf6,
390 RSL_IE_IPAC_HO_C_PARMS = 0xf7,
391 RSL_IE_IPAC_CONN_ID = 0xf8,
392 RSL_IE_IPAC_RTP_CSD_FMT = 0xf9,
393 RSL_IE_IPAC_RTP_JIT_BUF = 0xfa,
394 RSL_IE_IPAC_RTP_COMPR = 0xfb,
395 RSL_IE_IPAC_RTP_PAYLOAD2 = 0xfc,
396 RSL_IE_IPAC_RTP_MPLEX = 0xfd,
397 RSL_IE_IPAC_RTP_MPLEX_ID = 0xfe,
398};
399
400/* Ericsson specific IEs, clash with above partially, so they're not
401 * part of the enum */
402#define RSL_IE_ERIC_PAGING_GROUP 0x0e
403#define RSL_IE_ERIC_INST_NR 0x48
404#define RSL_IE_ERIC_PGSL_TIMERS 0x49
405#define RSL_IE_ERIC_REPEAT_DL_FACCH 0x4a
406#define RSL_IE_ERIC_POWER_INFO 0xf0
407#define RSL_IE_ERIC_MOBILE_ID 0xf1
408#define RSL_IE_ERIC_BCCH_MAPPING 0xf2
409#define RSL_IE_ERIC_PACKET_PAG_IND 0xf3
410#define RSL_IE_ERIC_CNTR_CTRL 0xf4
411#define RSL_IE_ERIC_CNTR_CTRL_ACK 0xf5
412#define RSL_IE_ERIC_CNTR_REPORT 0xf6
413#define RSL_IE_ERIC_ICP_CONN 0xf7
414#define RSL_IE_ERIC_EMR_SUPPORT 0xf8
415#define RSL_IE_ERIC_EGPRS_REQ_REF 0xf9
416#define RSL_IE_ERIC_VGCS_REL 0xfa
417#define RSL_IE_ERIC_REP_PER_NCH 0xfb
418#define RSL_IE_ERIC_NY2 0xfc
419#define RSL_IE_ERIC_T3115 0xfd
420#define RSL_IE_ERIC_ACTIVATE_FLAG 0xfe
421#define RSL_IE_ERIC_FULL_NCH_INFO 0xff
422
423/* IPAC MEAS_PREPROC AVERAGING METHOD */
424 enum {
425 IPAC_UNWEIGHTED_AVE = 0,
426 IPAC_WEIGHTED_AVE,
427 IPAC_MEDIAN_AVE,
428 /* EWMA is an Osmocom specific extension */
429 IPAC_OSMO_EWMA_AVE,
430};
431
432/* IPAC MEAS_PREPROC AVERAGING PARAM ID */
433 enum {
434 IPAC_RXLEV_AVE = 0,
435 IPAC_RXQUAL_AVE,
436 IPAC_MS_BTS_DIS_AVE
437};
438
439/* IPAC MEAS_PREPROC HO CAUSES */
440 enum {
441 IPAC_HO_RQD_CAUSE_L_RXLEV_UL_H = 0x01,
442 IPAC_HO_RQD_CAUSE_L_RXLEV_DL_H,
443 IPAC_HO_RQD_CAUSE_L_RXQUAL_UL_H,
444 IPAC_HO_RQD_CAUSE_L_RXQUAL_DL_H,
445 IPAC_HO_RQD_CAUSE_RXLEV_UL_IH,
446 IPAC_HO_RQD_CAUSE_RXLEV_DL_IH,
447 IPAC_HO_RQD_CAUSE_MAX_MS_RANGE,
448 IPAC_HO_RQD_CAUSE_POWER_BUDGET,
449 IPAC_HO_RQD_CAUSE_ENQUIRY,
450 IPAC_HO_RQD_CAUSE_ENQUIRY_FAILED,
451 IPAC_HO_RQD_CAUSE_NORMAL3G,
452 IPAC_HO_RQD_CAUSE_EMERGENCY3G,
453 IPAC_HO_RQD_CAUSE_SERVICE_PREFERRED3G,
454 IPAC_HO_RQD_CAUSE_O_M_SHUTDOWN,
455 IPAC_HO_RQD_CAUSE_QUALITY_PROMOTION,
456 IPAC_HO_RQD_CAUSE_LOAD_PROMOTION,
457 IPAC_HO_RQD_CAUSE_LOAD_DEMOTION,
458 IPAC_HO_RQD_CAUSE_MAX,
459};
460
461/* Chapter 9.3.1 */
462#define RSL_CHAN_NR_MASK 0xf8
463#define RSL_CHAN_NR_1 0x08 /*< bit to add for 2nd,... lchan */
464#define RSL_CHAN_Bm_ACCHs 0x08
465#define RSL_CHAN_Lm_ACCHs 0x10 /* .. 0x18 */
466#define RSL_CHAN_SDCCH4_ACCH 0x20 /* .. 0x38 */
467#define RSL_CHAN_SDCCH8_ACCH 0x40 /* ...0x78 */
468#define RSL_CHAN_BCCH 0x80
469#define RSL_CHAN_RACH 0x88
470#define RSL_CHAN_PCH_AGCH 0x90
471#define RSL_CHAN_OSMO_PDCH 0xc0 /*< non-standard, for dyn TS */
472#define RSL_CHAN_OSMO_CBCH4 0xc8 /*< non-standard, for CBCH/SDCCH4 */
473#define RSL_CHAN_OSMO_CBCH8 0xd0 /*< non-standard, for CBCH/SDCCH8 */
474
475/* non-standard, Osmocom specific Bm/Lm equivalents for VAMOS */
476#define RSL_CHAN_OSMO_VAMOS_Bm_ACCHs 0xe8 /* VAMOS TCH/F */
477#define RSL_CHAN_OSMO_VAMOS_Lm_ACCHs 0xf0 /* VAMOS TCH/H */
478#define RSL_CHAN_OSMO_VAMOS_MASK 0xe0 /* VAMOS TCH/{F,H} */
479
480/* Chapter 9.3.3 */
481#define RSL_ACT_TYPE_INITIAL 0x00
482#define RSL_ACT_TYPE_REACT 0x80
483#define RSL_ACT_INTRA_IMM_ASS 0x00
484#define RSL_ACT_INTRA_NORM_ASS 0x01
485#define RSL_ACT_INTER_ASYNC 0x02
486#define RSL_ACT_INTER_SYNC 0x03
487#define RSL_ACT_SECOND_ADD 0x04
488#define RSL_ACT_SECOND_MULTI 0x05
489#define RSL_ACT_OSMO_PDCH 0x0f /*< non-standard, for dyn TS */
490
492 struct rsl_ie_chan_mode {
493 uint8_t dtx_dtu;
494 uint8_t spd_ind;
495 uint8_t chan_rt;
496 uint8_t chan_rate;
497} __attribute__ ((packed));
498#define RSL_CMOD_DTXu 0x01 /* uplink */
499#define RSL_CMOD_DTXd 0x02 /* downlink */
500 enum rsl_cmod_spd {
501 RSL_CMOD_SPD_SPEECH = 0x01,
502 RSL_CMOD_SPD_DATA = 0x02,
503 RSL_CMOD_SPD_SIGN = 0x03,
504};
506 enum rsl_cmod_crt {
507 RSL_CMOD_CRT_SDCCH = 0x01,
508 RSL_CMOD_CRT_TCH_Bm = 0x08, /* full-rate */
509 RSL_CMOD_CRT_TCH_Lm = 0x09, /* half-rate */
510 RSL_CMOD_CRT_TCH_BI_Bm = 0x0a, /* full-rate: bi-directional (multislot) */
511 RSL_CMOD_CRT_TCH_UNI_Bm = 0x1a, /* full-rate: uni-directional (multislot) */
512 RSL_CMOD_CRT_TCH_GROUP_Bm = 0x18, /* full-rate: group call channel */
513 RSL_CMOD_CRT_TCH_GROUP_Lm = 0x19, /* half-rate: group call channel */
514 RSL_CMOD_CRT_TCH_BCAST_Bm = 0x28, /* full-rate: broadcast call channel */
515 RSL_CMOD_CRT_TCH_BCAST_Lm = 0x29, /* half-rate: broadcast call channel */
516 RSL_CMOD_CRT_OSMO_TCH_VAMOS_Bm = 0x88, /* full-rate in VAMOS mode */
517 RSL_CMOD_CRT_OSMO_TCH_VAMOS_Lm = 0x89, /* half-rate in VAMOS mode */
518};
520 enum rsl_cmod_sp {
521 RSL_CMOD_SP_GSM1 = 0x01,
522 RSL_CMOD_SP_GSM2 = 0x11,
523 RSL_CMOD_SP_GSM3 = 0x21,
524 RSL_CMOD_SP_GSM4 = 0x31,
525 RSL_CMOD_SP_GSM5 = 0x09,
526 RSL_CMOD_SP_GSM6 = 0x0d,
527};
529 enum rsl_cmod_csd_nt {
530 RSL_CMOD_CSD_NTA_43k5_14k5 = 0x61, /* asymmetric 43.5 kbit/s (DL) + 14.5 kbit/s (UL) */
531 RSL_CMOD_CSD_NTA_29k0_14k5 = 0x62, /* asymmetric 29.0 kbit/s (DL) + 14.5 kbit/s (UL) */
532 RSL_CMOD_CSD_NTA_43k5_29k0 = 0x63, /* asymmetric 43.5 kbit/s (DL) + 29.0 kbit/s (UL) */
533 RSL_CMOD_CSD_NTA_14k5_43k5 = 0x69, /* asymmetric 14.5 kbit/s (DL) + 43.5 kbit/s (UL) */
534 RSL_CMOD_CSD_NTA_14k5_29k0 = 0x6a, /* asymmetric 14.5 kbit/s (DL) + 29.0 kbit/s (UL) */
535 RSL_CMOD_CSD_NTA_29k0_43k5 = 0x6b, /* asymmetric 29.0 kbit/s (DL) + 43.5 kbit/s (UL) */
536 RSL_CMOD_CSD_NT_43k5 = 0x74,
537 RSL_CMOD_CSD_NT_28k8 = 0x71,
538 RSL_CMOD_CSD_NT_14k5 = 0x58,
539 RSL_CMOD_CSD_NT_12k0 = 0x50,
540 RSL_CMOD_CSD_NT_6k0 = 0x51,
541};
542/* legacy #defines with wrong name */
543#define RSL_CMOD_SP_NT_14k5 RSL_CMOD_CSD_NT_14k5
544#define RSL_CMOD_SP_NT_12k0 RSL_CMOD_CSD_NT_12k0
545#define RSL_CMOD_SP_NT_6k0 RSL_CMOD_CSD_NT_6k0
546#define RSL_CMOD_CSD_T_32000 RSL_CMOD_CSD_T_32k0
547#define RSL_CMOD_CSD_T_29000 RSL_CMOD_CSD_T_29k0
548#define RSL_CMOD_CSD_T_14400 RSL_CMOD_CSD_T_14k4
549#define RSL_CMOD_CSD_T_9600 RSL_CMOD_CSD_T_9k6
550#define RSL_CMOD_CSD_T_4800 RSL_CMOD_CSD_T_4k8
551#define RSL_CMOD_CSD_T_2400 RSL_CMOD_CSD_T_2k4
552#define RSL_CMOD_CSD_T_1200 RSL_CMOD_CSD_T_1k2
554 enum rsl_cmod_csd_t {
555 RSL_CMOD_CSD_T_32k0 = 0x38,
556 RSL_CMOD_CSD_T_29k0 = 0x39,
557 RSL_CMOD_CSD_T_14k4 = 0x18,
558 RSL_CMOD_CSD_T_9k6 = 0x10,
559 RSL_CMOD_CSD_T_4k8 = 0x11,
560 RSL_CMOD_CSD_T_2k4 = 0x12,
561 RSL_CMOD_CSD_T_1k2 = 0x13,
562 RSL_CMOD_CSD_T_600 = 0x14,
563 RSL_CMOD_CSD_T_1200_75 = 0x15,
564};
565
567 struct rsl_ie_chan_ident {
568 /* GSM 04.08 10.5.2.5 */
569 struct {
570 uint8_t iei;
571 uint8_t chan_nr; /* enc_chan_nr */
572 uint8_t oct3;
573 uint8_t oct4;
574 } chan_desc;
575#if 0 /* spec says we need this but Abissim doesn't use it */
576 struct {
577 uint8_t tag;
578 uint8_t len;
579 } mobile_alloc;
580#endif
581} __attribute__ ((packed));
582
583/* Chapter 9.3.22 */
584#define RLL_CAUSE_T200_EXPIRED 0x01
585#define RLL_CAUSE_REEST_REQ 0x02
586#define RLL_CAUSE_UNSOL_UA_RESP 0x03
587#define RLL_CAUSE_UNSOL_DM_RESP 0x04
588#define RLL_CAUSE_UNSOL_DM_RESP_MF 0x05
589#define RLL_CAUSE_UNSOL_SPRV_RESP 0x06
590#define RLL_CAUSE_SEQ_ERR 0x07
591#define RLL_CAUSE_UFRM_INC_PARAM 0x08
592#define RLL_CAUSE_SFRM_INC_PARAM 0x09
593#define RLL_CAUSE_IFRM_INC_MBITS 0x0a
594#define RLL_CAUSE_IFRM_INC_LEN 0x0b
595#define RLL_CAUSE_FRM_UNIMPL 0x0c
596#define RLL_CAUSE_SABM_MF 0x0d
597#define RLL_CAUSE_SABM_INFO_NOTALL 0x0e
598
599/* Chapter 9.3.26 */
600#define RSL_ERRCLS_NORMAL 0x00
601#define RSL_ERRCLS_RESOURCE_UNAVAIL 0x20
602#define RSL_ERRCLS_SERVICE_UNAVAIL 0x30
603#define RSL_ERRCLS_SERVICE_UNIMPL 0x40
604#define RSL_ERRCLS_INVAL_MSG 0x50
605#define RSL_ERRCLS_PROTO_ERROR 0x60
606#define RSL_ERRCLS_INTERWORKING 0x70
607
608/* normal event */
609#define RSL_ERR_RADIO_IF_FAIL 0x00
610#define RSL_ERR_RADIO_LINK_FAIL 0x01
611#define RSL_ERR_HANDOVER_ACC_FAIL 0x02
612#define RSL_ERR_TALKER_ACC_FAIL 0x03
613#define RSL_ERR_OM_INTERVENTION 0x07
614#define RSL_ERR_NORMAL_UNSPEC 0x0f
615#define RSL_ERR_T_MSRFPCI_EXP 0x18
616/* resource unavailable */
617#define RSL_ERR_EQUIPMENT_FAIL 0x20
618#define RSL_ERR_RR_UNAVAIL 0x21
619#define RSL_ERR_TERR_CH_FAIL 0x22
620#define RSL_ERR_CCCH_OVERLOAD 0x23
621#define RSL_ERR_ACCH_OVERLOAD 0x24
622#define RSL_ERR_PROCESSOR_OVERLOAD 0x25
623#define RSL_ERR_BTS_NOT_EQUIPPED 0x27
624#define RSL_ERR_REMOTE_TRANSC_FAIL 0x28
625#define RSL_ERR_NOTIFICATION_OVERFL 0x29
626#define RSL_ERR_RES_UNAVAIL 0x2f
627/* service or option not available */
628#define RSL_ERR_TRANSC_UNAVAIL 0x30
629#define RSL_ERR_SERV_OPT_UNAVAIL 0x3f
630/* service or option not implemented */
631#define RSL_ERR_ENCR_UNIMPL 0x40
632#define RSL_ERR_SERV_OPT_UNIMPL 0x4f
633/* invalid message */
634#define RSL_ERR_RCH_ALR_ACTV_ALLOC 0x50
635#define RSL_ERR_INVALID_MESSAGE 0x5f
636/* protocol error */
637#define RSL_ERR_MSG_DISCR 0x60
638#define RSL_ERR_MSG_TYPE 0x61
639#define RSL_ERR_MSG_SEQ 0x62
640#define RSL_ERR_IE_ERROR 0x63
641#define RSL_ERR_MAND_IE_ERROR 0x64
642#define RSL_ERR_OPT_IE_ERROR 0x65
643#define RSL_ERR_IE_NONEXIST 0x66
644#define RSL_ERR_IE_LENGTH 0x67
645#define RSL_ERR_IE_CONTENT 0x68
646#define RSL_ERR_PROTO 0x6f
647/* interworking */
648#define RSL_ERR_INTERWORKING 0x7f
649
650/* Chapter 9.3.30 */
651#define RSL_SYSTEM_INFO_8 0x00
652#define RSL_SYSTEM_INFO_1 0x01
653#define RSL_SYSTEM_INFO_2 0x02
654#define RSL_SYSTEM_INFO_3 0x03
655#define RSL_SYSTEM_INFO_4 0x04
656#define RSL_SYSTEM_INFO_5 0x05
657#define RSL_SYSTEM_INFO_6 0x06
658#define RSL_SYSTEM_INFO_7 0x07
659#define RSL_SYSTEM_INFO_16 0x08
660#define RSL_SYSTEM_INFO_17 0x09
661#define RSL_SYSTEM_INFO_2bis 0x0a
662#define RSL_SYSTEM_INFO_2ter 0x0b
663#define RSL_SYSTEM_INFO_5bis 0x0d
664#define RSL_SYSTEM_INFO_5ter 0x0e
665#define RSL_SYSTEM_INFO_10 0x0f
666#define RSL_EXT_MEAS_ORDER 0x47
667#define RSL_MEAS_INFO 0x48
668#define RSL_SYSTEM_INFO_13 0x28
669#define RSL_ERIC_SYSTEM_INFO_13 0x0C
670#define RSL_SYSTEM_INFO_2quater 0x29
671#define RSL_SYSTEM_INFO_9 0x2a
672#define RSL_SYSTEM_INFO_18 0x2b
673#define RSL_SYSTEM_INFO_19 0x2c
674#define RSL_SYSTEM_INFO_20 0x2d
675
676/* Chapter 9.3.40 */
677#define RSL_CHANNEED_ANY 0x00
678#define RSL_CHANNEED_SDCCH 0x01
679#define RSL_CHANNEED_TCH_F 0x02
680#define RSL_CHANNEED_TCH_ForH 0x03
681
683 struct rsl_ie_cb_cmd_type {
684#if OSMO_IS_LITTLE_ENDIAN
685 uint8_t last_block:2;
686 uint8_t spare:1;
687 uint8_t def_bcast:1;
688 uint8_t command:4;
689#elif OSMO_IS_BIG_ENDIAN
690/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
691 uint8_t command:4, def_bcast:1, spare:1, last_block:2;
692#endif
693} __attribute__ ((packed));
694/* ->command */
695#define RSL_CB_CMD_TYPE_NORMAL 0x00
696#define RSL_CB_CMD_TYPE_SCHEDULE 0x08
697#define RSL_CB_CMD_TYPE_DEFAULT 0x0e
698#define RSL_CB_CMD_TYPE_NULL 0x0f
699/* ->def_bcast */
700#define RSL_CB_CMD_DEFBCAST_NORMAL 0
701#define RSL_CB_CMD_DEFBCAST_NULL 1
702/* ->last_block */
703#define RSL_CB_CMD_LASTBLOCK_4 0
704#define RSL_CB_CMD_LASTBLOCK_1 1
705#define RSL_CB_CMD_LASTBLOCK_2 2
706#define RSL_CB_CMD_LASTBLOCK_3 3
707
709 struct rsl_ie_nch_drx_info {
710#if OSMO_IS_LITTLE_ENDIAN
711 uint8_t nln:2;
712 uint8_t emlpp_priority:3;
713 uint8_t nln_status:1;
714 uint8_t spare:2;
715#elif OSMO_IS_BIG_ENDIAN
716/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
717 uint8_t spare:2, nln_status:1, emlpp_priority:3, nln:2;
718#endif
719} __attribute__ ((packed));
720
722#define RSL_CMD_INDICATOR_START 0x00
723#define RSL_CMD_INDICATOR_STOP 0x01
724
725/* Chapter 3.3.2.3 Brocast control channel */
726/* CCCH-CONF, NC is not combined */
727#define RSL_BCCH_CCCH_CONF_1_NC 0x00
728#define RSL_BCCH_CCCH_CONF_1_C 0x01
729#define RSL_BCCH_CCCH_CONF_2_NC 0x02
730#define RSL_BCCH_CCCH_CONF_3_NC 0x04
731#define RSL_BCCH_CCCH_CONF_4_NC 0x06
732
733/* BS-PA-MFRMS */
734#define RSL_BS_PA_MFRMS_2 0x00
735#define RSL_BS_PA_MFRMS_3 0x01
736#define RSL_BS_PA_MFRMS_4 0x02
737#define RSL_BS_PA_MFRMS_5 0x03
738#define RSL_BS_PA_MFRMS_6 0x04
739#define RSL_BS_PA_MFRMS_7 0x05
740#define RSL_BS_PA_MFRMS_8 0x06
741#define RSL_BS_PA_MFRMS_9 0x07
742
743/* RSL_IE_IPAC_RTP_PAYLOAD[2] */
744 enum rsl_ipac_rtp_payload {
745 RSL_IPAC_RTP_GSM = 1,
746 RSL_IPAC_RTP_EFR,
747 RSL_IPAC_RTP_AMR,
748 RSL_IPAC_RTP_CSD,
749 RSL_IPAC_RTP_MUX,
750};
751
752/* RSL_IE_IPAC_SPEECH_MODE, lower four bits */
753 enum rsl_ipac_speech_mode_s {
754 RSL_IPAC_SPEECH_GSM_FR = 0, /* GSM FR (Type 1, FS) */
755 RSL_IPAC_SPEECH_GSM_EFR = 1, /* GSM EFR (Type 2, FS) */
756 RSL_IPAC_SPEECH_GSM_AMR_FR = 2, /* GSM AMR/FR (Type 3, FS) */
757 RSL_IPAC_SPEECH_GSM_HR = 3, /* GSM HR (Type 1, HS) */
758 RSL_IPAC_SPEECH_GSM_AMR_HR = 5, /* GSM AMR/hr (Type 3, HS) */
759 RSL_IPAC_SPEECH_AS_RTP = 0xf, /* As specified by RTP Payload IE */
760};
761/* RSL_IE_IPAC_SPEECH_MODE, upper four bits */
762 enum rsl_ipac_speech_mode_m {
763 RSL_IPAC_SPEECH_M_RXTX = 0, /* Send and Receive */
764 RSL_IPAC_SPEECH_M_RX = 1, /* Receive only */
765 RSL_IPAC_SPEECH_M_TX = 2, /* Send only */
766};
767
768/* RSL_IE_IPAC_RTP_CSD_FMT, lower four bits */
769 enum rsl_ipac_rtp_csd_format_d {
770 RSL_IPAC_RTP_CSD_EXT_TRAU = 0,
771 RSL_IPAC_RTP_CSD_NON_TRAU = 1,
772 RSL_IPAC_RTP_CSD_TRAU_BTS = 2,
773 RSL_IPAC_RTP_CSD_IWF_FREE = 3,
774};
775/* RSL_IE_IPAC_RTP_CSD_FMT, upper four bits */
776 enum rsl_ipac_rtp_csd_format_ir {
777 RSL_IPAC_RTP_CSD_IR_8k = 0,
778 RSL_IPAC_RTP_CSD_IR_16k = 1,
779 RSL_IPAC_RTP_CSD_IR_32k = 2,
780 RSL_IPAC_RTP_CSD_IR_64k = 3,
781};
782
783/* Siemens vendor-specific RSL extensions */
784 struct rsl_mrpci {
785 uint8_t power_class:3,
786 vgcs_capable:1,
787 vbs_capable:1,
788 gsm_phase:2;
789} __attribute__ ((packed));
790
791 enum rsl_mrpci_pwrclass {
792 RSL_MRPCI_PWRC_1 = 0,
793 RSL_MRPCI_PWRC_2 = 1,
794 RSL_MRPCI_PWRC_3 = 2,
795 RSL_MRPCI_PWRC_4 = 3,
796 RSL_MRPCI_PWRC_5 = 4,
797};
798 enum rsl_mrpci_phase {
799 RSL_MRPCI_PHASE_1 = 0,
800 /* reserved */
801 RSL_MRPCI_PHASE_2 = 2,
802 RSL_MRPCI_PHASE_2PLUS = 3,
803};
804
805/* 9.3.20 Release Mode */
806 enum rsl_rel_mode {
807 RSL_REL_NORMAL = 0,
808 RSL_REL_LOCAL_END = 1,
809};
810
812 enum rsl_ipac_embedded_ie {
813 RSL_IPAC_EIE_RXLEV = 0x00,
814 RSL_IPAC_EIE_RXQUAL = 0x01,
815 RSL_IPAC_EIE_FREQ_ERR = 0x02,
816 RSL_IPAC_EIE_TIMING_ERR = 0x03,
817 RSL_IPAC_EIE_MEAS_AVG_CFG = 0x04,
818 RSL_IPAC_EIE_BS_PWR_CTL = 0x05,
819 RSL_IPAC_EIE_MS_PWR_CTL = 0x06,
820 RSL_IPAC_EIE_HANDO_THRESH = 0x07,
821 RSL_IPAC_EIE_NCELL_DEFAULTS = 0x08,
822 RSL_IPAC_EIE_NCELL_LIST = 0x09,
823 RSL_IPAC_EIE_PC_THRESH_COMP = 0x0a,
824 RSL_IPAC_EIE_HO_THRESH_COMP = 0x0b,
825 RSL_IPAC_EIE_HO_CAUSE = 0x0c,
826 RSL_IPAC_EIE_HO_CANDIDATES = 0x0d,
827 RSL_IPAC_EIE_NCELL_BA_CHG_LIST = 0x0e,
828 RSL_IPAC_EIE_NUM_OF_MS = 0x10,
829 RSL_IPAC_EIE_HO_CAND_EXT = 0x11,
830 RSL_IPAC_EIE_NCELL_DEF_EXT = 0x12,
831 RSL_IPAC_EIE_NCELL_LIST_EXT = 0x13,
832 RSL_IPAC_EIE_MASTER_KEY = 0x14,
833 RSL_IPAC_EIE_MASTER_SALT = 0x15,
834 /* additional IPAC measurement pre-processing related IEI */
835 RSL_IPAC_EIE_MEAS_TRANS_RES = 0x16,
836 RSL_IPAC_EIE_3G_HO_PARAM = 0x17,
837 RSL_IPAC_EIE_3G_NCELL_LIST = 0x18,
838 RSL_IPAC_EIE_SDCCH_CTL_PARAM = 0x1a,
839 RSL_IPAC_EIE_AMR_CONV_THRESH = 0x1b,
840
841 /* Osmocom specific extensions: */
842 RSL_IPAC_EIE_OSMO_MEAS_AVG_CFG = 0xf0,
843 RSL_IPAC_EIE_OSMO_MS_PWR_CTL = 0xf1,
844 RSL_IPAC_EIE_OSMO_PC_THRESH_COMP = 0xf2,
845
846};
847
848/* Value of TLV IE RSL_IPAC_EIE_MEAS_AVG_CFG */
849 struct ipac_preproc_ave_cfg {
850#if OSMO_IS_LITTLE_ENDIAN
851 uint8_t h_reqave:5,
852 param_id:2,
853 reserved:1;
854 uint8_t h_reqt:5,
855 ave_method:3;
856 uint8_t params[0];
857#elif OSMO_IS_BIG_ENDIAN
858/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
859 uint8_t reserved:1, param_id:2, h_reqave:5;
860 uint8_t ave_method:3, h_reqt:5;
861 uint8_t params[0];
862#endif
863}__attribute__ ((packed));
864
865
866 struct osmo_preproc_ave_cfg_field {
867#if OSMO_IS_LITTLE_ENDIAN
868 uint8_t h_reqave:5,
869 ave_enabled:1,
870 reserved:2;
871 uint8_t h_reqt:5,
872 ave_method:3;
873#elif OSMO_IS_BIG_ENDIAN
874/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
875 uint8_t reserved:2, ave_enabled:1, h_reqave:5;
876 uint8_t ave_method:3, h_reqt:5;
877#endif
878}__attribute__ ((packed));
879/* Value of TLV IE RSL_IPAC_EIE_OSMO_MEAS_AVG_CFG: */
880 struct osmo_preproc_ave_cfg {
881 struct osmo_preproc_ave_cfg_field ci_fr;
882 struct osmo_preproc_ave_cfg_field ci_hr;
883 struct osmo_preproc_ave_cfg_field ci_amr_fr;
884 struct osmo_preproc_ave_cfg_field ci_amr_hr;
885 struct osmo_preproc_ave_cfg_field ci_sdcch;
886 struct osmo_preproc_ave_cfg_field ci_gprs;
887 uint8_t params[0]; /* Contains params for each above, appended one after the other */
888}__attribute__ ((packed));
889
891 struct ipac_preproc_pc_thresh {
892#if OSMO_IS_LITTLE_ENDIAN
893 uint8_t l_rxlev:6, reserved_l_rxlev:2;
894 uint8_t u_rxlev:6, reserved_u_rxlev:2;
895 uint8_t u_rxqual:3, reserved_u_rxqual:1,
896 l_rxqual:3, reserved_l_rxqual:1;
897#elif OSMO_IS_BIG_ENDIAN
898/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
899 uint8_t reserved_l_rxlev:2, l_rxlev:6;
900 uint8_t reserved_u_rxlev:2, u_rxlev:6;
901 uint8_t reserved_l_rxqual:1, l_rxqual:3, reserved_u_rxqual:1, u_rxqual:3;
902#endif
903}__attribute__ ((packed));
904
906 struct osmo_preproc_pc_thresh {
907 /* Carrier-to-Interference (C/I), in dB: */
908 int8_t l_ci_fr; int8_t u_ci_fr; /* FR/EFR */
909 int8_t l_ci_hr; int8_t u_ci_hr; /* HR */
910 int8_t l_ci_amr_fr; int8_t u_ci_amr_fr; /* AMR FR */
911 int8_t l_ci_amr_hr; int8_t u_ci_amr_hr; /* AMR HR */
912 int8_t l_ci_sdcch; int8_t u_ci_sdcch; /* SDCCH */
913 int8_t l_ci_gprs; int8_t u_ci_gprs; /* GPRS */
914}__attribute__ ((packed));
915
917 struct ipac_preproc_ho_thresh {
918#if OSMO_IS_LITTLE_ENDIAN
919 uint8_t l_rxlev_ul_h:6,
920 reserved_l_rxlev_ul:2;
921 uint8_t l_rxlev_dl_h:6,
922 reserved_l_rxlev_dl:2;
923 uint8_t rxlev_ul_ih:6,
924 reserved_rxlev_ul:2;
925 uint8_t rxlev_dl_ih:6,
926 reserved_rxlev_dl:2;
927 uint8_t l_rxqual_ul_h:3,
928 reserved_rxlqual_ul:1,
929 l_rxqual_dl_h:3,
930 reserved_rxqual_dl:1;
931 uint8_t ms_range_max:6,
932 reserved_ms_range:2;
933#elif OSMO_IS_BIG_ENDIAN
934/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
935 uint8_t reserved_l_rxlev_ul:2, l_rxlev_ul_h:6;
936 uint8_t reserved_l_rxlev_dl:2, l_rxlev_dl_h:6;
937 uint8_t reserved_rxlev_ul:2, rxlev_ul_ih:6;
938 uint8_t reserved_rxlev_dl:2, rxlev_dl_ih:6;
939 uint8_t reserved_rxqual_dl:1, l_rxqual_dl_h:3, reserved_rxlqual_ul:1, l_rxqual_ul_h:3;
940 uint8_t reserved_ms_range:2, ms_range_max:6;
941#endif
942}__attribute__ ((packed));
943
945 struct ipac_preproc_pc_comp {
946#if OSMO_IS_LITTLE_ENDIAN
947 uint8_t p1:5, reserved_p1:3;
948 uint8_t n1:5, reserved_n1:3;
949 uint8_t p2:5, reserved_p2:3;
950 uint8_t n2:5, reserved_n2:3;
951 uint8_t p3:5, reserved_p3:3;
952 uint8_t n3:5, reserved_n3:3;
953 uint8_t p4:5, reserved_p4:3;
954 uint8_t n4:5, reserved_n4:3;
955 uint8_t pc_interval:5, reserved_pc:3;
956 uint8_t red_step_size:4, inc_step_size:4;
957#elif OSMO_IS_BIG_ENDIAN
958/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
959 uint8_t reserved_p1:3, p1:5;
960 uint8_t reserved_n1:3, n1:5;
961 uint8_t reserved_p2:3, p2:5;
962 uint8_t reserved_n2:3, n2:5;
963 uint8_t reserved_p3:3, p3:5;
964 uint8_t reserved_n3:3, n3:5;
965 uint8_t reserved_p4:3, p4:5;
966 uint8_t reserved_n4:3, n4:5;
967 uint8_t reserved_pc:3, pc_interval:5;
968 uint8_t inc_step_size:4, red_step_size:4;
969#endif
970}__attribute__ ((packed));
971
973 struct ipac_preproc_pc_comp_field {
974#if OSMO_IS_LITTLE_ENDIAN
975 uint8_t lower_p:5, reserved_lower_p:3;
976 uint8_t lower_n:5, reserved_lower_n:3;
977 uint8_t upper_p:5, reserved_upper_p:3;
978 uint8_t upper_n:5, reserved_upper_n:3;
979#elif OSMO_IS_BIG_ENDIAN
980/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
981 uint8_t reserved_lower_p:3, lower_p:5;
982 uint8_t reserved_lower_n:3, lower_n:5;
983 uint8_t reserved_upper_p:3, upper_p:5;
984 uint8_t reserved_upper_n:3, upper_n:5;
985#endif
986}__attribute__ ((packed));
987 struct osmo_preproc_pc_comp {
988 /* Used for Carrier-to-Interference (C/I), in dB: */
989 struct ipac_preproc_pc_comp_field ci_fr;
990 struct ipac_preproc_pc_comp_field ci_hr;
991 struct ipac_preproc_pc_comp_field ci_amr_fr;
992 struct ipac_preproc_pc_comp_field ci_amr_hr;
993 struct ipac_preproc_pc_comp_field ci_sdcch;
994 struct ipac_preproc_pc_comp_field ci_gprs;
995}__attribute__ ((packed));
996
998 struct ipac_preproc_ho_comp {
999#if OSMO_IS_LITTLE_ENDIAN
1000 uint8_t p5:5,
1001 reserved_p5:3;
1002 uint8_t n5:5,
1003 reserved_n5:3;
1004 uint8_t p6:5,
1005 reserved_p6:3;
1006 uint8_t n6:5,
1007 reserved_n6:3;
1008 uint8_t p7:5,
1009 reserved_p7:3;
1010 uint8_t n7:5,
1011 reserved_n7:3;
1012 uint8_t p8:5,
1013 reserved_p8:3;
1014 uint8_t n8:5,
1015 reserved_n8:3;
1016 uint8_t ho_interval:5,
1017 reserved_ho:3;
1018 uint8_t reserved;
1019
1020#elif OSMO_IS_BIG_ENDIAN
1021/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
1022 uint8_t reserved_p5:3, p5:5;
1023 uint8_t reserved_n5:3, n5:5;
1024 uint8_t reserved_p6:3, p6:5;
1025 uint8_t reserved_n6:3, n6:5;
1026 uint8_t reserved_p7:3, p7:5;
1027 uint8_t reserved_n7:3, n7:5;
1028 uint8_t reserved_p8:3, p8:5;
1029 uint8_t reserved_n8:3, n8:5;
1030 uint8_t reserved_ho:3, ho_interval:5;
1031 uint8_t reserved;
1032#endif
1033}__attribute__ ((packed));
1034
1035 struct ipac_preproc_ho_candidates {
1036#if OSMO_IS_LITTLE_ENDIAN
1037 uint8_t bsic:6,
1038 reserved0:2;
1039 uint8_t bcch_freq:5,
1040 ba_used:1,
1041 s:1,
1042 reserved1:1;
1043#elif OSMO_IS_BIG_ENDIAN
1044/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
1045 uint8_t reserved0:2, bsic:6;
1046 uint8_t reserved1:1, s:1, ba_used:1, bcch_freq:5;
1047#endif
1048}__attribute__ ((packed));
1049
1050 struct ipac_preproc_ncell_dflts {
1051#if OSMO_IS_LITTLE_ENDIAN
1052 uint8_t rxlev_min_def:6,
1053 reserved_rxlev_min_def:2;
1054 uint8_t ho_margin_def:5,
1055 reserved_ho_margin_def:3;
1056 uint8_t ms_txpwr_max_def:5,
1057 reserved_ms_txpwr_max_def:3;
1058#elif OSMO_IS_BIG_ENDIAN
1059/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
1060 uint8_t reserved_rxlev_min_def:2, rxlev_min_def:6;
1061 uint8_t reserved_ho_margin_def:3, ho_margin_def:5;
1062 uint8_t reserved_ms_txpwr_max_def:3, ms_txpwr_max_def:5;
1063#endif
1064}__attribute__ ((packed));
1065
1066 struct ipac_preproc_ho_ctl_param {
1067#if OSMO_IS_LITTLE_ENDIAN
1068 uint8_t sdcch_ho_gsm:1,
1069 sdcch_ho_umts:1,
1070 reserved:6;
1071#elif OSMO_IS_BIG_ENDIAN
1072/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
1073 uint8_t reserved:6, sdcch_ho_umts:1, sdcch_ho_gsm:1;
1074#endif
1075}__attribute__ ((packed));
1076
1077 struct ipac_preproc_cfg {
1078 uint8_t meas_rep_mode;
1079 uint32_t meas_mode_flags;
1080 struct ipac_preproc_ave_cfg ms_ave_cfg[3];
1081 struct ipac_preproc_ave_cfg ave_cfg;
1082 struct ipac_preproc_ho_thresh ho_thresh;
1083 struct ipac_preproc_ho_comp ho_comp;
1084 struct ipac_preproc_ncell_dflts ncell_dflts;
1085 struct ipac_preproc_ho_ctl_param ho_ctl_param;
1086};
1087
1088 struct rsl_l1_info {
1089#if OSMO_IS_LITTLE_ENDIAN
1090 uint8_t reserved:1,
1091 srr_sro:1,
1092 fpc_epc:1,
1093 ms_pwr:5;
1094 uint8_t ta;
1095#elif OSMO_IS_BIG_ENDIAN
1096/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
1097 uint8_t ms_pwr:5, fpc_epc:1, srr_sro:1, reserved:1;
1098 uint8_t ta;
1099#endif
1100} __attribute__ ((packed));
1101
endian.h
rsl_ipac_rtp_csd_format_d
rsl_ipac_rtp_csd_format_d
Definition: gsm_08_58.h:769
rsl_mrpci_pwrclass
rsl_mrpci_pwrclass
Definition: gsm_08_58.h:791
rsl_rel_mode
rsl_rel_mode
Definition: gsm_08_58.h:806
abis_rsl_ie
abis_rsl_ie
RSL Information Element Identifiers (Chapter 9.3)
Definition: gsm_08_58.h:300
abis_rsl_msgtype_ericsson
abis_rsl_msgtype_ericsson
Ericsson vendor-specific RSL message types.
Definition: gsm_08_58.h:295
rsl_ipac_rtp_payload
rsl_ipac_rtp_payload
Definition: gsm_08_58.h:744
rsl_ipac_embedded_ie
rsl_ipac_embedded_ie
ip.access specific embedded information elements
Definition: gsm_08_58.h:812
rsl_ipac_speech_mode_m
rsl_ipac_speech_mode_m
Definition: gsm_08_58.h:762
rsl_ipac_rtp_csd_format_ir
rsl_ipac_rtp_csd_format_ir
Definition: gsm_08_58.h:776
rsl_cmod_spd
rsl_cmod_spd
Definition: gsm_08_58.h:500
rsl_mrpci_phase
rsl_mrpci_phase
Definition: gsm_08_58.h:798
rsl_cmod_sp
rsl_cmod_sp
Speech.
Definition: gsm_08_58.h:520
abis_rsl_msgtype_siemens
abis_rsl_msgtype_siemens
Siemens vendor-specific RSL message types.
Definition: gsm_08_58.h:275
abis_rsl_msgtype
abis_rsl_msgtype
Definition: gsm_08_58.h:170
rsl_ipac_speech_mode_s
rsl_ipac_speech_mode_s
Definition: gsm_08_58.h:753
__attribute__
enum abis_rsl_msgtype __attribute__
rsl_cmod_crt
rsl_cmod_crt
Channel rate and type.
Definition: gsm_08_58.h:506
rsl_cmod_csd_t
rsl_cmod_csd_t
Transparent data.
Definition: gsm_08_58.h:554
rsl_cmod_csd_nt
rsl_cmod_csd_nt
Non-transparent data.
Definition: gsm_08_58.h:529
RSL_IPAC_RTP_CSD_NON_TRAU
@ RSL_IPAC_RTP_CSD_NON_TRAU
packed 16k (252/288 bit) / 8k (126 bit) in RTP
Definition: gsm_08_58.h:771
RSL_IPAC_RTP_CSD_IWF_FREE
@ RSL_IPAC_RTP_CSD_IWF_FREE
unknown proprietary IWF-free BTS-BTS data
Definition: gsm_08_58.h:773
RSL_IPAC_RTP_CSD_EXT_TRAU
@ RSL_IPAC_RTP_CSD_EXT_TRAU
TRAU-like RTP format, without leading zero-bits.
Definition: gsm_08_58.h:770
RSL_IPAC_RTP_CSD_TRAU_BTS
@ RSL_IPAC_RTP_CSD_TRAU_BTS
TRAU in BTS; V.110 in RTP/CLEARMODE.
Definition: gsm_08_58.h:772
RSL_MRPCI_PWRC_2
@ RSL_MRPCI_PWRC_2
Definition: gsm_08_58.h:793
RSL_MRPCI_PWRC_4
@ RSL_MRPCI_PWRC_4
Definition: gsm_08_58.h:795
RSL_MRPCI_PWRC_1
@ RSL_MRPCI_PWRC_1
Definition: gsm_08_58.h:792
RSL_MRPCI_PWRC_3
@ RSL_MRPCI_PWRC_3
Definition: gsm_08_58.h:794
RSL_MRPCI_PWRC_5
@ RSL_MRPCI_PWRC_5
Definition: gsm_08_58.h:796
RSL_REL_LOCAL_END
@ RSL_REL_LOCAL_END
Definition: gsm_08_58.h:808
RSL_REL_NORMAL
@ RSL_REL_NORMAL
Definition: gsm_08_58.h:807
RSL_IE_SACCH_INFO
@ RSL_IE_SACCH_INFO
Definition: gsm_08_58.h:344
RSL_IE_RACH_LOAD
@ RSL_IE_RACH_LOAD
Definition: gsm_08_58.h:318
RSL_IE_CAUSE
@ RSL_IE_CAUSE
Definition: gsm_08_58.h:326
RSL_IE_OSMO_RTP_EXTENSIONS
@ RSL_IE_OSMO_RTP_EXTENSIONS
Definition: gsm_08_58.h:377
RSL_IE_FULL_BCCH_INFO
@ RSL_IE_FULL_BCCH_INFO
Definition: gsm_08_58.h:339
RSL_IE_CBCH_LOAD_INFO
@ RSL_IE_CBCH_LOAD_INFO
Definition: gsm_08_58.h:345
RSL_IE_FRAME_NUMBER
@ RSL_IE_FRAME_NUMBER
Definition: gsm_08_58.h:308
RSL_IE_IPAC_RTP_MPLEX
@ RSL_IE_IPAC_RTP_MPLEX
Definition: gsm_08_58.h:396
RSL_IE_ERR_MSG
@ RSL_IE_ERR_MSG
Definition: gsm_08_58.h:338
RSL_IE_SMSCB_INFO
@ RSL_IE_SMSCB_INFO
Definition: gsm_08_58.h:336
RSL_IE_CHAN_DESC
@ RSL_IE_CHAN_DESC
Definition: gsm_08_58.h:348
RSL_IE_OSMO_REP_ACCH_CAP
@ RSL_IE_OSMO_REP_ACCH_CAP
Definition: gsm_08_58.h:373
RSL_IE_PREPROC_MEAS
@ RSL_IE_PREPROC_MEAS
Definition: gsm_08_58.h:334
RSL_IE_SIEMENS_ININ_CELL_HO_PAR
@ RSL_IE_SIEMENS_ININ_CELL_HO_PAR
Definition: gsm_08_58.h:365
RSL_IE_OSMO_OSMUX_CID
@ RSL_IE_OSMO_OSMUX_CID
Definition: gsm_08_58.h:376
RSL_IE_RTD
@ RSL_IE_RTD
Definition: gsm_08_58.h:358
RSL_IE_CMD_INDICATOR
@ RSL_IE_CMD_INDICATOR
Definition: gsm_08_58.h:350
RSL_IE_MAIN_CHAN_REF
@ RSL_IE_MAIN_CHAN_REF
Definition: gsm_08_58.h:353
RSL_IE_IMM_ASS_INFO
@ RSL_IE_IMM_ASS_INFO
Definition: gsm_08_58.h:335
RSL_IE_SIEMENS_TRACE_REF_NR
@ RSL_IE_SIEMENS_TRACE_REF_NR
Definition: gsm_08_58.h:366
RSL_IE_L1_INFO
@ RSL_IE_L1_INFO
Definition: gsm_08_58.h:310
RSL_IE_MS_POWER
@ RSL_IE_MS_POWER
Definition: gsm_08_58.h:313
RSL_IE_IPAC_LOCAL_PORT
@ RSL_IE_IPAC_LOCAL_PORT
Definition: gsm_08_58.h:386
RSL_IE_LINK_IDENT
@ RSL_IE_LINK_IDENT
Definition: gsm_08_58.h:302
RSL_IE_MR_CONTROL
@ RSL_IE_MR_CONTROL
Definition: gsm_08_58.h:355
RSL_IE_ACCESS_DELAY
@ RSL_IE_ACCESS_DELAY
Definition: gsm_08_58.h:317
RSL_IE_IPAC_RTP_JIT_BUF
@ RSL_IE_IPAC_RTP_JIT_BUF
Definition: gsm_08_58.h:393
RSL_IE_SYSINFO_TYPE
@ RSL_IE_SYSINFO_TYPE
Definition: gsm_08_58.h:330
RSL_IE_MR_CONFIG
@ RSL_IE_MR_CONFIG
Definition: gsm_08_58.h:354
RSL_IE_IPAC_RTP_PAYLOAD2
@ RSL_IE_IPAC_RTP_PAYLOAD2
Definition: gsm_08_58.h:395
RSL_IE_RESOURCE_INFO
@ RSL_IE_RESOURCE_INFO
Definition: gsm_08_58.h:321
RSL_IE_SIEMENS_HIGHEST_RATE
@ RSL_IE_SIEMENS_HIGHEST_RATE
Definition: gsm_08_58.h:369
RSL_IE_NCH_DRX_INFO
@ RSL_IE_NCH_DRX_INFO
Definition: gsm_08_58.h:349
RSL_IE_IPAC_LOCAL_IP
@ RSL_IE_IPAC_LOCAL_IP
Definition: gsm_08_58.h:388
RSL_IE_IPAC_CONN_STAT
@ RSL_IE_IPAC_CONN_STAT
Definition: gsm_08_58.h:389
RSL_IE_OSMO_TEMP_OVP_ACCH_CAP
@ RSL_IE_OSMO_TEMP_OVP_ACCH_CAP
Definition: gsm_08_58.h:375
RSL_IE_SIEMENS_INT_TRACE_IDX
@ RSL_IE_SIEMENS_INT_TRACE_IDX
Definition: gsm_08_58.h:367
RSL_IE_EMLPP_PRIO
@ RSL_IE_EMLPP_PRIO
Definition: gsm_08_58.h:351
RSL_IE_ENCR_INFO
@ RSL_IE_ENCR_INFO
Definition: gsm_08_58.h:307
RSL_IE_SIEMENS_L2_HDR_INFO
@ RSL_IE_SIEMENS_L2_HDR_INFO
Definition: gsm_08_58.h:368
RSL_IE_IPAC_RTP_MPLEX_ID
@ RSL_IE_IPAC_RTP_MPLEX_ID
Definition: gsm_08_58.h:397
RSL_IE_FULL_IMM_ASS_INFO
@ RSL_IE_FULL_IMM_ASS_INFO
Definition: gsm_08_58.h:343
RSL_IE_OSMO_TRAINING_SEQUENCE
@ RSL_IE_OSMO_TRAINING_SEQUENCE
Definition: gsm_08_58.h:374
RSL_IE_CB_CMD_TYPE
@ RSL_IE_CB_CMD_TYPE
Definition: gsm_08_58.h:341
RSL_IE_UPLINK_MEAS
@ RSL_IE_UPLINK_MEAS
Definition: gsm_08_58.h:325
RSL_IE_SIEMENS_PREF_AREA_TYPE
@ RSL_IE_SIEMENS_PREF_AREA_TYPE
Definition: gsm_08_58.h:364
RSL_IE_SIEMENS_MRPCI
@ RSL_IE_SIEMENS_MRPCI
Definition: gsm_08_58.h:363
RSL_IE_UIC
@ RSL_IE_UIC
Definition: gsm_08_58.h:352
RSL_IE_IPAC_RTP_COMPR
@ RSL_IE_IPAC_RTP_COMPR
Definition: gsm_08_58.h:394
RSL_IE_HANDO_REF
@ RSL_IE_HANDO_REF
Definition: gsm_08_58.h:309
RSL_IE_LLP_APDU
@ RSL_IE_LLP_APDU
Definition: gsm_08_58.h:360
RSL_IE_IPAC_HO_C_PARMS
@ RSL_IE_IPAC_HO_C_PARMS
Definition: gsm_08_58.h:390
RSL_IE_SMSCB_MSG
@ RSL_IE_SMSCB_MSG
Definition: gsm_08_58.h:342
RSL_IE_MS_IDENTITY
@ RSL_IE_MS_IDENTITY
Definition: gsm_08_58.h:312
RSL_IE_MS_POWER_PARAM
@ RSL_IE_MS_POWER_PARAM
Definition: gsm_08_58.h:331
RSL_IE_RLM_CAUSE
@ RSL_IE_RLM_CAUSE
Definition: gsm_08_58.h:322
RSL_IE_REQ_REFERENCE
@ RSL_IE_REQ_REFERENCE
Definition: gsm_08_58.h:319
RSL_IE_IPAC_BSCMPL_TOUT
@ RSL_IE_IPAC_BSCMPL_TOUT
Definition: gsm_08_58.h:382
RSL_IE_STARTNG_TIME
@ RSL_IE_STARTNG_TIME
Definition: gsm_08_58.h:323
RSL_IE_RELEASE_MODE
@ RSL_IE_RELEASE_MODE
Definition: gsm_08_58.h:320
RSL_IE_MSG_ID
@ RSL_IE_MSG_ID
Definition: gsm_08_58.h:328
RSL_IE_SUP_CODEC_TYPES
@ RSL_IE_SUP_CODEC_TYPES
Definition: gsm_08_58.h:356
RSL_IE_PREPROC_PARAM
@ RSL_IE_PREPROC_PARAM
Definition: gsm_08_58.h:333
RSL_IE_CHAN_MODE
@ RSL_IE_CHAN_MODE
Definition: gsm_08_58.h:306
RSL_IE_IPAC_RTP_PAYLOAD
@ RSL_IE_IPAC_RTP_PAYLOAD
Definition: gsm_08_58.h:385
RSL_IE_TFO_STATUS
@ RSL_IE_TFO_STATUS
Definition: gsm_08_58.h:359
RSL_IE_SIEMENS_SUGGESTED_RATE
@ RSL_IE_SIEMENS_SUGGESTED_RATE
Definition: gsm_08_58.h:370
RSL_IE_CODEC_CONFIG
@ RSL_IE_CODEC_CONFIG
Definition: gsm_08_58.h:357
RSL_IE_PYHS_CONTEXT
@ RSL_IE_PYHS_CONTEXT
Definition: gsm_08_58.h:316
RSL_IE_IPAC_SPEECH_MODE
@ RSL_IE_IPAC_SPEECH_MODE
Definition: gsm_08_58.h:387
RSL_IE_IPAC_CONN_ID
@ RSL_IE_IPAC_CONN_ID
Definition: gsm_08_58.h:391
RSL_IE_SMSCB_CHAN_INDICATOR
@ RSL_IE_SMSCB_CHAN_INDICATOR
Definition: gsm_08_58.h:346
RSL_IE_IPAC_PROXY_UDP
@ RSL_IE_IPAC_PROXY_UDP
Definition: gsm_08_58.h:381
RSL_IE_MEAS_RES_NR
@ RSL_IE_MEAS_RES_NR
Definition: gsm_08_58.h:327
RSL_IE_IPAC_REMOTE_IP
@ RSL_IE_IPAC_REMOTE_IP
Definition: gsm_08_58.h:383
RSL_IE_CHAN_IDENT
@ RSL_IE_CHAN_IDENT
Definition: gsm_08_58.h:305
RSL_IE_IPAC_RTP_CSD_FMT
@ RSL_IE_IPAC_RTP_CSD_FMT
Definition: gsm_08_58.h:392
RSL_IE_PAGING_LOAD
@ RSL_IE_PAGING_LOAD
Definition: gsm_08_58.h:315
RSL_IE_CHAN_NR
@ RSL_IE_CHAN_NR
Definition: gsm_08_58.h:301
RSL_IE_GROUP_CALL_REF
@ RSL_IE_GROUP_CALL_REF
Definition: gsm_08_58.h:347
RSL_IE_MS_TIMING_OFFSET
@ RSL_IE_MS_TIMING_OFFSET
Definition: gsm_08_58.h:337
RSL_IE_TIMING_ADVANCE
@ RSL_IE_TIMING_ADVANCE
Definition: gsm_08_58.h:324
RSL_IE_CHAN_NEEDED
@ RSL_IE_CHAN_NEEDED
Definition: gsm_08_58.h:340
RSL_IE_IPAC_REMOTE_PORT
@ RSL_IE_IPAC_REMOTE_PORT
Definition: gsm_08_58.h:384
RSL_IE_TFO_XPAR_CONT
@ RSL_IE_TFO_XPAR_CONT
Definition: gsm_08_58.h:361
RSL_IE_L3_INFO
@ RSL_IE_L3_INFO
Definition: gsm_08_58.h:311
RSL_IE_ACT_TYPE
@ RSL_IE_ACT_TYPE
Definition: gsm_08_58.h:303
RSL_IE_PAGING_GROUP
@ RSL_IE_PAGING_GROUP
Definition: gsm_08_58.h:314
RSL_IE_IPAC_SRTP_CONFIG
@ RSL_IE_IPAC_SRTP_CONFIG
Definition: gsm_08_58.h:380
RSL_IE_BS_POWER
@ RSL_IE_BS_POWER
Definition: gsm_08_58.h:304
RSL_IE_BS_POWER_PARAM
@ RSL_IE_BS_POWER_PARAM
Definition: gsm_08_58.h:332
RSL_MT_ERICSSON_IMM_ASS_SENT
@ RSL_MT_ERICSSON_IMM_ASS_SENT
Definition: gsm_08_58.h:296
RSL_IPAC_RTP_EFR
@ RSL_IPAC_RTP_EFR
Definition: gsm_08_58.h:746
RSL_IPAC_RTP_AMR
@ RSL_IPAC_RTP_AMR
Definition: gsm_08_58.h:747
RSL_IPAC_RTP_GSM
@ RSL_IPAC_RTP_GSM
Definition: gsm_08_58.h:745
RSL_IPAC_RTP_MUX
@ RSL_IPAC_RTP_MUX
Definition: gsm_08_58.h:749
RSL_IPAC_RTP_CSD
@ RSL_IPAC_RTP_CSD
Definition: gsm_08_58.h:748
IPAC_RXQUAL_AVE
@ IPAC_RXQUAL_AVE
Definition: gsm_08_58.h:435
IPAC_RXLEV_AVE
@ IPAC_RXLEV_AVE
Definition: gsm_08_58.h:434
IPAC_MS_BTS_DIS_AVE
@ IPAC_MS_BTS_DIS_AVE
Definition: gsm_08_58.h:436
RSL_IPAC_EIE_MASTER_KEY
@ RSL_IPAC_EIE_MASTER_KEY
Definition: gsm_08_58.h:832
RSL_IPAC_EIE_MEAS_AVG_CFG
@ RSL_IPAC_EIE_MEAS_AVG_CFG
Definition: gsm_08_58.h:817
RSL_IPAC_EIE_MASTER_SALT
@ RSL_IPAC_EIE_MASTER_SALT
Definition: gsm_08_58.h:833
RSL_IPAC_EIE_NCELL_DEFAULTS
@ RSL_IPAC_EIE_NCELL_DEFAULTS
Definition: gsm_08_58.h:821
RSL_IPAC_EIE_NUM_OF_MS
@ RSL_IPAC_EIE_NUM_OF_MS
Definition: gsm_08_58.h:828
RSL_IPAC_EIE_PC_THRESH_COMP
@ RSL_IPAC_EIE_PC_THRESH_COMP
Definition: gsm_08_58.h:823
RSL_IPAC_EIE_3G_HO_PARAM
@ RSL_IPAC_EIE_3G_HO_PARAM
Definition: gsm_08_58.h:836
RSL_IPAC_EIE_NCELL_BA_CHG_LIST
@ RSL_IPAC_EIE_NCELL_BA_CHG_LIST
Definition: gsm_08_58.h:827
RSL_IPAC_EIE_FREQ_ERR
@ RSL_IPAC_EIE_FREQ_ERR
Definition: gsm_08_58.h:815
RSL_IPAC_EIE_HO_THRESH_COMP
@ RSL_IPAC_EIE_HO_THRESH_COMP
Definition: gsm_08_58.h:824
RSL_IPAC_EIE_HO_CAND_EXT
@ RSL_IPAC_EIE_HO_CAND_EXT
Definition: gsm_08_58.h:829
RSL_IPAC_EIE_MS_PWR_CTL
@ RSL_IPAC_EIE_MS_PWR_CTL
Definition: gsm_08_58.h:819
RSL_IPAC_EIE_3G_NCELL_LIST
@ RSL_IPAC_EIE_3G_NCELL_LIST
Definition: gsm_08_58.h:837
RSL_IPAC_EIE_HO_CANDIDATES
@ RSL_IPAC_EIE_HO_CANDIDATES
Definition: gsm_08_58.h:826
RSL_IPAC_EIE_AMR_CONV_THRESH
@ RSL_IPAC_EIE_AMR_CONV_THRESH
Definition: gsm_08_58.h:839
RSL_IPAC_EIE_NCELL_LIST_EXT
@ RSL_IPAC_EIE_NCELL_LIST_EXT
Definition: gsm_08_58.h:831
RSL_IPAC_EIE_NCELL_LIST
@ RSL_IPAC_EIE_NCELL_LIST
Definition: gsm_08_58.h:822
RSL_IPAC_EIE_SDCCH_CTL_PARAM
@ RSL_IPAC_EIE_SDCCH_CTL_PARAM
Definition: gsm_08_58.h:838
RSL_IPAC_EIE_NCELL_DEF_EXT
@ RSL_IPAC_EIE_NCELL_DEF_EXT
Definition: gsm_08_58.h:830
RSL_IPAC_EIE_OSMO_PC_THRESH_COMP
@ RSL_IPAC_EIE_OSMO_PC_THRESH_COMP
Definition: gsm_08_58.h:844
RSL_IPAC_EIE_HANDO_THRESH
@ RSL_IPAC_EIE_HANDO_THRESH
Definition: gsm_08_58.h:820
RSL_IPAC_EIE_MEAS_TRANS_RES
@ RSL_IPAC_EIE_MEAS_TRANS_RES
Definition: gsm_08_58.h:835
RSL_IPAC_EIE_TIMING_ERR
@ RSL_IPAC_EIE_TIMING_ERR
Definition: gsm_08_58.h:816
RSL_IPAC_EIE_RXLEV
@ RSL_IPAC_EIE_RXLEV
Definition: gsm_08_58.h:813
RSL_IPAC_EIE_OSMO_MS_PWR_CTL
@ RSL_IPAC_EIE_OSMO_MS_PWR_CTL
Definition: gsm_08_58.h:843
RSL_IPAC_EIE_OSMO_MEAS_AVG_CFG
@ RSL_IPAC_EIE_OSMO_MEAS_AVG_CFG
Definition: gsm_08_58.h:842
RSL_IPAC_EIE_RXQUAL
@ RSL_IPAC_EIE_RXQUAL
Definition: gsm_08_58.h:814
RSL_IPAC_EIE_BS_PWR_CTL
@ RSL_IPAC_EIE_BS_PWR_CTL
Definition: gsm_08_58.h:818
RSL_IPAC_EIE_HO_CAUSE
@ RSL_IPAC_EIE_HO_CAUSE
Definition: gsm_08_58.h:825
RSL_IPAC_SPEECH_M_TX
@ RSL_IPAC_SPEECH_M_TX
Definition: gsm_08_58.h:765
RSL_IPAC_SPEECH_M_RX
@ RSL_IPAC_SPEECH_M_RX
Definition: gsm_08_58.h:764
RSL_IPAC_SPEECH_M_RXTX
@ RSL_IPAC_SPEECH_M_RXTX
Definition: gsm_08_58.h:763
RSL_IPAC_RTP_CSD_IR_32k
@ RSL_IPAC_RTP_CSD_IR_32k
Definition: gsm_08_58.h:779
RSL_IPAC_RTP_CSD_IR_64k
@ RSL_IPAC_RTP_CSD_IR_64k
Definition: gsm_08_58.h:780
RSL_IPAC_RTP_CSD_IR_8k
@ RSL_IPAC_RTP_CSD_IR_8k
Definition: gsm_08_58.h:777
RSL_IPAC_RTP_CSD_IR_16k
@ RSL_IPAC_RTP_CSD_IR_16k
Definition: gsm_08_58.h:778
RSL_CMOD_SPD_SPEECH
@ RSL_CMOD_SPD_SPEECH
Definition: gsm_08_58.h:501
RSL_CMOD_SPD_SIGN
@ RSL_CMOD_SPD_SIGN
Definition: gsm_08_58.h:503
RSL_CMOD_SPD_DATA
@ RSL_CMOD_SPD_DATA
Definition: gsm_08_58.h:502
IPAC_MEDIAN_AVE
@ IPAC_MEDIAN_AVE
Definition: gsm_08_58.h:427
IPAC_WEIGHTED_AVE
@ IPAC_WEIGHTED_AVE
Definition: gsm_08_58.h:426
IPAC_OSMO_EWMA_AVE
@ IPAC_OSMO_EWMA_AVE
Definition: gsm_08_58.h:429
IPAC_UNWEIGHTED_AVE
@ IPAC_UNWEIGHTED_AVE
Definition: gsm_08_58.h:425
RSL_MRPCI_PHASE_2
@ RSL_MRPCI_PHASE_2
Definition: gsm_08_58.h:801
RSL_MRPCI_PHASE_1
@ RSL_MRPCI_PHASE_1
Definition: gsm_08_58.h:799
RSL_MRPCI_PHASE_2PLUS
@ RSL_MRPCI_PHASE_2PLUS
Definition: gsm_08_58.h:802
RSL_CMOD_SP_GSM2
@ RSL_CMOD_SP_GSM2
Definition: gsm_08_58.h:522
RSL_CMOD_SP_GSM6
@ RSL_CMOD_SP_GSM6
Definition: gsm_08_58.h:526
RSL_CMOD_SP_GSM1
@ RSL_CMOD_SP_GSM1
Definition: gsm_08_58.h:521
RSL_CMOD_SP_GSM3
@ RSL_CMOD_SP_GSM3
Definition: gsm_08_58.h:523
RSL_CMOD_SP_GSM5
@ RSL_CMOD_SP_GSM5
Definition: gsm_08_58.h:525
RSL_CMOD_SP_GSM4
@ RSL_CMOD_SP_GSM4
Definition: gsm_08_58.h:524
IPAC_HO_RQD_CAUSE_ENQUIRY
@ IPAC_HO_RQD_CAUSE_ENQUIRY
Definition: gsm_08_58.h:449
IPAC_HO_RQD_CAUSE_NORMAL3G
@ IPAC_HO_RQD_CAUSE_NORMAL3G
Definition: gsm_08_58.h:451
IPAC_HO_RQD_CAUSE_RXLEV_UL_IH
@ IPAC_HO_RQD_CAUSE_RXLEV_UL_IH
Definition: gsm_08_58.h:445
IPAC_HO_RQD_CAUSE_L_RXQUAL_DL_H
@ IPAC_HO_RQD_CAUSE_L_RXQUAL_DL_H
Definition: gsm_08_58.h:444
IPAC_HO_RQD_CAUSE_EMERGENCY3G
@ IPAC_HO_RQD_CAUSE_EMERGENCY3G
Definition: gsm_08_58.h:452
IPAC_HO_RQD_CAUSE_LOAD_DEMOTION
@ IPAC_HO_RQD_CAUSE_LOAD_DEMOTION
Definition: gsm_08_58.h:457
IPAC_HO_RQD_CAUSE_QUALITY_PROMOTION
@ IPAC_HO_RQD_CAUSE_QUALITY_PROMOTION
Definition: gsm_08_58.h:455
IPAC_HO_RQD_CAUSE_L_RXLEV_UL_H
@ IPAC_HO_RQD_CAUSE_L_RXLEV_UL_H
Definition: gsm_08_58.h:441
IPAC_HO_RQD_CAUSE_L_RXQUAL_UL_H
@ IPAC_HO_RQD_CAUSE_L_RXQUAL_UL_H
Definition: gsm_08_58.h:443
IPAC_HO_RQD_CAUSE_ENQUIRY_FAILED
@ IPAC_HO_RQD_CAUSE_ENQUIRY_FAILED
Definition: gsm_08_58.h:450
IPAC_HO_RQD_CAUSE_MAX
@ IPAC_HO_RQD_CAUSE_MAX
Definition: gsm_08_58.h:458
IPAC_HO_RQD_CAUSE_L_RXLEV_DL_H
@ IPAC_HO_RQD_CAUSE_L_RXLEV_DL_H
Definition: gsm_08_58.h:442
IPAC_HO_RQD_CAUSE_POWER_BUDGET
@ IPAC_HO_RQD_CAUSE_POWER_BUDGET
Definition: gsm_08_58.h:448
IPAC_HO_RQD_CAUSE_SERVICE_PREFERRED3G
@ IPAC_HO_RQD_CAUSE_SERVICE_PREFERRED3G
Definition: gsm_08_58.h:453
IPAC_HO_RQD_CAUSE_O_M_SHUTDOWN
@ IPAC_HO_RQD_CAUSE_O_M_SHUTDOWN
Definition: gsm_08_58.h:454
IPAC_HO_RQD_CAUSE_LOAD_PROMOTION
@ IPAC_HO_RQD_CAUSE_LOAD_PROMOTION
Definition: gsm_08_58.h:456
IPAC_HO_RQD_CAUSE_RXLEV_DL_IH
@ IPAC_HO_RQD_CAUSE_RXLEV_DL_IH
Definition: gsm_08_58.h:446
IPAC_HO_RQD_CAUSE_MAX_MS_RANGE
@ IPAC_HO_RQD_CAUSE_MAX_MS_RANGE
Definition: gsm_08_58.h:447
RSL_MT_SIEMENS_HO_FAIL_IND
@ RSL_MT_SIEMENS_HO_FAIL_IND
Definition: gsm_08_58.h:286
RSL_MT_SIEMENS_STOP_TRACE_ACK
@ RSL_MT_SIEMENS_STOP_TRACE_ACK
Definition: gsm_08_58.h:287
RSL_MT_SIEMENS_FORCED_HO_REQ
@ RSL_MT_SIEMENS_FORCED_HO_REQ
Definition: gsm_08_58.h:279
RSL_MT_SIEMENS_START_TRACE
@ RSL_MT_SIEMENS_START_TRACE
Definition: gsm_08_58.h:282
RSL_MT_SIEMENS_SET_SYS_INFO_10
@ RSL_MT_SIEMENS_SET_SYS_INFO_10
Definition: gsm_08_58.h:290
RSL_MT_SIEMENS_MODIF_COND_IND
@ RSL_MT_SIEMENS_MODIF_COND_IND
Definition: gsm_08_58.h:291
RSL_MT_SIEMENS_STOP_TRACE
@ RSL_MT_SIEMENS_STOP_TRACE
Definition: gsm_08_58.h:284
RSL_MT_SIEMENS_MRPCI
@ RSL_MT_SIEMENS_MRPCI
Definition: gsm_08_58.h:276
RSL_MT_SIEMENS_TRMR
@ RSL_MT_SIEMENS_TRMR
Definition: gsm_08_58.h:285
RSL_MT_SIEMENS_START_TRACE_ACK
@ RSL_MT_SIEMENS_START_TRACE_ACK
Definition: gsm_08_58.h:283
RSL_MT_SIEMENS_UPLF
@ RSL_MT_SIEMENS_UPLF
Definition: gsm_08_58.h:288
RSL_MT_SIEMENS_INTERC_HO_COND_IND
@ RSL_MT_SIEMENS_INTERC_HO_COND_IND
Definition: gsm_08_58.h:278
RSL_MT_SIEMENS_PREF_AREA
@ RSL_MT_SIEMENS_PREF_AREA
Definition: gsm_08_58.h:281
RSL_MT_SIEMENS_PREF_AREA_REQ
@ RSL_MT_SIEMENS_PREF_AREA_REQ
Definition: gsm_08_58.h:280
RSL_MT_SIEMENS_INTRAC_HO_COND_IND
@ RSL_MT_SIEMENS_INTRAC_HO_COND_IND
Definition: gsm_08_58.h:277
RSL_MT_SIEMENS_UPLB
@ RSL_MT_SIEMENS_UPLB
Definition: gsm_08_58.h:289
RSL_MT_MS_POWER_CONTROL
@ RSL_MT_MS_POWER_CONTROL
Definition: gsm_08_58.h:221
RSL_MT_IMMEDIATE_ASSIGN_CMD
@ RSL_MT_IMMEDIATE_ASSIGN_CMD
Definition: gsm_08_58.h:194
RSL_MT_MR_CODEC_MOD_NACK
@ RSL_MT_MR_CODEC_MOD_NACK
Definition: gsm_08_58.h:234
RSL_MT_IPAC_CONNECT_MUX_ACK
@ RSL_MT_IPAC_CONNECT_MUX_ACK
Definition: gsm_08_58.h:249
RSL_MT_IPAC_DISC_MUX
@ RSL_MT_IPAC_DISC_MUX
Definition: gsm_08_58.h:254
RSL_MT_REL_IND
@ RSL_MT_REL_IND
Definition: gsm_08_58.h:180
RSL_MT_EST_IND
@ RSL_MT_EST_IND
Definition: gsm_08_58.h:177
RSL_MT_IPAC_CRCX_ACK
@ RSL_MT_IPAC_CRCX_ACK
Definition: gsm_08_58.h:261
RSL_MT_MODE_MODIFY_NACK
@ RSL_MT_MODE_MODIFY_NACK
Definition: gsm_08_58.h:217
RSL_MT_IPAC_BIND_MUX
@ RSL_MT_IPAC_BIND_MUX
Definition: gsm_08_58.h:251
RSL_MT_NOT_CMD
@ RSL_MT_NOT_CMD
Definition: gsm_08_58.h:204
RSL_MT_MODE_MODIFY_REQ
@ RSL_MT_MODE_MODIFY_REQ
Definition: gsm_08_58.h:215
RSL_MT_IPAC_CRCX_NACK
@ RSL_MT_IPAC_CRCX_NACK
Definition: gsm_08_58.h:262
RSL_MT_BS_POWER_CONTROL
@ RSL_MT_BS_POWER_CONTROL
Definition: gsm_08_58.h:222
RSL_MT_LOCATION_INFO
@ RSL_MT_LOCATION_INFO
Definition: gsm_08_58.h:238
RSL_MT_MEAS_RES
@ RSL_MT_MEAS_RES
Definition: gsm_08_58.h:214
RSL_MT_IPAC_HO_CAN_RES
@ RSL_MT_IPAC_HO_CAN_RES
Definition: gsm_08_58.h:259
RSL_MT_EST_REQ
@ RSL_MT_EST_REQ
Definition: gsm_08_58.h:175
RSL_MT_UNIT_DATA_IND
@ RSL_MT_UNIT_DATA_IND
Definition: gsm_08_58.h:182
RSL_MT_ENCR_CMD
@ RSL_MT_ENCR_CMD
Definition: gsm_08_58.h:212
RSL_MT_IPAC_PDCH_DEACT
@ RSL_MT_IPAC_PDCH_DEACT
Definition: gsm_08_58.h:245
RSL_MT_DATA_REQ
@ RSL_MT_DATA_REQ
Definition: gsm_08_58.h:172
RSL_MT_DATA_IND
@ RSL_MT_DATA_IND
Definition: gsm_08_58.h:173
RSL_MT_RF_RES_IND
@ RSL_MT_RF_RES_IND
Definition: gsm_08_58.h:198
RSL_MT_BCCH_INFO
@ RSL_MT_BCCH_INFO
Definition: gsm_08_58.h:189
RSL_MT_IPAC_DIR_RETR_ENQ
@ RSL_MT_IPAC_DIR_RETR_ENQ
Definition: gsm_08_58.h:241
RSL_MT_UNIT_DATA_REQ
@ RSL_MT_UNIT_DATA_REQ
Definition: gsm_08_58.h:181
RSL_MT_RTD_REP
@ RSL_MT_RTD_REP
Definition: gsm_08_58.h:230
RSL_MT_OVERLOAD
@ RSL_MT_OVERLOAD
Definition: gsm_08_58.h:200
RSL_MT_RF_CHAN_REL_ACK
@ RSL_MT_RF_CHAN_REL_ACK
Definition: gsm_08_58.h:225
RSL_MT_IPAC_PDCH_ACT_NACK
@ RSL_MT_IPAC_PDCH_ACT_NACK
Definition: gsm_08_58.h:244
RSL_MT_SUSP_REQ
@ RSL_MT_SUSP_REQ
Definition: gsm_08_58.h:183
RSL_MT_IPAC_PDCH_ACT
@ RSL_MT_IPAC_PDCH_ACT
Definition: gsm_08_58.h:242
RSL_MT_OSMO_ETWS_CMD
@ RSL_MT_OSMO_ETWS_CMD
Definition: gsm_08_58.h:271
RSL_MT_MR_CODEC_MOD_ACK
@ RSL_MT_MR_CODEC_MOD_ACK
Definition: gsm_08_58.h:233
RSL_MT_IPAC_DLCX_ACK
@ RSL_MT_IPAC_DLCX_ACK
Definition: gsm_08_58.h:268
RSL_MT_IPAC_PDCH_ACT_ACK
@ RSL_MT_IPAC_PDCH_ACT_ACK
Definition: gsm_08_58.h:243
RSL_MT_CHAN_RQD
@ RSL_MT_CHAN_RQD
Definition: gsm_08_58.h:191
RSL_MT_PHY_CONTEXT_REQ
@ RSL_MT_PHY_CONTEXT_REQ
Definition: gsm_08_58.h:218
RSL_MT_RF_CHAN_REL
@ RSL_MT_RF_CHAN_REL
Definition: gsm_08_58.h:220
RSL_MT_MR_CODEC_MOD_REQ
@ RSL_MT_MR_CODEC_MOD_REQ
Definition: gsm_08_58.h:232
RSL_MT_IPAC_MDCX_NACK
@ RSL_MT_IPAC_MDCX_NACK
Definition: gsm_08_58.h:265
RSL_MT_CHAN_ACTIV
@ RSL_MT_CHAN_ACTIV
Definition: gsm_08_58.h:207
RSL_MT_IPAC_DLCX_IND
@ RSL_MT_IPAC_DLCX_IND
Definition: gsm_08_58.h:266
RSL_MT_REMOTE_CODEC_CONF_REP
@ RSL_MT_REMOTE_CODEC_CONF_REP
Definition: gsm_08_58.h:229
RSL_MT_IPAC_DISC_MUX_ACK
@ RSL_MT_IPAC_DISC_MUX_ACK
Definition: gsm_08_58.h:255
RSL_MT_REL_REQ
@ RSL_MT_REL_REQ
Definition: gsm_08_58.h:178
RSL_MT_PRE_HANDO_NOTIF
@ RSL_MT_PRE_HANDO_NOTIF
Definition: gsm_08_58.h:231
RSL_MT_IPAC_DLCX_NACK
@ RSL_MT_IPAC_DLCX_NACK
Definition: gsm_08_58.h:269
RSL_MT_SMS_BC_REQ
@ RSL_MT_SMS_BC_REQ
Definition: gsm_08_58.h:195
RSL_MT_TFO_MOD_REQ
@ RSL_MT_TFO_MOD_REQ
Definition: gsm_08_58.h:237
RSL_MT_CHAN_ACTIV_ACK
@ RSL_MT_CHAN_ACTIV_ACK
Definition: gsm_08_58.h:208
RSL_MT_CHAN_ACTIV_NACK
@ RSL_MT_CHAN_ACTIV_NACK
Definition: gsm_08_58.h:209
RSL_MT_IPAC_MDCX
@ RSL_MT_IPAC_MDCX
Definition: gsm_08_58.h:263
RSL_MT_RES_REQ
@ RSL_MT_RES_REQ
Definition: gsm_08_58.h:185
RSL_MT_CONN_FAIL
@ RSL_MT_CONN_FAIL
Definition: gsm_08_58.h:210
RSL_MT_RECON_REQ
@ RSL_MT_RECON_REQ
Definition: gsm_08_58.h:186
RSL_MT_ERROR_REPORT
@ RSL_MT_ERROR_REPORT
Definition: gsm_08_58.h:201
RSL_MT_PHY_CONTEXT_CONF
@ RSL_MT_PHY_CONTEXT_CONF
Definition: gsm_08_58.h:219
RSL_MT_IPAC_DISC_MUX_NACK
@ RSL_MT_IPAC_DISC_MUX_NACK
Definition: gsm_08_58.h:256
RSL_MT_SMS_BC_CMD
@ RSL_MT_SMS_BC_CMD
Definition: gsm_08_58.h:202
RSL_MT_CCCH_LOAD_IND
@ RSL_MT_CCCH_LOAD_IND
Definition: gsm_08_58.h:190
RSL_MT_IPAC_CONNECT_MUX
@ RSL_MT_IPAC_CONNECT_MUX
Definition: gsm_08_58.h:248
RSL_MT_HANDO_DET
@ RSL_MT_HANDO_DET
Definition: gsm_08_58.h:213
RSL_MT_IPAC_MEAS_PREPROC_DFT
@ RSL_MT_IPAC_MEAS_PREPROC_DFT
Definition: gsm_08_58.h:257
RSL_MT_REL_CONF
@ RSL_MT_REL_CONF
Definition: gsm_08_58.h:179
RSL_MT_IPAC_CRCX
@ RSL_MT_IPAC_CRCX
Definition: gsm_08_58.h:260
RSL_MT_DEACTIVATE_SACCH
@ RSL_MT_DEACTIVATE_SACCH
Definition: gsm_08_58.h:211
RSL_MT_MODE_MODIFY_ACK
@ RSL_MT_MODE_MODIFY_ACK
Definition: gsm_08_58.h:216
RSL_MT_IPAC_BIND_MUX_NACK
@ RSL_MT_IPAC_BIND_MUX_NACK
Definition: gsm_08_58.h:253
RSL_MT_IPAC_MDCX_ACK
@ RSL_MT_IPAC_MDCX_ACK
Definition: gsm_08_58.h:264
RSL_MT_SACCH_FILL
@ RSL_MT_SACCH_FILL
Definition: gsm_08_58.h:199
RSL_MT_IPAC_CONNECT_MUX_NACK
@ RSL_MT_IPAC_CONNECT_MUX_NACK
Definition: gsm_08_58.h:250
RSL_MT_SACCH_INFO_MODIFY
@ RSL_MT_SACCH_INFO_MODIFY
Definition: gsm_08_58.h:226
RSL_MT_CBCH_LOAD_IND
@ RSL_MT_CBCH_LOAD_IND
Definition: gsm_08_58.h:203
RSL_MT_IPAC_HO_CAN_ENQ
@ RSL_MT_IPAC_HO_CAN_ENQ
Definition: gsm_08_58.h:258
RSL_MT_ERROR_IND
@ RSL_MT_ERROR_IND
Definition: gsm_08_58.h:174
RSL_MT_MR_CODEC_MOD_PER
@ RSL_MT_MR_CODEC_MOD_PER
Definition: gsm_08_58.h:235
RSL_MT_IPAC_BIND_MUX_ACK
@ RSL_MT_IPAC_BIND_MUX_ACK
Definition: gsm_08_58.h:252
RSL_MT_IPAC_PDCH_DEACT_ACK
@ RSL_MT_IPAC_PDCH_DEACT_ACK
Definition: gsm_08_58.h:246
RSL_MT_SUSP_CONF
@ RSL_MT_SUSP_CONF
Definition: gsm_08_58.h:184
RSL_MT_DELETE_IND
@ RSL_MT_DELETE_IND
Definition: gsm_08_58.h:192
RSL_MT_CHAN_CONF
@ RSL_MT_CHAN_CONF
Definition: gsm_08_58.h:196
RSL_MT_PREPROC_MEAS_RES
@ RSL_MT_PREPROC_MEAS_RES
Definition: gsm_08_58.h:224
RSL_MT_EST_CONF
@ RSL_MT_EST_CONF
Definition: gsm_08_58.h:176
RSL_MT_PAGING_CMD
@ RSL_MT_PAGING_CMD
Definition: gsm_08_58.h:193
RSL_MT_TFO_REP
@ RSL_MT_TFO_REP
Definition: gsm_08_58.h:236
RSL_MT_IPAC_PDCH_DEACT_NACK
@ RSL_MT_IPAC_PDCH_DEACT_NACK
Definition: gsm_08_58.h:247
RSL_MT_LISTENER_DET
@ RSL_MT_LISTENER_DET
Definition: gsm_08_58.h:228
RSL_MT_PREPROC_CONFIG
@ RSL_MT_PREPROC_CONFIG
Definition: gsm_08_58.h:223
RSL_MT_TALKER_DET
@ RSL_MT_TALKER_DET
Definition: gsm_08_58.h:227
RSL_MT_IPAC_DLCX
@ RSL_MT_IPAC_DLCX
Definition: gsm_08_58.h:267
RSL_IPAC_SPEECH_GSM_FR
@ RSL_IPAC_SPEECH_GSM_FR
Definition: gsm_08_58.h:754
RSL_IPAC_SPEECH_GSM_HR
@ RSL_IPAC_SPEECH_GSM_HR
Definition: gsm_08_58.h:757
RSL_IPAC_SPEECH_GSM_AMR_HR
@ RSL_IPAC_SPEECH_GSM_AMR_HR
Definition: gsm_08_58.h:758
RSL_IPAC_SPEECH_GSM_AMR_FR
@ RSL_IPAC_SPEECH_GSM_AMR_FR
Definition: gsm_08_58.h:756
RSL_IPAC_SPEECH_AS_RTP
@ RSL_IPAC_SPEECH_AS_RTP
Definition: gsm_08_58.h:759
RSL_IPAC_SPEECH_GSM_EFR
@ RSL_IPAC_SPEECH_GSM_EFR
Definition: gsm_08_58.h:755
RSL_CMOD_CRT_TCH_BCAST_Bm
@ RSL_CMOD_CRT_TCH_BCAST_Bm
Definition: gsm_08_58.h:514
RSL_CMOD_CRT_TCH_GROUP_Bm
@ RSL_CMOD_CRT_TCH_GROUP_Bm
Definition: gsm_08_58.h:512
RSL_CMOD_CRT_OSMO_TCH_VAMOS_Bm
@ RSL_CMOD_CRT_OSMO_TCH_VAMOS_Bm
Definition: gsm_08_58.h:516
RSL_CMOD_CRT_TCH_Bm
@ RSL_CMOD_CRT_TCH_Bm
Definition: gsm_08_58.h:508
RSL_CMOD_CRT_TCH_GROUP_Lm
@ RSL_CMOD_CRT_TCH_GROUP_Lm
Definition: gsm_08_58.h:513
RSL_CMOD_CRT_SDCCH
@ RSL_CMOD_CRT_SDCCH
Definition: gsm_08_58.h:507
RSL_CMOD_CRT_TCH_UNI_Bm
@ RSL_CMOD_CRT_TCH_UNI_Bm
Definition: gsm_08_58.h:511
RSL_CMOD_CRT_OSMO_TCH_VAMOS_Lm
@ RSL_CMOD_CRT_OSMO_TCH_VAMOS_Lm
Definition: gsm_08_58.h:517
RSL_CMOD_CRT_TCH_BCAST_Lm
@ RSL_CMOD_CRT_TCH_BCAST_Lm
Definition: gsm_08_58.h:515
RSL_CMOD_CRT_TCH_BI_Bm
@ RSL_CMOD_CRT_TCH_BI_Bm
Definition: gsm_08_58.h:510
RSL_CMOD_CRT_TCH_Lm
@ RSL_CMOD_CRT_TCH_Lm
Definition: gsm_08_58.h:509
RSL_CMOD_CSD_T_1200_75
@ RSL_CMOD_CSD_T_1200_75
Definition: gsm_08_58.h:563
RSL_CMOD_CSD_T_14k4
@ RSL_CMOD_CSD_T_14k4
Definition: gsm_08_58.h:557
RSL_CMOD_CSD_T_2k4
@ RSL_CMOD_CSD_T_2k4
Definition: gsm_08_58.h:560
RSL_CMOD_CSD_T_1k2
@ RSL_CMOD_CSD_T_1k2
Definition: gsm_08_58.h:561
RSL_CMOD_CSD_T_600
@ RSL_CMOD_CSD_T_600
Definition: gsm_08_58.h:562
RSL_CMOD_CSD_T_9k6
@ RSL_CMOD_CSD_T_9k6
Definition: gsm_08_58.h:558
RSL_CMOD_CSD_T_32k0
@ RSL_CMOD_CSD_T_32k0
Definition: gsm_08_58.h:555
RSL_CMOD_CSD_T_29k0
@ RSL_CMOD_CSD_T_29k0
Definition: gsm_08_58.h:556
RSL_CMOD_CSD_T_4k8
@ RSL_CMOD_CSD_T_4k8
Definition: gsm_08_58.h:559
RSL_CMOD_CSD_NT_14k5
@ RSL_CMOD_CSD_NT_14k5
Definition: gsm_08_58.h:538
RSL_CMOD_CSD_NTA_43k5_29k0
@ RSL_CMOD_CSD_NTA_43k5_29k0
Definition: gsm_08_58.h:532
RSL_CMOD_CSD_NT_6k0
@ RSL_CMOD_CSD_NT_6k0
Definition: gsm_08_58.h:540
RSL_CMOD_CSD_NTA_14k5_29k0
@ RSL_CMOD_CSD_NTA_14k5_29k0
Definition: gsm_08_58.h:534
RSL_CMOD_CSD_NTA_29k0_43k5
@ RSL_CMOD_CSD_NTA_29k0_43k5
Definition: gsm_08_58.h:535
RSL_CMOD_CSD_NTA_29k0_14k5
@ RSL_CMOD_CSD_NTA_29k0_14k5
Definition: gsm_08_58.h:531
RSL_CMOD_CSD_NTA_43k5_14k5
@ RSL_CMOD_CSD_NTA_43k5_14k5
Definition: gsm_08_58.h:530
RSL_CMOD_CSD_NT_43k5
@ RSL_CMOD_CSD_NT_43k5
Definition: gsm_08_58.h:536
RSL_CMOD_CSD_NTA_14k5_43k5
@ RSL_CMOD_CSD_NTA_14k5_43k5
Definition: gsm_08_58.h:533
RSL_CMOD_CSD_NT_28k8
@ RSL_CMOD_CSD_NT_28k8
Definition: gsm_08_58.h:537
RSL_CMOD_CSD_NT_12k0
@ RSL_CMOD_CSD_NT_12k0
Definition: gsm_08_58.h:539
ta
uint8_t ta
Definition: gsm_04_08.h:2
len
uint8_t len
Definition: gsm_04_11.h:0
params
uint8_t params[0]
Definition: gsm_08_58.h:6
abis_rsl_cchan_hdr
Definition: gsm_08_58.h:113
abis_rsl_cchan_hdr::chan_nr
uint8_t chan_nr
Definition: gsm_08_58.h:117
abis_rsl_cchan_hdr::c
struct abis_rsl_common_hdr c
Definition: gsm_08_58.h:114
abis_rsl_cchan_hdr::chan_nr_fields
union abis_rsl_chan_nr chan_nr_fields
RSL channel number (value)
Definition: gsm_08_58.h:118
abis_rsl_cchan_hdr::data
uint8_t data[0]
message payload data
Definition: gsm_08_58.h:120
abis_rsl_cchan_hdr::ie_chan
uint8_t ie_chan
RSL_IE_CHAN_NR (tag)
Definition: gsm_08_58.h:115
abis_rsl_common_hdr
RSL common header.
Definition: gsm_08_58.h:79
abis_rsl_common_hdr::data
uint8_t data[0]
actual payload data
Definition: gsm_08_58.h:82
abis_rsl_common_hdr::msg_discr
uint8_t msg_discr
message discriminator (ABIS_RSL_MDISC_*)
Definition: gsm_08_58.h:80
abis_rsl_common_hdr::msg_type
uint8_t msg_type
message type (abis_rsl_msgtype)
Definition: gsm_08_58.h:81
abis_rsl_dchan_hdr
Definition: gsm_08_58.h:102
abis_rsl_dchan_hdr::ie_chan
uint8_t ie_chan
RSL_IE_CHAN_NR (tag)
Definition: gsm_08_58.h:104
abis_rsl_dchan_hdr::chan_nr_fields
union abis_rsl_chan_nr chan_nr_fields
RSL channel number (value)
Definition: gsm_08_58.h:107
abis_rsl_dchan_hdr::data
uint8_t data[0]
message payload data
Definition: gsm_08_58.h:109
abis_rsl_dchan_hdr::chan_nr
uint8_t chan_nr
Definition: gsm_08_58.h:106
abis_rsl_dchan_hdr::c
struct abis_rsl_common_hdr c
Definition: gsm_08_58.h:103
abis_rsl_osmo_rep_acch_cap
Definition: gsm_08_58.h:124
abis_rsl_osmo_temp_ovp_acch_cap
Definition: gsm_08_58.h:139
abis_rsl_rll_hdr
Definition: gsm_08_58.h:86
abis_rsl_rll_hdr::ie_link_id
uint8_t ie_link_id
RSL_IE_LINK_IDENT (tag)
Definition: gsm_08_58.h:93
abis_rsl_rll_hdr::chan_nr_fields
union abis_rsl_chan_nr chan_nr_fields
RSL channel number (value)
Definition: gsm_08_58.h:91
abis_rsl_rll_hdr::c
struct abis_rsl_common_hdr c
Definition: gsm_08_58.h:87
abis_rsl_rll_hdr::data
uint8_t data[0]
message payload data
Definition: gsm_08_58.h:98
abis_rsl_rll_hdr::chan_nr
uint8_t chan_nr
Definition: gsm_08_58.h:90
abis_rsl_rll_hdr::ie_chan
uint8_t ie_chan
RSL_IE_CHAN_NR (tag)
Definition: gsm_08_58.h:88
abis_rsl_rll_hdr::link_id
uint8_t link_id
Definition: gsm_08_58.h:95
abis_rsl_rll_hdr::link_id_fields
union abis_rsl_link_id link_id_fields
RSL link identifier (value)
Definition: gsm_08_58.h:96
ipac_preproc_ave_cfg
Definition: gsm_08_58.h:849
ipac_preproc_cfg
Definition: gsm_08_58.h:1077
ipac_preproc_cfg::ho_ctl_param
struct ipac_preproc_ho_ctl_param ho_ctl_param
Definition: gsm_08_58.h:1085
ipac_preproc_cfg::ms_ave_cfg
struct ipac_preproc_ave_cfg ms_ave_cfg[3]
Definition: gsm_08_58.h:1080
ipac_preproc_cfg::meas_rep_mode
uint8_t meas_rep_mode
Definition: gsm_08_58.h:1078
ipac_preproc_cfg::ncell_dflts
struct ipac_preproc_ncell_dflts ncell_dflts
Definition: gsm_08_58.h:1084
ipac_preproc_cfg::ho_comp
struct ipac_preproc_ho_comp ho_comp
Definition: gsm_08_58.h:1083
ipac_preproc_cfg::ho_thresh
struct ipac_preproc_ho_thresh ho_thresh
Definition: gsm_08_58.h:1082
ipac_preproc_cfg::meas_mode_flags
uint32_t meas_mode_flags
Definition: gsm_08_58.h:1079
ipac_preproc_cfg::ave_cfg
struct ipac_preproc_ave_cfg ave_cfg
Definition: gsm_08_58.h:1081
ipac_preproc_ho_candidates
Definition: gsm_08_58.h:1035
ipac_preproc_ho_comp
HO Threshold Comparators.
Definition: gsm_08_58.h:998
ipac_preproc_ho_ctl_param
Definition: gsm_08_58.h:1066
ipac_preproc_ho_thresh
Handover Thresholds.
Definition: gsm_08_58.h:917
ipac_preproc_ncell_dflts
Definition: gsm_08_58.h:1050
ipac_preproc_pc_comp_field
Osmocom extension for: PC Threshold Comparators (RSL_IPAC_EIE_OSMO_PC_THRESH_COMP)
Definition: gsm_08_58.h:973
ipac_preproc_pc_comp
PC Threshold Comparators (RSL_IPAC_EIE_PC_THRESH_COMP)
Definition: gsm_08_58.h:945
ipac_preproc_pc_thresh
MS/BS Power Control Thresholds (RSL_IPAC_EIE_MS_PWR_CTL)
Definition: gsm_08_58.h:891
osmo_preproc_ave_cfg_field
Definition: gsm_08_58.h:866
osmo_preproc_ave_cfg
Definition: gsm_08_58.h:880
osmo_preproc_ave_cfg::ci_hr
struct osmo_preproc_ave_cfg_field ci_hr
Definition: gsm_08_58.h:882
osmo_preproc_ave_cfg::ci_amr_hr
struct osmo_preproc_ave_cfg_field ci_amr_hr
Definition: gsm_08_58.h:884
osmo_preproc_ave_cfg::ci_gprs
struct osmo_preproc_ave_cfg_field ci_gprs
Definition: gsm_08_58.h:886
osmo_preproc_ave_cfg::ci_fr
struct osmo_preproc_ave_cfg_field ci_fr
Definition: gsm_08_58.h:881
osmo_preproc_ave_cfg::ci_sdcch
struct osmo_preproc_ave_cfg_field ci_sdcch
Definition: gsm_08_58.h:885
osmo_preproc_ave_cfg::ci_amr_fr
struct osmo_preproc_ave_cfg_field ci_amr_fr
Definition: gsm_08_58.h:883
osmo_preproc_ave_cfg::params
uint8_t params[0]
Definition: gsm_08_58.h:887
osmo_preproc_pc_comp
Definition: gsm_08_58.h:987
osmo_preproc_pc_comp::ci_sdcch
struct ipac_preproc_pc_comp_field ci_sdcch
Definition: gsm_08_58.h:993
osmo_preproc_pc_comp::ci_hr
struct ipac_preproc_pc_comp_field ci_hr
Definition: gsm_08_58.h:990
osmo_preproc_pc_comp::ci_gprs
struct ipac_preproc_pc_comp_field ci_gprs
Definition: gsm_08_58.h:994
osmo_preproc_pc_comp::ci_fr
struct ipac_preproc_pc_comp_field ci_fr
Definition: gsm_08_58.h:989
osmo_preproc_pc_comp::ci_amr_hr
struct ipac_preproc_pc_comp_field ci_amr_hr
Definition: gsm_08_58.h:992
osmo_preproc_pc_comp::ci_amr_fr
struct ipac_preproc_pc_comp_field ci_amr_fr
Definition: gsm_08_58.h:991
osmo_preproc_pc_thresh
Osmocom extension for: MS/BS Power Control Thresholds (RSL_IPAC_EIE_OSMO_MS_PWR_CTL)
Definition: gsm_08_58.h:906
osmo_preproc_pc_thresh::l_ci_sdcch
int8_t l_ci_sdcch
Definition: gsm_08_58.h:912
osmo_preproc_pc_thresh::l_ci_fr
int8_t l_ci_fr
Definition: gsm_08_58.h:908
osmo_preproc_pc_thresh::l_ci_gprs
int8_t l_ci_gprs
Definition: gsm_08_58.h:913
osmo_preproc_pc_thresh::u_ci_sdcch
int8_t u_ci_sdcch
Definition: gsm_08_58.h:912
osmo_preproc_pc_thresh::u_ci_hr
int8_t u_ci_hr
Definition: gsm_08_58.h:909
osmo_preproc_pc_thresh::l_ci_amr_hr
int8_t l_ci_amr_hr
Definition: gsm_08_58.h:911
osmo_preproc_pc_thresh::l_ci_amr_fr
int8_t l_ci_amr_fr
Definition: gsm_08_58.h:910
osmo_preproc_pc_thresh::l_ci_hr
int8_t l_ci_hr
Definition: gsm_08_58.h:909
osmo_preproc_pc_thresh::u_ci_amr_fr
int8_t u_ci_amr_fr
Definition: gsm_08_58.h:910
osmo_preproc_pc_thresh::u_ci_fr
int8_t u_ci_fr
Definition: gsm_08_58.h:908
osmo_preproc_pc_thresh::u_ci_gprs
int8_t u_ci_gprs
Definition: gsm_08_58.h:913
osmo_preproc_pc_thresh::u_ci_amr_hr
int8_t u_ci_amr_hr
Definition: gsm_08_58.h:911
rsl_ie_cb_cmd_type
RSL Cell Broadcast Command (Chapter 9.3.41)
Definition: gsm_08_58.h:683
rsl_ie_chan_ident
RSL Channel Identification IE (Chapter 9.3.5)
Definition: gsm_08_58.h:567
rsl_ie_chan_ident::chan_nr
uint8_t chan_nr
Definition: gsm_08_58.h:571
rsl_ie_chan_ident::oct4
uint8_t oct4
Definition: gsm_08_58.h:573
rsl_ie_chan_ident::iei
uint8_t iei
Definition: gsm_08_58.h:570
rsl_ie_chan_ident::chan_desc
struct rsl_ie_chan_ident::@109 chan_desc
rsl_ie_chan_ident::oct3
uint8_t oct3
Definition: gsm_08_58.h:572
rsl_ie_chan_mode
RSL Channel Mode IF (Chapter 9.3.6)
Definition: gsm_08_58.h:492
rsl_ie_chan_mode::chan_rt
uint8_t chan_rt
Definition: gsm_08_58.h:495
rsl_ie_chan_mode::dtx_dtu
uint8_t dtx_dtu
Definition: gsm_08_58.h:493
rsl_ie_chan_mode::spd_ind
uint8_t spd_ind
Definition: gsm_08_58.h:494
rsl_ie_chan_mode::chan_rate
uint8_t chan_rate
Definition: gsm_08_58.h:496
rsl_ie_nch_drx_info
NCH DRX Information (Chapter 9.3.47)
Definition: gsm_08_58.h:709
rsl_l1_info
Definition: gsm_08_58.h:1088
rsl_mrpci
Definition: gsm_08_58.h:784
rsl_mrpci::power_class
uint8_t power_class
Definition: gsm_08_58.h:785
rsl_mrpci::gsm_phase
uint8_t gsm_phase
Definition: gsm_08_58.h:788
rsl_mrpci::vgcs_capable
uint8_t vgcs_capable
Definition: gsm_08_58.h:786
rsl_mrpci::vbs_capable
uint8_t vbs_capable
Definition: gsm_08_58.h:787
abis_rsl_chan_nr
Definition: gsm_08_58.h:31
abis_rsl_chan_nr::__attribute__
struct abis_rsl_chan_nr::@90 __attribute__((packed))
abis_rsl_chan_nr::chan_nr
uint8_t chan_nr
Definition: gsm_08_58.h:41
abis_rsl_link_id
Definition: gsm_08_58.h:59
abis_rsl_link_id::link_id
uint8_t link_id
Definition: gsm_08_58.h:73
abis_rsl_link_id::__attribute__
struct abis_rsl_link_id::@92 __attribute__((packed))