libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - a -

- a5_bits : gsm48_classmark3
- abort : bsslap_pdu
- acc_delay : ph_rach_ind_param
- acc_delay_256bits : ph_rach_ind_param
- access_network_proto : osmo_gsup_an_apdu
- act_cnf : mph_info_param
- act_req : mph_info_param
- active : osmo_iuup_rnl_config
- add_pos_cap : gsm48_classmark3
- addr : osmo_gsn_address
- addr1 : sdp_header_entry
- addr2 : sdp_header_entry
- algo : gprs_cipher_impl, osmo_auth_impl, osmo_sub_auth_data2, osmo_sub_auth_data
- alive_retries : abis_nm_ipacc_att_ns_cfg
- alive_timer : abis_nm_ipacc_att_ns_cfg
- alpha : osmo_gprs_power_ctrl_pars
- alt : gad_raw_ell_point_alt, osmo_gad_ell_point_alt, osmo_gad_ell_point_alt_unc_ell, osmo_gad_ha_ell_point_alt_unc_ell
- amf : osmo_sub_auth_data2, osmo_sub_auth_data
- an_apdu : osmo_gsup_message
- aoip_transport_layer : gsm0808_handover_request, gsm0808_handover_request_ack, gsm0808_vgcs_vbs_assign_req, gsm0808_vgcs_vbs_assign_res
- aoip_transport_layer_present : gsm0808_vgcs_vbs_assign_req, gsm0808_vgcs_vbs_assign_res
- apdu : bssmap_le_conn_oriented_info, bssmap_le_perform_loc_req
- apdu_present : bssmap_le_perform_loc_req
- apn_enc : osmo_gsup_pdp_info
- apn_enc_len : osmo_gsup_pdp_info
- app_data : gsm0808_notification_data
- arfcn : osmo_earfcn_si2q
- arfcn_first : gsm_freq_range
- arfcn_last : gsm_freq_range
- ass_req : gsm0808_vgcs_vbs_area_cell_info, gsm0808_vgcs_vbs_assign_req
- ass_req_present : gsm0808_vgcs_vbs_area_cell_info
- assoc_radio_cap : gsm48_classmark3
- assoc_radio_cap_1 : gsm48_classmark3
- assoc_radio_cap_2 : gsm48_classmark3
- async : gsm_mncc_bearer_cap
- attrib : abis_nm_channel
- auth_types : osmo_auth_vector
- auth_vectors : osmo_gsup_message
- autn : osmo_auth_vector, osmo_oap_message
- autn_present : osmo_oap_message
- auts : osmo_gsup_message, osmo_oap_message
- auts_present : osmo_oap_message
- ave_cfg : ipac_preproc_cfg