libosmogsm 1.13.1.1-afb4 Osmocom GSM library

### - t -

- t1 : gsm_time
- t1_blocking_retries : abis_nm_ipacc_att_bssgp_cfg
- t1_s : abis_nm_ipacc_att_bssgp_cfg
- t1_unblocking_retries : abis_nm_ipacc_att_bssgp_cfg
- t2 : gsm_time
- t200_fn : lapdm_datalink
- t200_timeout : lapdm_datalink
- t2_retries : abis_nm_ipacc_att_bssgp_cfg
- t2_s : abis_nm_ipacc_att_bssgp_cfg
- t3 : gsm_time
- t3142 : abis_nm_ipacc_att_rlc_cfg
- t3168 : osmo_gprs_cell_options
- t3169 : abis_nm_ipacc_att_rlc_cfg
- t3191 : abis_nm_ipacc_att_rlc_cfg
- t3192 : osmo_gprs_cell_options
- t3193_10ms : abis_nm_ipacc_att_rlc_cfg
- t3195 : abis_nm_ipacc_att_rlc_cfg
- t3_100ms : abis_nm_ipacc_att_bssgp_cfg
- t3_retries : abis_nm_ipacc_att_bssgp_cfg
- t4_100ms : abis_nm_ipacc_att_bssgp_cfg
- t4_retries : abis_nm_ipacc_att_bssgp_cfg
- t5_retries : abis_nm_ipacc_att_bssgp_cfg
- t5_s : abis_nm_ipacc_att_bssgp_cfg
- t_avg_t : osmo_gprs_power_ctrl_pars
- t_avg_w : osmo_gprs_power_ctrl_pars
- t_dl_tbf_ext_10ms : abis_nm_ipacc_att_rlc_cfg_2
- t_gsm_400_bands_supp : gsm48_classmark3
- t_gsm_810_assoc_radio_cap : gsm48_classmark3
- t_init : osmo_iuup_rnl_config
- t_ms : osmo_iuup_rnl_config_timer
- t_rc : osmo_iuup_rnl_config
- t_ta : osmo_iuup_rnl_config
- t_ul_tbf_ext_10ms : abis_nm_ipacc_att_rlc_cfg_2
- ta : bsslap_reset, bsslap_ta_layer3, bsslap_ta_response, gsm0408_vgcs_ul_grant, lapdm_entity, osmo_iuup_instance, ph_rach_req_param
- ta_ind : lapdm_msg_ctx
- ta_layer3 : bsslap_pdu
- ta_offs_256bits : info_meas_ind_param, ph_data_param, ph_tch_param
- ta_offs_qbits : info_meas_ind_param, ph_data_param
- ta_response : bsslap_pdu
- table_offset : sdp_firmware
- tac : osmo_tracking_area_id
- talker_id : gsm0808_talker_identity
- talker_identity : gsm0808_uplink_reject_cmd, gsm0808_uplink_request_ack, gsm0808_uplink_request_cnf, gsm0808_uplink_seized_cmd
- talker_identity_present : gsm0808_uplink_reject_cmd, gsm0808_uplink_request_ack, gsm0808_uplink_request_cnf, gsm0808_uplink_seized_cmd
- talker_priority : gsm0808_uplink_release_ind, gsm0808_uplink_request, gsm0808_uplink_request_ack, gsm0808_uplink_seized_cmd
- talker_priority_present : gsm0808_uplink_release_ind, gsm0808_uplink_request, gsm0808_uplink_request_ack, gsm0808_uplink_seized_cmd
- tc : gsm_time
- tch : osmo_phsap_prim
- temp_offs : osmo_gsm48_si_selection_params
- test_timer : abis_nm_ipacc_att_ns_cfg
- text : ussd_request
- text1 : sdp_firmware, sdp_header_entry
- text2 : sdp_firmware, sdp_header_entry
- tf : gsm0808_speech_codec
- thresh_hi : osmo_earfcn_si2q
- thresh_lo : osmo_earfcn_si2q
- thresh_lo_valid : osmo_earfcn_si2q
- tighter_capability : gsm48_classmark3
- time : sdp_firmware, sdp_header_entry
- time_alignment : osmo_iuup_rnl_status
- time_ind : mph_info_param
- timer : osmo_iuup_instance, osmo_timer_nt
- timeslot : abis_nm_channel
- timing_advance : gsm48_imm_ass
- timing_advance1 : gsm48_imm_ass_ext
- timing_advance2 : gsm48_imm_ass_ext
- tlli : gsm48_gprs_susp_req
- tlv_def : osmo_tlv_prot_def
- traf_class : gsm48_qos
- transaction_id : ss_request, ussd_request
- transfer : gsm_mncc_bearer_cap
- transp : gsm_mncc_bearer_cap
- transparent : osmo_iuup_rnl_config
- transport_prim_cb : osmo_iuup_instance
- transport_prim_priv : osmo_iuup_instance
- trx_id : ipaccess_unit
- trx_nr : abis_om_obj_inst
- ts_nr : abis_om_obj_inst
- tx_pending : lapdm_entity
- tx_power : lapdm_entity, ph_rach_req_param
- tx_power_ind : lapdm_msg_ctx
- tx_ui_queue : lapdm_datalink
- type : bssmap_header, dtap_header, gsm0808_speech_codec, gsm48_pdp_address, gsm_mncc_number, mph_info_param, osmo_bssap_le_header, osmo_gad, osmo_gad_err, osmo_gsn_address, osmo_sub_auth_data2, osmo_sub_auth_data, smcdatastate, smcdownstate, smrdatastate, smrdownstate, tlv_def
- type14_fn : osmo_iuup_instance