libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Macros
gsm_23_003.h File Reference

Go to the source code of this file.

## Macros
#define | GSM23003_IMSI_MAX_DIGITS 15
#define | GSM23003_IMSI_MIN_DIGITS 6
#define | OSMO_IMSI_BUF_SIZE (GSM23003_IMSI_MAX_DIGITS+2)
| The char[] buffer size to completely contain an IMSI including the optional checksum digit as well as the terminating nul character. More...
#define | GSM23003_TMSI_NUM_BYTES 4
#define | GSM23003_TMSI_SGSN_MASK 0xC0000000UL
#define | GSM23003_LMSI_NUM_BYTES 4
#define | GSM23003_TLLI_NUM_BYTES 4
#define | GSM23003_PTMSI_SIG_NUM_BYTES 3
#define | GSM23003_MME_CODE_NUM_BYTES 1
#define | GSM23003_MME_GROUP_NUM_BYTES 2
#define | GSM23003_MTMSI_NUM_BYTES 4
#define | GSM23003_MSISDN_MAX_DIGITS 15 /* ITU-T Rec. E.164 6.1 */
#define | GSM23003_MSISDN_MIN_DIGITS 1
#define | GSM23003_IMEI_TAC_NUM_DIGITS 8
#define | GSM23003_IMEI_SNR_NUM_DIGITS 6
#define | GSM23003_IMEI_NUM_DIGITS
#define | GSM23003_IMEISV_NUM_DIGITS
#define | GSM23003_IMEI_NUM_DIGITS_NO_CHK
#define | GSM23003_HOME_NETWORK_DOMAIN_LEN 33
#define | GSM23003_MME_DOMAIN_LEN 55

## Macro Definition Documentation

## ◆ GSM23003_HOME_NETWORK_DOMAIN_LEN

#define GSM23003_HOME_NETWORK_DOMAIN_LEN 33

## ◆ GSM23003_IMEI_NUM_DIGITS

#define GSM23003_IMEI_NUM_DIGITS

Value:
(GSM23003_IMEI_TAC_NUM_DIGITS + \
GSM23003_IMEI_SNR_NUM_DIGITS + 1)
GSM23003_IMEI_TAC_NUM_DIGITS
#define GSM23003_IMEI_TAC_NUM_DIGITS
Definition: gsm_23_003.h:28

## ◆ GSM23003_IMEI_NUM_DIGITS_NO_CHK

#define GSM23003_IMEI_NUM_DIGITS_NO_CHK

Value:
(GSM23003_IMEI_TAC_NUM_DIGITS + \
GSM23003_IMEI_SNR_NUM_DIGITS)

## ◆ GSM23003_IMEI_SNR_NUM_DIGITS

#define GSM23003_IMEI_SNR_NUM_DIGITS 6

## ◆ GSM23003_IMEI_TAC_NUM_DIGITS

#define GSM23003_IMEI_TAC_NUM_DIGITS 8

## ◆ GSM23003_IMEISV_NUM_DIGITS

#define GSM23003_IMEISV_NUM_DIGITS

Value:
(GSM23003_IMEI_TAC_NUM_DIGITS + \
GSM23003_IMEI_SNR_NUM_DIGITS + 2)

## ◆ GSM23003_IMSI_MAX_DIGITS

#define GSM23003_IMSI_MAX_DIGITS 15

## ◆ GSM23003_IMSI_MIN_DIGITS

#define GSM23003_IMSI_MIN_DIGITS 6

## ◆ GSM23003_LMSI_NUM_BYTES

#define GSM23003_LMSI_NUM_BYTES 4

## ◆ GSM23003_MME_CODE_NUM_BYTES

#define GSM23003_MME_CODE_NUM_BYTES 1

## ◆ GSM23003_MME_DOMAIN_LEN

#define GSM23003_MME_DOMAIN_LEN 55

## ◆ GSM23003_MME_GROUP_NUM_BYTES

#define GSM23003_MME_GROUP_NUM_BYTES 2

## ◆ GSM23003_MSISDN_MAX_DIGITS

#define GSM23003_MSISDN_MAX_DIGITS 15 /* ITU-T Rec. E.164 6.1 */

## ◆ GSM23003_MSISDN_MIN_DIGITS

#define GSM23003_MSISDN_MIN_DIGITS 1

## ◆ GSM23003_MTMSI_NUM_BYTES

#define GSM23003_MTMSI_NUM_BYTES 4

## ◆ GSM23003_PTMSI_SIG_NUM_BYTES

#define GSM23003_PTMSI_SIG_NUM_BYTES 3

## ◆ GSM23003_TLLI_NUM_BYTES

#define GSM23003_TLLI_NUM_BYTES 4

## ◆ GSM23003_TMSI_NUM_BYTES

#define GSM23003_TMSI_NUM_BYTES 4

## ◆ GSM23003_TMSI_SGSN_MASK

#define GSM23003_TMSI_SGSN_MASK 0xC0000000UL

## ◆ OSMO_IMSI_BUF_SIZE

#define OSMO_IMSI_BUF_SIZE (GSM23003_IMSI_MAX_DIGITS+2)

The char[] buffer size to completely contain an IMSI including the optional checksum digit as well as the terminating nul character.