libosmo-netif 1.7.0.10-3a9e Osmocom network interface library

Data Fields
osmo_twrtp_stats Struct Reference
Themyscira Wireless RTP endpoint implementation

Stats collected during the lifetime of a twrtp instance. More...

`#include <twrtp.h>`

## Data Fields
uint32_t | rx_rtp_pkt
uint32_t | rx_rtp_badsrc
uint32_t | rx_rtcp_pkt
uint32_t | rx_rtcp_badsrc
uint32_t | rx_rtcp_invalid
uint32_t | rx_rtcp_wrong_ssrc
uint32_t | tx_rtp_pkt
uint32_t | tx_rtp_bytes
uint32_t | tx_rtcp_pkt

## Detailed Description

Stats collected during the lifetime of a twrtp instance.

For a detailed description of each of these counters, see Chapter 6 of twrtp guide document.

This stats structure is never allocated or accessed in a writable manner by applications; instead it is allocated inside the library as part of opaque struct osmo_twrtp, while applications are given const pointers to these structs.

The documentation for this struct was generated from the following file:

- include/osmocom/netif/twrtp.h