libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Files | Data Structures | Macros | Enumerations | Functions | Variables
A-bis RSL

GSM Radio Signalling Link messages on the A-bis interface. More...

## Files
file | gsm_08_58.h
| GSM Radio Signalling Link messages on the A-bis interface.
file | rsl.h
file | rsl.c

## Data Structures
union | abis_rsl_chan_nr
union | abis_rsl_link_id
struct | abis_rsl_common_hdr
| RSL common header. More...
struct | abis_rsl_rll_hdr
struct | abis_rsl_dchan_hdr
struct | abis_rsl_cchan_hdr
struct | abis_rsl_osmo_rep_acch_cap
struct | abis_rsl_osmo_temp_ovp_acch_cap
struct | rsl_ie_chan_mode
| RSL Channel Mode IF (Chapter 9.3.6) More...
struct | rsl_ie_chan_ident
| RSL Channel Identification IE (Chapter 9.3.5) More...
struct | rsl_ie_cb_cmd_type
| RSL Cell Broadcast Command (Chapter 9.3.41) More...
struct | rsl_ie_nch_drx_info
| NCH DRX Information (Chapter 9.3.47) More...
struct | rsl_mrpci
struct | ipac_preproc_ave_cfg
struct | osmo_preproc_ave_cfg_field
struct | osmo_preproc_ave_cfg
struct | ipac_preproc_pc_thresh
| MS/BS Power Control Thresholds (RSL_IPAC_EIE_MS_PWR_CTL) More...
struct | osmo_preproc_pc_thresh
| Osmocom extension for: MS/BS Power Control Thresholds (RSL_IPAC_EIE_OSMO_MS_PWR_CTL) More...
struct | ipac_preproc_ho_thresh
| Handover Thresholds. More...
struct | ipac_preproc_pc_comp
| PC Threshold Comparators (RSL_IPAC_EIE_PC_THRESH_COMP) More...
struct | ipac_preproc_pc_comp_field
| Osmocom extension for: PC Threshold Comparators (RSL_IPAC_EIE_OSMO_PC_THRESH_COMP) More...
struct | osmo_preproc_pc_comp
struct | ipac_preproc_ho_comp
| HO Threshold Comparators. More...
struct | ipac_preproc_ho_candidates
struct | ipac_preproc_ncell_dflts
struct | ipac_preproc_ho_ctl_param
struct | ipac_preproc_cfg
struct | rsl_l1_info

## Macros
#define | ABIS_RSL_CHAN_NR_CBITS_Bm_ACCHs 0x01
#define | ABIS_RSL_CHAN_NR_CBITS_Lm_ACCHs(ss) (0x02 + (ss))
#define | ABIS_RSL_CHAN_NR_CBITS_SDCCH4_ACCH(ss) (0x04 + (ss))
#define | ABIS_RSL_CHAN_NR_CBITS_SDCCH8_ACCH(ss) (0x08 + (ss))
#define | ABIS_RSL_CHAN_NR_CBITS_BCCH 0x10
#define | ABIS_RSL_CHAN_NR_CBITS_RACH 0x11
#define | ABIS_RSL_CHAN_NR_CBITS_PCH_AGCH 0x12
#define | ABIS_RSL_CHAN_NR_CBITS_OSMO_PDCH 0x18 /*< non-standard, for dyn TS */
#define | ABIS_RSL_CHAN_NR_CBITS_OSMO_CBCH4 0x19 /*< non-standard, for CBCH/SDCCH4 */
#define | ABIS_RSL_CHAN_NR_CBITS_OSMO_CBCH8 0x1a /*< non-standard, for CBCH/SDCCH8 */
#define | ABIS_RSL_CHAN_NR_CBITS_OSMO_VAMOS_Bm_ACCHs 0x1d /*< VAMOS TCH/F */
#define | ABIS_RSL_CHAN_NR_CBITS_OSMO_VAMOS_Lm_ACCHs(ss) (0x1e + (ss)) /*< VAMOS TCH/H */
#define | ABIS_RSL_LINK_ID_CBITS_FACCH_SDCCH 0x00
#define | ABIS_RSL_LINK_ID_CBITS_SACCH 0x01
#define | ABIS_RSL_MDISC_RLL 0x02
#define | ABIS_RSL_MDISC_DED_CHAN 0x08
#define | ABIS_RSL_MDISC_COM_CHAN 0x0c
#define | ABIS_RSL_MDISC_TRX 0x10
#define | ABIS_RSL_MDISC_LOC 0x20
#define | ABIS_RSL_MDISC_IPACCESS 0x7e
#define | ABIS_RSL_MDISC_TRANSP 0x01
#define | ABIS_RSL_MDISC_IS_TRANSP(x) (x & 0x01)
#define | RSL_IE_ERIC_PAGING_GROUP 0x0e
#define | RSL_IE_ERIC_INST_NR 0x48
#define | RSL_IE_ERIC_PGSL_TIMERS 0x49
#define | RSL_IE_ERIC_REPEAT_DL_FACCH 0x4a
#define | RSL_IE_ERIC_POWER_INFO 0xf0
#define | RSL_IE_ERIC_MOBILE_ID 0xf1
#define | RSL_IE_ERIC_BCCH_MAPPING 0xf2
#define | RSL_IE_ERIC_PACKET_PAG_IND 0xf3
#define | RSL_IE_ERIC_CNTR_CTRL 0xf4
#define | RSL_IE_ERIC_CNTR_CTRL_ACK 0xf5
#define | RSL_IE_ERIC_CNTR_REPORT 0xf6
#define | RSL_IE_ERIC_ICP_CONN 0xf7
#define | RSL_IE_ERIC_EMR_SUPPORT 0xf8
#define | RSL_IE_ERIC_EGPRS_REQ_REF 0xf9
#define | RSL_IE_ERIC_VGCS_REL 0xfa
#define | RSL_IE_ERIC_REP_PER_NCH 0xfb
#define | RSL_IE_ERIC_NY2 0xfc
#define | RSL_IE_ERIC_T3115 0xfd
#define | RSL_IE_ERIC_ACTIVATE_FLAG 0xfe
#define | RSL_IE_ERIC_FULL_NCH_INFO 0xff
#define | RSL_CHAN_NR_MASK 0xf8
#define | RSL_CHAN_NR_1 0x08 /*< bit to add for 2nd,... lchan */
#define | RSL_CHAN_Bm_ACCHs 0x08
#define | RSL_CHAN_Lm_ACCHs 0x10 /* .. 0x18 */
#define | RSL_CHAN_SDCCH4_ACCH 0x20 /* .. 0x38 */
#define | RSL_CHAN_SDCCH8_ACCH 0x40 /* ...0x78 */
#define | RSL_CHAN_BCCH 0x80
#define | RSL_CHAN_RACH 0x88
#define | RSL_CHAN_PCH_AGCH 0x90
#define | RSL_CHAN_OSMO_PDCH 0xc0 /*< non-standard, for dyn TS */
#define | RSL_CHAN_OSMO_CBCH4 0xc8 /*< non-standard, for CBCH/SDCCH4 */
#define | RSL_CHAN_OSMO_CBCH8 0xd0 /*< non-standard, for CBCH/SDCCH8 */
#define | RSL_CHAN_OSMO_VAMOS_Bm_ACCHs 0xe8 /* VAMOS TCH/F */
#define | RSL_CHAN_OSMO_VAMOS_Lm_ACCHs 0xf0 /* VAMOS TCH/H */
#define | RSL_CHAN_OSMO_VAMOS_MASK 0xe0 /* VAMOS TCH/{F,H} */
#define | RSL_ACT_TYPE_INITIAL 0x00
#define | RSL_ACT_TYPE_REACT 0x80
#define | RSL_ACT_INTRA_IMM_ASS 0x00
#define | RSL_ACT_INTRA_NORM_ASS 0x01
#define | RSL_ACT_INTER_ASYNC 0x02
#define | RSL_ACT_INTER_SYNC 0x03
#define | RSL_ACT_SECOND_ADD 0x04
#define | RSL_ACT_SECOND_MULTI 0x05
#define | RSL_ACT_OSMO_PDCH 0x0f /*< non-standard, for dyn TS */
#define | RSL_CMOD_DTXu 0x01 /* uplink */
#define | RSL_CMOD_DTXd 0x02 /* downlink */
#define | RSL_CMOD_SP_NT_14k5 RSL_CMOD_CSD_NT_14k5
#define | RSL_CMOD_SP_NT_12k0 RSL_CMOD_CSD_NT_12k0
#define | RSL_CMOD_SP_NT_6k0 RSL_CMOD_CSD_NT_6k0
#define | RSL_CMOD_CSD_T_32000 RSL_CMOD_CSD_T_32k0
#define | RSL_CMOD_CSD_T_29000 RSL_CMOD_CSD_T_29k0
#define | RSL_CMOD_CSD_T_14400 RSL_CMOD_CSD_T_14k4
#define | RSL_CMOD_CSD_T_9600 RSL_CMOD_CSD_T_9k6
#define | RSL_CMOD_CSD_T_4800 RSL_CMOD_CSD_T_4k8
#define | RSL_CMOD_CSD_T_2400 RSL_CMOD_CSD_T_2k4
#define | RSL_CMOD_CSD_T_1200 RSL_CMOD_CSD_T_1k2
#define | RLL_CAUSE_T200_EXPIRED 0x01
#define | RLL_CAUSE_REEST_REQ 0x02
#define | RLL_CAUSE_UNSOL_UA_RESP 0x03
#define | RLL_CAUSE_UNSOL_DM_RESP 0x04
#define | RLL_CAUSE_UNSOL_DM_RESP_MF 0x05
#define | RLL_CAUSE_UNSOL_SPRV_RESP 0x06
#define | RLL_CAUSE_SEQ_ERR 0x07
#define | RLL_CAUSE_UFRM_INC_PARAM 0x08
#define | RLL_CAUSE_SFRM_INC_PARAM 0x09
#define | RLL_CAUSE_IFRM_INC_MBITS 0x0a
#define | RLL_CAUSE_IFRM_INC_LEN 0x0b
#define | RLL_CAUSE_FRM_UNIMPL 0x0c
#define | RLL_CAUSE_SABM_MF 0x0d
#define | RLL_CAUSE_SABM_INFO_NOTALL 0x0e
#define | RSL_ERRCLS_NORMAL 0x00
#define | RSL_ERRCLS_RESOURCE_UNAVAIL 0x20
#define | RSL_ERRCLS_SERVICE_UNAVAIL 0x30
#define | RSL_ERRCLS_SERVICE_UNIMPL 0x40
#define | RSL_ERRCLS_INVAL_MSG 0x50
#define | RSL_ERRCLS_PROTO_ERROR 0x60
#define | RSL_ERRCLS_INTERWORKING 0x70
#define | RSL_ERR_RADIO_IF_FAIL 0x00
#define | RSL_ERR_RADIO_LINK_FAIL 0x01
#define | RSL_ERR_HANDOVER_ACC_FAIL 0x02
#define | RSL_ERR_TALKER_ACC_FAIL 0x03
#define | RSL_ERR_OM_INTERVENTION 0x07
#define | RSL_ERR_NORMAL_UNSPEC 0x0f
#define | RSL_ERR_T_MSRFPCI_EXP 0x18
#define | RSL_ERR_EQUIPMENT_FAIL 0x20
#define | RSL_ERR_RR_UNAVAIL 0x21
#define | RSL_ERR_TERR_CH_FAIL 0x22
#define | RSL_ERR_CCCH_OVERLOAD 0x23
#define | RSL_ERR_ACCH_OVERLOAD 0x24
#define | RSL_ERR_PROCESSOR_OVERLOAD 0x25
#define | RSL_ERR_BTS_NOT_EQUIPPED 0x27
#define | RSL_ERR_REMOTE_TRANSC_FAIL 0x28
#define | RSL_ERR_NOTIFICATION_OVERFL 0x29
#define | RSL_ERR_RES_UNAVAIL 0x2f
#define | RSL_ERR_TRANSC_UNAVAIL 0x30
#define | RSL_ERR_SERV_OPT_UNAVAIL 0x3f
#define | RSL_ERR_ENCR_UNIMPL 0x40
#define | RSL_ERR_SERV_OPT_UNIMPL 0x4f
#define | RSL_ERR_RCH_ALR_ACTV_ALLOC 0x50
#define | RSL_ERR_INVALID_MESSAGE 0x5f
#define | RSL_ERR_MSG_DISCR 0x60
#define | RSL_ERR_MSG_TYPE 0x61
#define | RSL_ERR_MSG_SEQ 0x62
#define | RSL_ERR_IE_ERROR 0x63
#define | RSL_ERR_MAND_IE_ERROR 0x64
#define | RSL_ERR_OPT_IE_ERROR 0x65
#define | RSL_ERR_IE_NONEXIST 0x66
#define | RSL_ERR_IE_LENGTH 0x67
#define | RSL_ERR_IE_CONTENT 0x68
#define | RSL_ERR_PROTO 0x6f
#define | RSL_ERR_INTERWORKING 0x7f
#define | RSL_SYSTEM_INFO_8 0x00
#define | RSL_SYSTEM_INFO_1 0x01
#define | RSL_SYSTEM_INFO_2 0x02
#define | RSL_SYSTEM_INFO_3 0x03
#define | RSL_SYSTEM_INFO_4 0x04
#define | RSL_SYSTEM_INFO_5 0x05
#define | RSL_SYSTEM_INFO_6 0x06
#define | RSL_SYSTEM_INFO_7 0x07
#define | RSL_SYSTEM_INFO_16 0x08
#define | RSL_SYSTEM_INFO_17 0x09
#define | RSL_SYSTEM_INFO_2bis 0x0a
#define | RSL_SYSTEM_INFO_2ter 0x0b
#define | RSL_SYSTEM_INFO_5bis 0x0d
#define | RSL_SYSTEM_INFO_5ter 0x0e
#define | RSL_SYSTEM_INFO_10 0x0f
#define | RSL_EXT_MEAS_ORDER 0x47
#define | RSL_MEAS_INFO 0x48
#define | RSL_SYSTEM_INFO_13 0x28
#define | RSL_ERIC_SYSTEM_INFO_13 0x0C
#define | RSL_SYSTEM_INFO_2quater 0x29
#define | RSL_SYSTEM_INFO_9 0x2a
#define | RSL_SYSTEM_INFO_18 0x2b
#define | RSL_SYSTEM_INFO_19 0x2c
#define | RSL_SYSTEM_INFO_20 0x2d
#define | RSL_CHANNEED_ANY 0x00
#define | RSL_CHANNEED_SDCCH 0x01
#define | RSL_CHANNEED_TCH_F 0x02
#define | RSL_CHANNEED_TCH_ForH 0x03
#define | RSL_CB_CMD_TYPE_NORMAL 0x00
#define | RSL_CB_CMD_TYPE_SCHEDULE 0x08
#define | RSL_CB_CMD_TYPE_DEFAULT 0x0e
#define | RSL_CB_CMD_TYPE_NULL 0x0f
#define | RSL_CB_CMD_DEFBCAST_NORMAL 0
#define | RSL_CB_CMD_DEFBCAST_NULL 1
#define | RSL_CB_CMD_LASTBLOCK_4 0
#define | RSL_CB_CMD_LASTBLOCK_1 1
#define | RSL_CB_CMD_LASTBLOCK_2 2
#define | RSL_CB_CMD_LASTBLOCK_3 3
#define | RSL_CMD_INDICATOR_START 0x00
| Command Indicator (Chapter 9.3.48) More...
#define | RSL_CMD_INDICATOR_STOP 0x01
#define | RSL_BCCH_CCCH_CONF_1_NC 0x00
#define | RSL_BCCH_CCCH_CONF_1_C 0x01
#define | RSL_BCCH_CCCH_CONF_2_NC 0x02
#define | RSL_BCCH_CCCH_CONF_3_NC 0x04
#define | RSL_BCCH_CCCH_CONF_4_NC 0x06
#define | RSL_BS_PA_MFRMS_2 0x00
#define | RSL_BS_PA_MFRMS_3 0x01
#define | RSL_BS_PA_MFRMS_4 0x02
#define | RSL_BS_PA_MFRMS_5 0x03
#define | RSL_BS_PA_MFRMS_6 0x04
#define | RSL_BS_PA_MFRMS_7 0x05
#define | RSL_BS_PA_MFRMS_8 0x06
#define | RSL_BS_PA_MFRMS_9 0x07
#define | rsl_tlv_parse(dec, buf, len) tlv_parse(dec, &rsl_att_tlvdef, buf, len, 0, 0)
| Parse RSL TLV structure using tlv_parse. More...
#define | rsl_ipac_eie_tlv_parse(dec, buf, len) tlv_parse(dec, &rsl_ipac_eie_tlvdef, buf, len, 0, 0)
| Parse RSL IPAC EIE TLV structure using tlv_parse. More...
#define | RSL_ALLOC_SIZE 200
| Size for RSL msgb_alloc. More...
#define | RSL_ALLOC_HEADROOM 56
| Headroom size for RSL msgb_alloc. More...

## Enumerations
enum | abis_rsl_msgtype { RSL_MT_DATA_REQ = 0x01 , RSL_MT_DATA_IND , RSL_MT_ERROR_IND , RSL_MT_EST_REQ , RSL_MT_EST_CONF , RSL_MT_EST_IND , RSL_MT_REL_REQ , RSL_MT_REL_CONF , RSL_MT_REL_IND , RSL_MT_UNIT_DATA_REQ , RSL_MT_UNIT_DATA_IND , RSL_MT_SUSP_REQ , RSL_MT_SUSP_CONF , RSL_MT_RES_REQ , RSL_MT_RECON_REQ , RSL_MT_BCCH_INFO = 0x11 , RSL_MT_CCCH_LOAD_IND , RSL_MT_CHAN_RQD , RSL_MT_DELETE_IND , RSL_MT_PAGING_CMD , RSL_MT_IMMEDIATE_ASSIGN_CMD , RSL_MT_SMS_BC_REQ , RSL_MT_CHAN_CONF , RSL_MT_RF_RES_IND = 0x19 , RSL_MT_SACCH_FILL , RSL_MT_OVERLOAD , RSL_MT_ERROR_REPORT , RSL_MT_SMS_BC_CMD , RSL_MT_CBCH_LOAD_IND , RSL_MT_NOT_CMD , RSL_MT_CHAN_ACTIV = 0x21 , RSL_MT_CHAN_ACTIV_ACK , RSL_MT_CHAN_ACTIV_NACK , RSL_MT_CONN_FAIL , RSL_MT_DEACTIVATE_SACCH , RSL_MT_ENCR_CMD , RSL_MT_HANDO_DET , RSL_MT_MEAS_RES , RSL_MT_MODE_MODIFY_REQ , RSL_MT_MODE_MODIFY_ACK , RSL_MT_MODE_MODIFY_NACK , RSL_MT_PHY_CONTEXT_REQ , RSL_MT_PHY_CONTEXT_CONF , RSL_MT_RF_CHAN_REL , RSL_MT_MS_POWER_CONTROL , RSL_MT_BS_POWER_CONTROL , RSL_MT_PREPROC_CONFIG , RSL_MT_PREPROC_MEAS_RES , RSL_MT_RF_CHAN_REL_ACK , RSL_MT_SACCH_INFO_MODIFY , RSL_MT_TALKER_DET , RSL_MT_LISTENER_DET , RSL_MT_REMOTE_CODEC_CONF_REP , RSL_MT_RTD_REP , RSL_MT_PRE_HANDO_NOTIF , RSL_MT_MR_CODEC_MOD_REQ , RSL_MT_MR_CODEC_MOD_ACK , RSL_MT_MR_CODEC_MOD_NACK , RSL_MT_MR_CODEC_MOD_PER , RSL_MT_TFO_REP , RSL_MT_TFO_MOD_REQ , RSL_MT_LOCATION_INFO = 0x41 , RSL_MT_IPAC_DIR_RETR_ENQ = 0x40 , RSL_MT_IPAC_PDCH_ACT = 0x48 , RSL_MT_IPAC_PDCH_ACT_ACK , RSL_MT_IPAC_PDCH_ACT_NACK , RSL_MT_IPAC_PDCH_DEACT = 0x4b , RSL_MT_IPAC_PDCH_DEACT_ACK , RSL_MT_IPAC_PDCH_DEACT_NACK , RSL_MT_IPAC_CONNECT_MUX = 0x50 , RSL_MT_IPAC_CONNECT_MUX_ACK , RSL_MT_IPAC_CONNECT_MUX_NACK , RSL_MT_IPAC_BIND_MUX = 0x53 , RSL_MT_IPAC_BIND_MUX_ACK , RSL_MT_IPAC_BIND_MUX_NACK , RSL_MT_IPAC_DISC_MUX = 0x56 , RSL_MT_IPAC_DISC_MUX_ACK , RSL_MT_IPAC_DISC_MUX_NACK , RSL_MT_IPAC_MEAS_PREPROC_DFT = 0x60 , RSL_MT_IPAC_HO_CAN_ENQ = 0x61 , RSL_MT_IPAC_HO_CAN_RES = 0x62 , RSL_MT_IPAC_CRCX = 0x70 , RSL_MT_IPAC_CRCX_ACK , RSL_MT_IPAC_CRCX_NACK , RSL_MT_IPAC_MDCX = 0x73 , RSL_MT_IPAC_MDCX_ACK , RSL_MT_IPAC_MDCX_NACK , RSL_MT_IPAC_DLCX_IND = 0x76 , RSL_MT_IPAC_DLCX = 0x77 , RSL_MT_IPAC_DLCX_ACK , RSL_MT_IPAC_DLCX_NACK , RSL_MT_OSMO_ETWS_CMD = 0x7f }
enum | abis_rsl_msgtype_siemens { RSL_MT_SIEMENS_MRPCI = 0x41 , RSL_MT_SIEMENS_INTRAC_HO_COND_IND = 0x42 , RSL_MT_SIEMENS_INTERC_HO_COND_IND = 0x43 , RSL_MT_SIEMENS_FORCED_HO_REQ = 0x44 , RSL_MT_SIEMENS_PREF_AREA_REQ = 0x45 , RSL_MT_SIEMENS_PREF_AREA = 0x46 , RSL_MT_SIEMENS_START_TRACE = 0x47 , RSL_MT_SIEMENS_START_TRACE_ACK = 0x48 , RSL_MT_SIEMENS_STOP_TRACE = 0x49 , RSL_MT_SIEMENS_TRMR = 0x4a , RSL_MT_SIEMENS_HO_FAIL_IND = 0x4b , RSL_MT_SIEMENS_STOP_TRACE_ACK = 0x4c , RSL_MT_SIEMENS_UPLF = 0x4d , RSL_MT_SIEMENS_UPLB = 0x4e , RSL_MT_SIEMENS_SET_SYS_INFO_10 = 0x4f , RSL_MT_SIEMENS_MODIF_COND_IND = 0x50 }
| Siemens vendor-specific RSL message types. More...
enum | abis_rsl_msgtype_ericsson { RSL_MT_ERICSSON_IMM_ASS_SENT = 0x10 }
| Ericsson vendor-specific RSL message types. More...
enum | abis_rsl_ie { RSL_IE_CHAN_NR = 0x01 , RSL_IE_LINK_IDENT , RSL_IE_ACT_TYPE , RSL_IE_BS_POWER , RSL_IE_CHAN_IDENT , RSL_IE_CHAN_MODE , RSL_IE_ENCR_INFO , RSL_IE_FRAME_NUMBER , RSL_IE_HANDO_REF , RSL_IE_L1_INFO , RSL_IE_L3_INFO , RSL_IE_MS_IDENTITY , RSL_IE_MS_POWER , RSL_IE_PAGING_GROUP , RSL_IE_PAGING_LOAD , RSL_IE_PYHS_CONTEXT = 0x10 , RSL_IE_ACCESS_DELAY , RSL_IE_RACH_LOAD , RSL_IE_REQ_REFERENCE , RSL_IE_RELEASE_MODE , RSL_IE_RESOURCE_INFO , RSL_IE_RLM_CAUSE , RSL_IE_STARTNG_TIME , RSL_IE_TIMING_ADVANCE , RSL_IE_UPLINK_MEAS , RSL_IE_CAUSE , RSL_IE_MEAS_RES_NR , RSL_IE_MSG_ID , RSL_IE_SYSINFO_TYPE = 0x1e , RSL_IE_MS_POWER_PARAM , RSL_IE_BS_POWER_PARAM , RSL_IE_PREPROC_PARAM , RSL_IE_PREPROC_MEAS , RSL_IE_IMM_ASS_INFO , RSL_IE_SMSCB_INFO = 0x24 , RSL_IE_MS_TIMING_OFFSET , RSL_IE_ERR_MSG , RSL_IE_FULL_BCCH_INFO , RSL_IE_CHAN_NEEDED , RSL_IE_CB_CMD_TYPE , RSL_IE_SMSCB_MSG , RSL_IE_FULL_IMM_ASS_INFO , RSL_IE_SACCH_INFO , RSL_IE_CBCH_LOAD_INFO , RSL_IE_SMSCB_CHAN_INDICATOR , RSL_IE_GROUP_CALL_REF , RSL_IE_CHAN_DESC = 0x30 , RSL_IE_NCH_DRX_INFO , RSL_IE_CMD_INDICATOR , RSL_IE_EMLPP_PRIO , RSL_IE_UIC , RSL_IE_MAIN_CHAN_REF , RSL_IE_MR_CONFIG , RSL_IE_MR_CONTROL , RSL_IE_SUP_CODEC_TYPES , RSL_IE_CODEC_CONFIG , RSL_IE_RTD , RSL_IE_TFO_STATUS , RSL_IE_LLP_APDU , RSL_IE_TFO_XPAR_CONT , RSL_IE_SIEMENS_MRPCI = 0x40 , RSL_IE_SIEMENS_PREF_AREA_TYPE = 0x43 , RSL_IE_SIEMENS_ININ_CELL_HO_PAR = 0x45 , RSL_IE_SIEMENS_TRACE_REF_NR = 0x46 , RSL_IE_SIEMENS_INT_TRACE_IDX = 0x47 , RSL_IE_SIEMENS_L2_HDR_INFO = 0x48 , RSL_IE_SIEMENS_HIGHEST_RATE = 0x4e , RSL_IE_SIEMENS_SUGGESTED_RATE = 0x4f , RSL_IE_OSMO_REP_ACCH_CAP = 0x60 , RSL_IE_OSMO_TRAINING_SEQUENCE = 0x61 , RSL_IE_OSMO_TEMP_OVP_ACCH_CAP = 0x62 , RSL_IE_OSMO_OSMUX_CID = 0x63 , RSL_IE_OSMO_RTP_EXTENSIONS = 0x64 , RSL_IE_IPAC_SRTP_CONFIG = 0xe0 , RSL_IE_IPAC_PROXY_UDP = 0xe1 , RSL_IE_IPAC_BSCMPL_TOUT = 0xe2 , RSL_IE_IPAC_REMOTE_IP = 0xf0 , RSL_IE_IPAC_REMOTE_PORT = 0xf1 , RSL_IE_IPAC_RTP_PAYLOAD = 0xf2 , RSL_IE_IPAC_LOCAL_PORT = 0xf3 , RSL_IE_IPAC_SPEECH_MODE = 0xf4 , RSL_IE_IPAC_LOCAL_IP = 0xf5 , RSL_IE_IPAC_CONN_STAT = 0xf6 , RSL_IE_IPAC_HO_C_PARMS = 0xf7 , RSL_IE_IPAC_CONN_ID = 0xf8 , RSL_IE_IPAC_RTP_CSD_FMT = 0xf9 , RSL_IE_IPAC_RTP_JIT_BUF = 0xfa , RSL_IE_IPAC_RTP_COMPR = 0xfb , RSL_IE_IPAC_RTP_PAYLOAD2 = 0xfc , RSL_IE_IPAC_RTP_MPLEX = 0xfd , RSL_IE_IPAC_RTP_MPLEX_ID = 0xfe }
| RSL Information Element Identifiers (Chapter 9.3) More...
enum | { IPAC_UNWEIGHTED_AVE = 0 , IPAC_WEIGHTED_AVE , IPAC_MEDIAN_AVE , IPAC_OSMO_EWMA_AVE }
enum | { IPAC_RXLEV_AVE = 0 , IPAC_RXQUAL_AVE , IPAC_MS_BTS_DIS_AVE }
enum | { IPAC_HO_RQD_CAUSE_L_RXLEV_UL_H = 0x01 , IPAC_HO_RQD_CAUSE_L_RXLEV_DL_H , IPAC_HO_RQD_CAUSE_L_RXQUAL_UL_H , IPAC_HO_RQD_CAUSE_L_RXQUAL_DL_H , IPAC_HO_RQD_CAUSE_RXLEV_UL_IH , IPAC_HO_RQD_CAUSE_RXLEV_DL_IH , IPAC_HO_RQD_CAUSE_MAX_MS_RANGE , IPAC_HO_RQD_CAUSE_POWER_BUDGET , IPAC_HO_RQD_CAUSE_ENQUIRY , IPAC_HO_RQD_CAUSE_ENQUIRY_FAILED , IPAC_HO_RQD_CAUSE_NORMAL3G , IPAC_HO_RQD_CAUSE_EMERGENCY3G , IPAC_HO_RQD_CAUSE_SERVICE_PREFERRED3G , IPAC_HO_RQD_CAUSE_O_M_SHUTDOWN , IPAC_HO_RQD_CAUSE_QUALITY_PROMOTION , IPAC_HO_RQD_CAUSE_LOAD_PROMOTION , IPAC_HO_RQD_CAUSE_LOAD_DEMOTION , IPAC_HO_RQD_CAUSE_MAX }
enum | rsl_cmod_spd { RSL_CMOD_SPD_SPEECH = 0x01 , RSL_CMOD_SPD_DATA = 0x02 , RSL_CMOD_SPD_SIGN = 0x03 }
enum | rsl_cmod_crt { RSL_CMOD_CRT_SDCCH = 0x01 , RSL_CMOD_CRT_TCH_Bm = 0x08 , RSL_CMOD_CRT_TCH_Lm = 0x09 , RSL_CMOD_CRT_TCH_BI_Bm = 0x0a , RSL_CMOD_CRT_TCH_UNI_Bm = 0x1a , RSL_CMOD_CRT_TCH_GROUP_Bm = 0x18 , RSL_CMOD_CRT_TCH_GROUP_Lm = 0x19 , RSL_CMOD_CRT_TCH_BCAST_Bm = 0x28 , RSL_CMOD_CRT_TCH_BCAST_Lm = 0x29 , RSL_CMOD_CRT_OSMO_TCH_VAMOS_Bm = 0x88 , RSL_CMOD_CRT_OSMO_TCH_VAMOS_Lm = 0x89 }
| Channel rate and type. More...
enum | rsl_cmod_sp { RSL_CMOD_SP_GSM1 = 0x01 , RSL_CMOD_SP_GSM2 = 0x11 , RSL_CMOD_SP_GSM3 = 0x21 , RSL_CMOD_SP_GSM4 = 0x31 , RSL_CMOD_SP_GSM5 = 0x09 , RSL_CMOD_SP_GSM6 = 0x0d }
| Speech. More...
enum | rsl_cmod_csd_nt { RSL_CMOD_CSD_NTA_43k5_14k5 = 0x61 , RSL_CMOD_CSD_NTA_29k0_14k5 = 0x62 , RSL_CMOD_CSD_NTA_43k5_29k0 = 0x63 , RSL_CMOD_CSD_NTA_14k5_43k5 = 0x69 , RSL_CMOD_CSD_NTA_14k5_29k0 = 0x6a , RSL_CMOD_CSD_NTA_29k0_43k5 = 0x6b , RSL_CMOD_CSD_NT_43k5 = 0x74 , RSL_CMOD_CSD_NT_28k8 = 0x71 , RSL_CMOD_CSD_NT_14k5 = 0x58 , RSL_CMOD_CSD_NT_12k0 = 0x50 , RSL_CMOD_CSD_NT_6k0 = 0x51 }
| Non-transparent data. More...
enum | rsl_cmod_csd_t { RSL_CMOD_CSD_T_32k0 = 0x38 , RSL_CMOD_CSD_T_29k0 = 0x39 , RSL_CMOD_CSD_T_14k4 = 0x18 , RSL_CMOD_CSD_T_9k6 = 0x10 , RSL_CMOD_CSD_T_4k8 = 0x11 , RSL_CMOD_CSD_T_2k4 = 0x12 , RSL_CMOD_CSD_T_1k2 = 0x13 , RSL_CMOD_CSD_T_600 = 0x14 , RSL_CMOD_CSD_T_1200_75 = 0x15 }
| Transparent data. More...
enum | rsl_ipac_rtp_payload { RSL_IPAC_RTP_GSM = 1 , RSL_IPAC_RTP_EFR , RSL_IPAC_RTP_AMR , RSL_IPAC_RTP_CSD , RSL_IPAC_RTP_MUX }
enum | rsl_ipac_speech_mode_s { RSL_IPAC_SPEECH_GSM_FR = 0 , RSL_IPAC_SPEECH_GSM_EFR = 1 , RSL_IPAC_SPEECH_GSM_AMR_FR = 2 , RSL_IPAC_SPEECH_GSM_HR = 3 , RSL_IPAC_SPEECH_GSM_AMR_HR = 5 , RSL_IPAC_SPEECH_AS_RTP = 0xf }
enum | rsl_ipac_speech_mode_m { RSL_IPAC_SPEECH_M_RXTX = 0 , RSL_IPAC_SPEECH_M_RX = 1 , RSL_IPAC_SPEECH_M_TX = 2 }
enum | rsl_ipac_rtp_csd_format_d { RSL_IPAC_RTP_CSD_EXT_TRAU = 0 , RSL_IPAC_RTP_CSD_NON_TRAU = 1 , RSL_IPAC_RTP_CSD_TRAU_BTS = 2 , RSL_IPAC_RTP_CSD_IWF_FREE = 3 }
enum | rsl_ipac_rtp_csd_format_ir { RSL_IPAC_RTP_CSD_IR_8k = 0 , RSL_IPAC_RTP_CSD_IR_16k = 1 , RSL_IPAC_RTP_CSD_IR_32k = 2 , RSL_IPAC_RTP_CSD_IR_64k = 3 }
enum | rsl_mrpci_pwrclass { RSL_MRPCI_PWRC_1 = 0 , RSL_MRPCI_PWRC_2 = 1 , RSL_MRPCI_PWRC_3 = 2 , RSL_MRPCI_PWRC_4 = 3 , RSL_MRPCI_PWRC_5 = 4 }
enum | rsl_mrpci_phase { RSL_MRPCI_PHASE_1 = 0 , RSL_MRPCI_PHASE_2 = 2 , RSL_MRPCI_PHASE_2PLUS = 3 }
enum | rsl_rel_mode { RSL_REL_NORMAL = 0 , RSL_REL_LOCAL_END = 1 }
enum | rsl_ipac_embedded_ie { RSL_IPAC_EIE_RXLEV = 0x00 , RSL_IPAC_EIE_RXQUAL = 0x01 , RSL_IPAC_EIE_FREQ_ERR = 0x02 , RSL_IPAC_EIE_TIMING_ERR = 0x03 , RSL_IPAC_EIE_MEAS_AVG_CFG = 0x04 , RSL_IPAC_EIE_BS_PWR_CTL = 0x05 , RSL_IPAC_EIE_MS_PWR_CTL = 0x06 , RSL_IPAC_EIE_HANDO_THRESH = 0x07 , RSL_IPAC_EIE_NCELL_DEFAULTS = 0x08 , RSL_IPAC_EIE_NCELL_LIST = 0x09 , RSL_IPAC_EIE_PC_THRESH_COMP = 0x0a , RSL_IPAC_EIE_HO_THRESH_COMP = 0x0b , RSL_IPAC_EIE_HO_CAUSE = 0x0c , RSL_IPAC_EIE_HO_CANDIDATES = 0x0d , RSL_IPAC_EIE_NCELL_BA_CHG_LIST = 0x0e , RSL_IPAC_EIE_NUM_OF_MS = 0x10 , RSL_IPAC_EIE_HO_CAND_EXT = 0x11 , RSL_IPAC_EIE_NCELL_DEF_EXT = 0x12 , RSL_IPAC_EIE_NCELL_LIST_EXT = 0x13 , RSL_IPAC_EIE_MASTER_KEY = 0x14 , RSL_IPAC_EIE_MASTER_SALT = 0x15 , RSL_IPAC_EIE_MEAS_TRANS_RES = 0x16 , RSL_IPAC_EIE_3G_HO_PARAM = 0x17 , RSL_IPAC_EIE_3G_NCELL_LIST = 0x18 , RSL_IPAC_EIE_SDCCH_CTL_PARAM = 0x1a , RSL_IPAC_EIE_AMR_CONV_THRESH = 0x1b , RSL_IPAC_EIE_OSMO_MEAS_AVG_CFG = 0xf0 , RSL_IPAC_EIE_OSMO_MS_PWR_CTL = 0xf1 , RSL_IPAC_EIE_OSMO_PC_THRESH_COMP = 0xf2 }
| ip.access specific embedded information elements More...

## Functions
union abis_rsl_chan_nr | __attribute__ ((packed))
void | rsl_init_rll_hdr (struct abis_rsl_rll_hdr *dh, uint8_t msg_type)
| Initialize a RSL RLL header. More...
void | rsl_init_cchan_hdr (struct abis_rsl_cchan_hdr *ch, uint8_t msg_type)
| Initialize a RSL Common Channel header. More...
uint8_t | rsl_enc_chan_nr (uint8_t type, uint8_t subch, uint8_t timeslot)
| Encode channel number as per Section 9.3.1. More...
int | rsl_dec_chan_nr (uint8_t chan_nr, uint8_t *type, uint8_t *subch, uint8_t *timeslot)
| Decode RSL channel number. More...
char * | rsl_chan_nr_str_buf (char *buf, size_t buf_len, uint8_t chan_nr)
| Get human-readable string for RSL channel number, in caller-provided buffer. More...
const char * | rsl_chan_nr_str (uint8_t chan_nr)
| Get human-readable string for RSL channel number, in static buffer. More...
char * | rsl_chan_nr_str_c (const void *ctx, uint8_t chan_nr)
| Get human-readable string for RSL channel number, in dynamically-allocated buffer. More...
const char * | rsl_err_name (uint8_t err)
| Get human-readable name for RSL Error. More...
const char * | rsl_rlm_cause_name (uint8_t err)
| Get human-readable string for RLM cause. More...
const char * | rsl_msg_name (uint8_t msg_type)
| Get human-readable string for RSL Message Type. More...
const char * | rsl_ipac_msg_name (uint8_t msg_type)
| Get human-readable name of ip.access RSL msg type. More...
const char * | rsl_or_ipac_msg_name (uint8_t msg_type)
| Get human-readable name of standard or ip.access RSL msg type. More...
int | rsl_ccch_conf_to_bs_cc_chans (int ccch_conf)
void | rsl_rll_push_hdr (struct msgb *msg, uint8_t msg_type, uint8_t chan_nr, uint8_t link_id, int transparent)
| Push a RSL RLL header onto an existing msgb. More...
void | rsl_rll_push_l3 (struct msgb *msg, uint8_t msg_type, uint8_t chan_nr, uint8_t link_id, int transparent)
| Wrap msgb in L3 Info IE and push a RSL RLL header. More...
struct msgb * | rsl_rll_simple (uint8_t msg_type, uint8_t chan_nr, uint8_t link_id, int transparent)
| Create msgb with RSL RLL header. More...
static const char * | rsl_act_type_name (uint8_t act_type)
| Return a human readable name for GSM 08.58 RSL_ACT_* constants. More...
int | rsl_ccch_conf_to_bs_ccch_sdcch_comb (int ccch_conf)

## Variables
enum abis_rsl_msgtype | __attribute__
const struct tlv_definition | rsl_att_tlvdef
const struct tlv_definition | rsl_ipac_eie_tlvdef
| TLV parser definitions for IPA embedded IEs. More...
const struct value_string | rsl_act_type_names []
| String names of RSL Channel Activation Types. More...
const struct tlv_definition | rsl_att_tlvdef
static const struct value_string | rsl_err_vals []
static const struct value_string | rsl_msgt_names []
static const struct value_string | rsl_ipac_msgt_names []
| ip.access specific More...
static const struct value_string | rsl_rlm_cause_strs []
const struct tlv_definition | rsl_ipac_eie_tlvdef
| TLV parser definitions for IPA embedded IEs. More...
const struct value_string | rsl_act_type_names []
| String names of RSL Channel Activation Types. More...

## Detailed Description

GSM Radio Signalling Link messages on the A-bis interface.

3GPP TS 08.58 version 8.6.0 Release 1999 / ETSI TS 100 596 V8.6.0.

## Macro Definition Documentation

## ◆ ABIS_RSL_CHAN_NR_CBITS_BCCH

#define ABIS_RSL_CHAN_NR_CBITS_BCCH 0x10

## ◆ ABIS_RSL_CHAN_NR_CBITS_Bm_ACCHs

#define ABIS_RSL_CHAN_NR_CBITS_Bm_ACCHs 0x01

## ◆ ABIS_RSL_CHAN_NR_CBITS_Lm_ACCHs

#define ABIS_RSL_CHAN_NR_CBITS_Lm_ACCHs | ( |  | ss | ) | (0x02 + (ss))

## ◆ ABIS_RSL_CHAN_NR_CBITS_OSMO_CBCH4

#define ABIS_RSL_CHAN_NR_CBITS_OSMO_CBCH4 0x19 /*< non-standard, for CBCH/SDCCH4 */

## ◆ ABIS_RSL_CHAN_NR_CBITS_OSMO_CBCH8

#define ABIS_RSL_CHAN_NR_CBITS_OSMO_CBCH8 0x1a /*< non-standard, for CBCH/SDCCH8 */

## ◆ ABIS_RSL_CHAN_NR_CBITS_OSMO_PDCH

#define ABIS_RSL_CHAN_NR_CBITS_OSMO_PDCH 0x18 /*< non-standard, for dyn TS */

## ◆ ABIS_RSL_CHAN_NR_CBITS_OSMO_VAMOS_Bm_ACCHs

#define ABIS_RSL_CHAN_NR_CBITS_OSMO_VAMOS_Bm_ACCHs 0x1d /*< VAMOS TCH/F */

## ◆ ABIS_RSL_CHAN_NR_CBITS_OSMO_VAMOS_Lm_ACCHs

#define ABIS_RSL_CHAN_NR_CBITS_OSMO_VAMOS_Lm_ACCHs | ( |  | ss | ) | (0x1e + (ss)) /*< VAMOS TCH/H */

## ◆ ABIS_RSL_CHAN_NR_CBITS_PCH_AGCH

#define ABIS_RSL_CHAN_NR_CBITS_PCH_AGCH 0x12

## ◆ ABIS_RSL_CHAN_NR_CBITS_RACH

#define ABIS_RSL_CHAN_NR_CBITS_RACH 0x11

## ◆ ABIS_RSL_CHAN_NR_CBITS_SDCCH4_ACCH

#define ABIS_RSL_CHAN_NR_CBITS_SDCCH4_ACCH | ( |  | ss | ) | (0x04 + (ss))

## ◆ ABIS_RSL_CHAN_NR_CBITS_SDCCH8_ACCH

#define ABIS_RSL_CHAN_NR_CBITS_SDCCH8_ACCH | ( |  | ss | ) | (0x08 + (ss))

## ◆ ABIS_RSL_LINK_ID_CBITS_FACCH_SDCCH

#define ABIS_RSL_LINK_ID_CBITS_FACCH_SDCCH 0x00

## ◆ ABIS_RSL_LINK_ID_CBITS_SACCH

#define ABIS_RSL_LINK_ID_CBITS_SACCH 0x01

## ◆ ABIS_RSL_MDISC_COM_CHAN

#define ABIS_RSL_MDISC_COM_CHAN 0x0c

## ◆ ABIS_RSL_MDISC_DED_CHAN

#define ABIS_RSL_MDISC_DED_CHAN 0x08

## ◆ ABIS_RSL_MDISC_IPACCESS

#define ABIS_RSL_MDISC_IPACCESS 0x7e

## ◆ ABIS_RSL_MDISC_IS_TRANSP

#define ABIS_RSL_MDISC_IS_TRANSP | ( |  | x | ) | (x & 0x01)

## ◆ ABIS_RSL_MDISC_LOC

#define ABIS_RSL_MDISC_LOC 0x20

## ◆ ABIS_RSL_MDISC_RLL

#define ABIS_RSL_MDISC_RLL 0x02

## ◆ ABIS_RSL_MDISC_TRANSP

#define ABIS_RSL_MDISC_TRANSP 0x01

## ◆ ABIS_RSL_MDISC_TRX

#define ABIS_RSL_MDISC_TRX 0x10

## ◆ RLL_CAUSE_FRM_UNIMPL

#define RLL_CAUSE_FRM_UNIMPL 0x0c

## ◆ RLL_CAUSE_IFRM_INC_LEN

#define RLL_CAUSE_IFRM_INC_LEN 0x0b

## ◆ RLL_CAUSE_IFRM_INC_MBITS

#define RLL_CAUSE_IFRM_INC_MBITS 0x0a

## ◆ RLL_CAUSE_REEST_REQ

#define RLL_CAUSE_REEST_REQ 0x02

## ◆ RLL_CAUSE_SABM_INFO_NOTALL

#define RLL_CAUSE_SABM_INFO_NOTALL 0x0e

## ◆ RLL_CAUSE_SABM_MF

#define RLL_CAUSE_SABM_MF 0x0d

## ◆ RLL_CAUSE_SEQ_ERR

#define RLL_CAUSE_SEQ_ERR 0x07

## ◆ RLL_CAUSE_SFRM_INC_PARAM

#define RLL_CAUSE_SFRM_INC_PARAM 0x09

## ◆ RLL_CAUSE_T200_EXPIRED

#define RLL_CAUSE_T200_EXPIRED 0x01

## ◆ RLL_CAUSE_UFRM_INC_PARAM

#define RLL_CAUSE_UFRM_INC_PARAM 0x08

## ◆ RLL_CAUSE_UNSOL_DM_RESP

#define RLL_CAUSE_UNSOL_DM_RESP 0x04

## ◆ RLL_CAUSE_UNSOL_DM_RESP_MF

#define RLL_CAUSE_UNSOL_DM_RESP_MF 0x05

## ◆ RLL_CAUSE_UNSOL_SPRV_RESP

#define RLL_CAUSE_UNSOL_SPRV_RESP 0x06

## ◆ RLL_CAUSE_UNSOL_UA_RESP

#define RLL_CAUSE_UNSOL_UA_RESP 0x03

## ◆ RSL_ACT_INTER_ASYNC

#define RSL_ACT_INTER_ASYNC 0x02

## ◆ RSL_ACT_INTER_SYNC

#define RSL_ACT_INTER_SYNC 0x03

## ◆ RSL_ACT_INTRA_IMM_ASS

#define RSL_ACT_INTRA_IMM_ASS 0x00

## ◆ RSL_ACT_INTRA_NORM_ASS

#define RSL_ACT_INTRA_NORM_ASS 0x01

## ◆ RSL_ACT_OSMO_PDCH

#define RSL_ACT_OSMO_PDCH 0x0f /*< non-standard, for dyn TS */

## ◆ RSL_ACT_SECOND_ADD

#define RSL_ACT_SECOND_ADD 0x04

## ◆ RSL_ACT_SECOND_MULTI

#define RSL_ACT_SECOND_MULTI 0x05

## ◆ RSL_ACT_TYPE_INITIAL

#define RSL_ACT_TYPE_INITIAL 0x00

## ◆ RSL_ACT_TYPE_REACT

#define RSL_ACT_TYPE_REACT 0x80

## ◆ RSL_ALLOC_HEADROOM

#define RSL_ALLOC_HEADROOM 56

Headroom size for RSL msgb_alloc.

## ◆ RSL_ALLOC_SIZE

#define RSL_ALLOC_SIZE 200

Size for RSL msgb_alloc.

## ◆ RSL_BCCH_CCCH_CONF_1_C

#define RSL_BCCH_CCCH_CONF_1_C 0x01

## ◆ RSL_BCCH_CCCH_CONF_1_NC

#define RSL_BCCH_CCCH_CONF_1_NC 0x00

## ◆ RSL_BCCH_CCCH_CONF_2_NC

#define RSL_BCCH_CCCH_CONF_2_NC 0x02

## ◆ RSL_BCCH_CCCH_CONF_3_NC

#define RSL_BCCH_CCCH_CONF_3_NC 0x04

## ◆ RSL_BCCH_CCCH_CONF_4_NC

#define RSL_BCCH_CCCH_CONF_4_NC 0x06

## ◆ RSL_BS_PA_MFRMS_2

#define RSL_BS_PA_MFRMS_2 0x00

## ◆ RSL_BS_PA_MFRMS_3

#define RSL_BS_PA_MFRMS_3 0x01

## ◆ RSL_BS_PA_MFRMS_4

#define RSL_BS_PA_MFRMS_4 0x02

## ◆ RSL_BS_PA_MFRMS_5

#define RSL_BS_PA_MFRMS_5 0x03

## ◆ RSL_BS_PA_MFRMS_6

#define RSL_BS_PA_MFRMS_6 0x04

## ◆ RSL_BS_PA_MFRMS_7

#define RSL_BS_PA_MFRMS_7 0x05

## ◆ RSL_BS_PA_MFRMS_8

#define RSL_BS_PA_MFRMS_8 0x06

## ◆ RSL_BS_PA_MFRMS_9

#define RSL_BS_PA_MFRMS_9 0x07

## ◆ RSL_CB_CMD_DEFBCAST_NORMAL

#define RSL_CB_CMD_DEFBCAST_NORMAL 0

## ◆ RSL_CB_CMD_DEFBCAST_NULL

#define RSL_CB_CMD_DEFBCAST_NULL 1

## ◆ RSL_CB_CMD_LASTBLOCK_1

#define RSL_CB_CMD_LASTBLOCK_1 1

## ◆ RSL_CB_CMD_LASTBLOCK_2

#define RSL_CB_CMD_LASTBLOCK_2 2

## ◆ RSL_CB_CMD_LASTBLOCK_3

#define RSL_CB_CMD_LASTBLOCK_3 3

## ◆ RSL_CB_CMD_LASTBLOCK_4

#define RSL_CB_CMD_LASTBLOCK_4 0

## ◆ RSL_CB_CMD_TYPE_DEFAULT

#define RSL_CB_CMD_TYPE_DEFAULT 0x0e

## ◆ RSL_CB_CMD_TYPE_NORMAL

#define RSL_CB_CMD_TYPE_NORMAL 0x00

## ◆ RSL_CB_CMD_TYPE_NULL

#define RSL_CB_CMD_TYPE_NULL 0x0f

## ◆ RSL_CB_CMD_TYPE_SCHEDULE

#define RSL_CB_CMD_TYPE_SCHEDULE 0x08

## ◆ RSL_CHAN_BCCH

#define RSL_CHAN_BCCH 0x80

## ◆ RSL_CHAN_Bm_ACCHs

#define RSL_CHAN_Bm_ACCHs 0x08

## ◆ RSL_CHAN_Lm_ACCHs

#define RSL_CHAN_Lm_ACCHs 0x10 /* .. 0x18 */

## ◆ RSL_CHAN_NR_1

#define RSL_CHAN_NR_1 0x08 /*< bit to add for 2nd,... lchan */

## ◆ RSL_CHAN_NR_MASK

#define RSL_CHAN_NR_MASK 0xf8

## ◆ RSL_CHAN_OSMO_CBCH4

#define RSL_CHAN_OSMO_CBCH4 0xc8 /*< non-standard, for CBCH/SDCCH4 */

## ◆ RSL_CHAN_OSMO_CBCH8

#define RSL_CHAN_OSMO_CBCH8 0xd0 /*< non-standard, for CBCH/SDCCH8 */

## ◆ RSL_CHAN_OSMO_PDCH

#define RSL_CHAN_OSMO_PDCH 0xc0 /*< non-standard, for dyn TS */

## ◆ RSL_CHAN_OSMO_VAMOS_Bm_ACCHs

#define RSL_CHAN_OSMO_VAMOS_Bm_ACCHs 0xe8 /* VAMOS TCH/F */

## ◆ RSL_CHAN_OSMO_VAMOS_Lm_ACCHs

#define RSL_CHAN_OSMO_VAMOS_Lm_ACCHs 0xf0 /* VAMOS TCH/H */

## ◆ RSL_CHAN_OSMO_VAMOS_MASK

#define RSL_CHAN_OSMO_VAMOS_MASK 0xe0 /* VAMOS TCH/{F,H} */

## ◆ RSL_CHAN_PCH_AGCH

#define RSL_CHAN_PCH_AGCH 0x90

## ◆ RSL_CHAN_RACH

#define RSL_CHAN_RACH 0x88

## ◆ RSL_CHAN_SDCCH4_ACCH

#define RSL_CHAN_SDCCH4_ACCH 0x20 /* .. 0x38 */

## ◆ RSL_CHAN_SDCCH8_ACCH

#define RSL_CHAN_SDCCH8_ACCH 0x40 /* ...0x78 */

## ◆ RSL_CHANNEED_ANY

#define RSL_CHANNEED_ANY 0x00

## ◆ RSL_CHANNEED_SDCCH

#define RSL_CHANNEED_SDCCH 0x01

## ◆ RSL_CHANNEED_TCH_F

#define RSL_CHANNEED_TCH_F 0x02

## ◆ RSL_CHANNEED_TCH_ForH

#define RSL_CHANNEED_TCH_ForH 0x03

## ◆ RSL_CMD_INDICATOR_START

#define RSL_CMD_INDICATOR_START 0x00

Command Indicator (Chapter 9.3.48)

## ◆ RSL_CMD_INDICATOR_STOP

#define RSL_CMD_INDICATOR_STOP 0x01

## ◆ RSL_CMOD_CSD_T_1200

#define RSL_CMOD_CSD_T_1200 RSL_CMOD_CSD_T_1k2

## ◆ RSL_CMOD_CSD_T_14400

#define RSL_CMOD_CSD_T_14400 RSL_CMOD_CSD_T_14k4

## ◆ RSL_CMOD_CSD_T_2400

#define RSL_CMOD_CSD_T_2400 RSL_CMOD_CSD_T_2k4

## ◆ RSL_CMOD_CSD_T_29000

#define RSL_CMOD_CSD_T_29000 RSL_CMOD_CSD_T_29k0

## ◆ RSL_CMOD_CSD_T_32000

#define RSL_CMOD_CSD_T_32000 RSL_CMOD_CSD_T_32k0

## ◆ RSL_CMOD_CSD_T_4800

#define RSL_CMOD_CSD_T_4800 RSL_CMOD_CSD_T_4k8

## ◆ RSL_CMOD_CSD_T_9600

#define RSL_CMOD_CSD_T_9600 RSL_CMOD_CSD_T_9k6

## ◆ RSL_CMOD_DTXd

#define RSL_CMOD_DTXd 0x02 /* downlink */

## ◆ RSL_CMOD_DTXu

#define RSL_CMOD_DTXu 0x01 /* uplink */

## ◆ RSL_CMOD_SP_NT_12k0

#define RSL_CMOD_SP_NT_12k0 RSL_CMOD_CSD_NT_12k0

## ◆ RSL_CMOD_SP_NT_14k5

#define RSL_CMOD_SP_NT_14k5 RSL_CMOD_CSD_NT_14k5

## ◆ RSL_CMOD_SP_NT_6k0

#define RSL_CMOD_SP_NT_6k0 RSL_CMOD_CSD_NT_6k0

## ◆ RSL_ERIC_SYSTEM_INFO_13

#define RSL_ERIC_SYSTEM_INFO_13 0x0C

## ◆ RSL_ERR_ACCH_OVERLOAD

#define RSL_ERR_ACCH_OVERLOAD 0x24

## ◆ RSL_ERR_BTS_NOT_EQUIPPED

#define RSL_ERR_BTS_NOT_EQUIPPED 0x27

## ◆ RSL_ERR_CCCH_OVERLOAD

#define RSL_ERR_CCCH_OVERLOAD 0x23

## ◆ RSL_ERR_ENCR_UNIMPL

#define RSL_ERR_ENCR_UNIMPL 0x40

## ◆ RSL_ERR_EQUIPMENT_FAIL

#define RSL_ERR_EQUIPMENT_FAIL 0x20

## ◆ RSL_ERR_HANDOVER_ACC_FAIL

#define RSL_ERR_HANDOVER_ACC_FAIL 0x02

## ◆ RSL_ERR_IE_CONTENT

#define RSL_ERR_IE_CONTENT 0x68

## ◆ RSL_ERR_IE_ERROR

#define RSL_ERR_IE_ERROR 0x63

## ◆ RSL_ERR_IE_LENGTH

#define RSL_ERR_IE_LENGTH 0x67

## ◆ RSL_ERR_IE_NONEXIST

#define RSL_ERR_IE_NONEXIST 0x66

## ◆ RSL_ERR_INTERWORKING

#define RSL_ERR_INTERWORKING 0x7f

## ◆ RSL_ERR_INVALID_MESSAGE

#define RSL_ERR_INVALID_MESSAGE 0x5f

## ◆ RSL_ERR_MAND_IE_ERROR

#define RSL_ERR_MAND_IE_ERROR 0x64

## ◆ RSL_ERR_MSG_DISCR

#define RSL_ERR_MSG_DISCR 0x60

## ◆ RSL_ERR_MSG_SEQ

#define RSL_ERR_MSG_SEQ 0x62

## ◆ RSL_ERR_MSG_TYPE

#define RSL_ERR_MSG_TYPE 0x61

## ◆ RSL_ERR_NORMAL_UNSPEC

#define RSL_ERR_NORMAL_UNSPEC 0x0f

## ◆ RSL_ERR_NOTIFICATION_OVERFL

#define RSL_ERR_NOTIFICATION_OVERFL 0x29

## ◆ RSL_ERR_OM_INTERVENTION

#define RSL_ERR_OM_INTERVENTION 0x07

## ◆ RSL_ERR_OPT_IE_ERROR

#define RSL_ERR_OPT_IE_ERROR 0x65

## ◆ RSL_ERR_PROCESSOR_OVERLOAD

#define RSL_ERR_PROCESSOR_OVERLOAD 0x25

## ◆ RSL_ERR_PROTO

#define RSL_ERR_PROTO 0x6f

## ◆ RSL_ERR_RADIO_IF_FAIL

#define RSL_ERR_RADIO_IF_FAIL 0x00

## ◆ RSL_ERR_RADIO_LINK_FAIL

#define RSL_ERR_RADIO_LINK_FAIL 0x01

## ◆ RSL_ERR_RCH_ALR_ACTV_ALLOC

#define RSL_ERR_RCH_ALR_ACTV_ALLOC 0x50

## ◆ RSL_ERR_REMOTE_TRANSC_FAIL

#define RSL_ERR_REMOTE_TRANSC_FAIL 0x28

## ◆ RSL_ERR_RES_UNAVAIL

#define RSL_ERR_RES_UNAVAIL 0x2f

## ◆ RSL_ERR_RR_UNAVAIL

#define RSL_ERR_RR_UNAVAIL 0x21

## ◆ RSL_ERR_SERV_OPT_UNAVAIL

#define RSL_ERR_SERV_OPT_UNAVAIL 0x3f

## ◆ RSL_ERR_SERV_OPT_UNIMPL

#define RSL_ERR_SERV_OPT_UNIMPL 0x4f

## ◆ RSL_ERR_T_MSRFPCI_EXP

#define RSL_ERR_T_MSRFPCI_EXP 0x18

## ◆ RSL_ERR_TALKER_ACC_FAIL

#define RSL_ERR_TALKER_ACC_FAIL 0x03

## ◆ RSL_ERR_TERR_CH_FAIL

#define RSL_ERR_TERR_CH_FAIL 0x22

## ◆ RSL_ERR_TRANSC_UNAVAIL

#define RSL_ERR_TRANSC_UNAVAIL 0x30

## ◆ RSL_ERRCLS_INTERWORKING

#define RSL_ERRCLS_INTERWORKING 0x70

## ◆ RSL_ERRCLS_INVAL_MSG

#define RSL_ERRCLS_INVAL_MSG 0x50

## ◆ RSL_ERRCLS_NORMAL

#define RSL_ERRCLS_NORMAL 0x00

## ◆ RSL_ERRCLS_PROTO_ERROR

#define RSL_ERRCLS_PROTO_ERROR 0x60

## ◆ RSL_ERRCLS_RESOURCE_UNAVAIL

#define RSL_ERRCLS_RESOURCE_UNAVAIL 0x20

## ◆ RSL_ERRCLS_SERVICE_UNAVAIL

#define RSL_ERRCLS_SERVICE_UNAVAIL 0x30

## ◆ RSL_ERRCLS_SERVICE_UNIMPL

#define RSL_ERRCLS_SERVICE_UNIMPL 0x40

## ◆ RSL_EXT_MEAS_ORDER

#define RSL_EXT_MEAS_ORDER 0x47

## ◆ RSL_IE_ERIC_ACTIVATE_FLAG

#define RSL_IE_ERIC_ACTIVATE_FLAG 0xfe

## ◆ RSL_IE_ERIC_BCCH_MAPPING

#define RSL_IE_ERIC_BCCH_MAPPING 0xf2

## ◆ RSL_IE_ERIC_CNTR_CTRL

#define RSL_IE_ERIC_CNTR_CTRL 0xf4

## ◆ RSL_IE_ERIC_CNTR_CTRL_ACK

#define RSL_IE_ERIC_CNTR_CTRL_ACK 0xf5

## ◆ RSL_IE_ERIC_CNTR_REPORT

#define RSL_IE_ERIC_CNTR_REPORT 0xf6

## ◆ RSL_IE_ERIC_EGPRS_REQ_REF

#define RSL_IE_ERIC_EGPRS_REQ_REF 0xf9

## ◆ RSL_IE_ERIC_EMR_SUPPORT

#define RSL_IE_ERIC_EMR_SUPPORT 0xf8

## ◆ RSL_IE_ERIC_FULL_NCH_INFO

#define RSL_IE_ERIC_FULL_NCH_INFO 0xff

## ◆ RSL_IE_ERIC_ICP_CONN

#define RSL_IE_ERIC_ICP_CONN 0xf7

## ◆ RSL_IE_ERIC_INST_NR

#define RSL_IE_ERIC_INST_NR 0x48

## ◆ RSL_IE_ERIC_MOBILE_ID

#define RSL_IE_ERIC_MOBILE_ID 0xf1

## ◆ RSL_IE_ERIC_NY2

#define RSL_IE_ERIC_NY2 0xfc

## ◆ RSL_IE_ERIC_PACKET_PAG_IND

#define RSL_IE_ERIC_PACKET_PAG_IND 0xf3

## ◆ RSL_IE_ERIC_PAGING_GROUP

#define RSL_IE_ERIC_PAGING_GROUP 0x0e

## ◆ RSL_IE_ERIC_PGSL_TIMERS

#define RSL_IE_ERIC_PGSL_TIMERS 0x49

## ◆ RSL_IE_ERIC_POWER_INFO

#define RSL_IE_ERIC_POWER_INFO 0xf0

## ◆ RSL_IE_ERIC_REP_PER_NCH

#define RSL_IE_ERIC_REP_PER_NCH 0xfb

## ◆ RSL_IE_ERIC_REPEAT_DL_FACCH

#define RSL_IE_ERIC_REPEAT_DL_FACCH 0x4a

## ◆ RSL_IE_ERIC_T3115

#define RSL_IE_ERIC_T3115 0xfd

## ◆ RSL_IE_ERIC_VGCS_REL

#define RSL_IE_ERIC_VGCS_REL 0xfa

## ◆ rsl_ipac_eie_tlv_parse

#define rsl_ipac_eie_tlv_parse | ( |  | dec,
|  |  | buf,
|  |  | len
| ) |  | tlv_parse(dec, &rsl_ipac_eie_tlvdef, buf, len, 0, 0)

Parse RSL IPAC EIE TLV structure using tlv_parse.

## ◆ RSL_MEAS_INFO

#define RSL_MEAS_INFO 0x48

## ◆ RSL_SYSTEM_INFO_1

#define RSL_SYSTEM_INFO_1 0x01

## ◆ RSL_SYSTEM_INFO_10

#define RSL_SYSTEM_INFO_10 0x0f

## ◆ RSL_SYSTEM_INFO_13

#define RSL_SYSTEM_INFO_13 0x28

## ◆ RSL_SYSTEM_INFO_16

#define RSL_SYSTEM_INFO_16 0x08

## ◆ RSL_SYSTEM_INFO_17

#define RSL_SYSTEM_INFO_17 0x09

## ◆ RSL_SYSTEM_INFO_18

#define RSL_SYSTEM_INFO_18 0x2b

## ◆ RSL_SYSTEM_INFO_19

#define RSL_SYSTEM_INFO_19 0x2c

## ◆ RSL_SYSTEM_INFO_2

#define RSL_SYSTEM_INFO_2 0x02

## ◆ RSL_SYSTEM_INFO_20

#define RSL_SYSTEM_INFO_20 0x2d

## ◆ RSL_SYSTEM_INFO_2bis

#define RSL_SYSTEM_INFO_2bis 0x0a

## ◆ RSL_SYSTEM_INFO_2quater

#define RSL_SYSTEM_INFO_2quater 0x29

## ◆ RSL_SYSTEM_INFO_2ter

#define RSL_SYSTEM_INFO_2ter 0x0b

## ◆ RSL_SYSTEM_INFO_3

#define RSL_SYSTEM_INFO_3 0x03

## ◆ RSL_SYSTEM_INFO_4

#define RSL_SYSTEM_INFO_4 0x04

## ◆ RSL_SYSTEM_INFO_5

#define RSL_SYSTEM_INFO_5 0x05

## ◆ RSL_SYSTEM_INFO_5bis

#define RSL_SYSTEM_INFO_5bis 0x0d

## ◆ RSL_SYSTEM_INFO_5ter

#define RSL_SYSTEM_INFO_5ter 0x0e

## ◆ RSL_SYSTEM_INFO_6

#define RSL_SYSTEM_INFO_6 0x06

## ◆ RSL_SYSTEM_INFO_7

#define RSL_SYSTEM_INFO_7 0x07

## ◆ RSL_SYSTEM_INFO_8

#define RSL_SYSTEM_INFO_8 0x00

## ◆ RSL_SYSTEM_INFO_9

#define RSL_SYSTEM_INFO_9 0x2a

## ◆ rsl_tlv_parse

#define rsl_tlv_parse | ( |  | dec,
|  |  | buf,
|  |  | len
| ) |  | tlv_parse(dec, &rsl_att_tlvdef, buf, len, 0, 0)

Parse RSL TLV structure using tlv_parse.

## Enumeration Type Documentation

## ◆ anonymous enum

anonymous enum

Enumerator
IPAC_UNWEIGHTED_AVE |
IPAC_WEIGHTED_AVE |
IPAC_MEDIAN_AVE |
IPAC_OSMO_EWMA_AVE |

## ◆ anonymous enum

anonymous enum

Enumerator
IPAC_RXLEV_AVE |
IPAC_RXQUAL_AVE |
IPAC_MS_BTS_DIS_AVE |

## ◆ anonymous enum

anonymous enum

Enumerator
IPAC_HO_RQD_CAUSE_L_RXLEV_UL_H |
IPAC_HO_RQD_CAUSE_L_RXLEV_DL_H |
IPAC_HO_RQD_CAUSE_L_RXQUAL_UL_H |
IPAC_HO_RQD_CAUSE_L_RXQUAL_DL_H |
IPAC_HO_RQD_CAUSE_RXLEV_UL_IH |
IPAC_HO_RQD_CAUSE_RXLEV_DL_IH |
IPAC_HO_RQD_CAUSE_MAX_MS_RANGE |
IPAC_HO_RQD_CAUSE_POWER_BUDGET |
IPAC_HO_RQD_CAUSE_ENQUIRY |
IPAC_HO_RQD_CAUSE_ENQUIRY_FAILED |
IPAC_HO_RQD_CAUSE_NORMAL3G |
IPAC_HO_RQD_CAUSE_EMERGENCY3G |
IPAC_HO_RQD_CAUSE_SERVICE_PREFERRED3G |
IPAC_HO_RQD_CAUSE_O_M_SHUTDOWN |
IPAC_HO_RQD_CAUSE_QUALITY_PROMOTION |
IPAC_HO_RQD_CAUSE_LOAD_PROMOTION |
IPAC_HO_RQD_CAUSE_LOAD_DEMOTION |
IPAC_HO_RQD_CAUSE_MAX |

## ◆ abis_rsl_ie

enum abis_rsl_ie

RSL Information Element Identifiers (Chapter 9.3)

Enumerator
RSL_IE_CHAN_NR |
RSL_IE_LINK_IDENT |
RSL_IE_ACT_TYPE |
RSL_IE_BS_POWER |
RSL_IE_CHAN_IDENT |
RSL_IE_CHAN_MODE |
RSL_IE_ENCR_INFO |
RSL_IE_FRAME_NUMBER |
RSL_IE_HANDO_REF |
RSL_IE_L1_INFO |
RSL_IE_L3_INFO |
RSL_IE_MS_IDENTITY |
RSL_IE_MS_POWER |
RSL_IE_PAGING_GROUP |
RSL_IE_PAGING_LOAD |
RSL_IE_PYHS_CONTEXT |
RSL_IE_ACCESS_DELAY |
RSL_IE_RACH_LOAD |
RSL_IE_REQ_REFERENCE |
RSL_IE_RELEASE_MODE |
RSL_IE_RESOURCE_INFO |
RSL_IE_RLM_CAUSE |
RSL_IE_STARTNG_TIME |
RSL_IE_TIMING_ADVANCE |
RSL_IE_UPLINK_MEAS |
RSL_IE_CAUSE |
RSL_IE_MEAS_RES_NR |
RSL_IE_MSG_ID |
RSL_IE_SYSINFO_TYPE |
RSL_IE_MS_POWER_PARAM |
RSL_IE_BS_POWER_PARAM |
RSL_IE_PREPROC_PARAM |
RSL_IE_PREPROC_MEAS |
RSL_IE_IMM_ASS_INFO |
RSL_IE_SMSCB_INFO |
RSL_IE_MS_TIMING_OFFSET |
RSL_IE_ERR_MSG |
RSL_IE_FULL_BCCH_INFO |
RSL_IE_CHAN_NEEDED |
RSL_IE_CB_CMD_TYPE |
RSL_IE_SMSCB_MSG |
RSL_IE_FULL_IMM_ASS_INFO |
RSL_IE_SACCH_INFO |
RSL_IE_CBCH_LOAD_INFO |
RSL_IE_SMSCB_CHAN_INDICATOR |
RSL_IE_GROUP_CALL_REF |
RSL_IE_CHAN_DESC |
RSL_IE_NCH_DRX_INFO |
RSL_IE_CMD_INDICATOR |
RSL_IE_EMLPP_PRIO |
RSL_IE_UIC |
RSL_IE_MAIN_CHAN_REF |
RSL_IE_MR_CONFIG |
RSL_IE_MR_CONTROL |
RSL_IE_SUP_CODEC_TYPES |
RSL_IE_CODEC_CONFIG |
RSL_IE_RTD |
RSL_IE_TFO_STATUS |
RSL_IE_LLP_APDU |
RSL_IE_TFO_XPAR_CONT |
RSL_IE_SIEMENS_MRPCI |
RSL_IE_SIEMENS_PREF_AREA_TYPE |
RSL_IE_SIEMENS_ININ_CELL_HO_PAR |
RSL_IE_SIEMENS_TRACE_REF_NR |
RSL_IE_SIEMENS_INT_TRACE_IDX |
RSL_IE_SIEMENS_L2_HDR_INFO |
RSL_IE_SIEMENS_HIGHEST_RATE |
RSL_IE_SIEMENS_SUGGESTED_RATE |
RSL_IE_OSMO_REP_ACCH_CAP |
RSL_IE_OSMO_TRAINING_SEQUENCE |
RSL_IE_OSMO_TEMP_OVP_ACCH_CAP |
RSL_IE_OSMO_OSMUX_CID |
RSL_IE_OSMO_RTP_EXTENSIONS |
RSL_IE_IPAC_SRTP_CONFIG |
RSL_IE_IPAC_PROXY_UDP |
RSL_IE_IPAC_BSCMPL_TOUT |
RSL_IE_IPAC_REMOTE_IP |
RSL_IE_IPAC_REMOTE_PORT |
RSL_IE_IPAC_RTP_PAYLOAD |
RSL_IE_IPAC_LOCAL_PORT |
RSL_IE_IPAC_SPEECH_MODE |
RSL_IE_IPAC_LOCAL_IP |
RSL_IE_IPAC_CONN_STAT |
RSL_IE_IPAC_HO_C_PARMS |
RSL_IE_IPAC_CONN_ID |
RSL_IE_IPAC_RTP_CSD_FMT |
RSL_IE_IPAC_RTP_JIT_BUF |
RSL_IE_IPAC_RTP_COMPR |
RSL_IE_IPAC_RTP_PAYLOAD2 |
RSL_IE_IPAC_RTP_MPLEX |
RSL_IE_IPAC_RTP_MPLEX_ID |

## ◆ abis_rsl_msgtype

enum abis_rsl_msgtype

Enumerator
RSL_MT_DATA_REQ |
RSL_MT_DATA_IND |
RSL_MT_ERROR_IND |
RSL_MT_EST_REQ |
RSL_MT_EST_CONF |
RSL_MT_EST_IND |
RSL_MT_REL_REQ |
RSL_MT_REL_CONF |
RSL_MT_REL_IND |
RSL_MT_UNIT_DATA_REQ |
RSL_MT_UNIT_DATA_IND |
RSL_MT_SUSP_REQ |
RSL_MT_SUSP_CONF |
RSL_MT_RES_REQ |
RSL_MT_RECON_REQ |
RSL_MT_BCCH_INFO |
RSL_MT_CCCH_LOAD_IND |
RSL_MT_CHAN_RQD |
RSL_MT_DELETE_IND |
RSL_MT_PAGING_CMD |
RSL_MT_IMMEDIATE_ASSIGN_CMD |
RSL_MT_SMS_BC_REQ |
RSL_MT_CHAN_CONF |
RSL_MT_RF_RES_IND |
RSL_MT_SACCH_FILL |
RSL_MT_OVERLOAD |
RSL_MT_ERROR_REPORT |
RSL_MT_SMS_BC_CMD |
RSL_MT_CBCH_LOAD_IND |
RSL_MT_NOT_CMD |
RSL_MT_CHAN_ACTIV |
RSL_MT_CHAN_ACTIV_ACK |
RSL_MT_CHAN_ACTIV_NACK |
RSL_MT_CONN_FAIL |
RSL_MT_DEACTIVATE_SACCH |
RSL_MT_ENCR_CMD |
RSL_MT_HANDO_DET |
RSL_MT_MEAS_RES |
RSL_MT_MODE_MODIFY_REQ |
RSL_MT_MODE_MODIFY_ACK |
RSL_MT_MODE_MODIFY_NACK |
RSL_MT_PHY_CONTEXT_REQ |
RSL_MT_PHY_CONTEXT_CONF |
RSL_MT_RF_CHAN_REL |
RSL_MT_MS_POWER_CONTROL |
RSL_MT_BS_POWER_CONTROL |
RSL_MT_PREPROC_CONFIG |
RSL_MT_PREPROC_MEAS_RES |
RSL_MT_RF_CHAN_REL_ACK |
RSL_MT_SACCH_INFO_MODIFY |
RSL_MT_TALKER_DET |
RSL_MT_LISTENER_DET |
RSL_MT_REMOTE_CODEC_CONF_REP |
RSL_MT_RTD_REP |
RSL_MT_PRE_HANDO_NOTIF |
RSL_MT_MR_CODEC_MOD_REQ |
RSL_MT_MR_CODEC_MOD_ACK |
RSL_MT_MR_CODEC_MOD_NACK |
RSL_MT_MR_CODEC_MOD_PER |
RSL_MT_TFO_REP |
RSL_MT_TFO_MOD_REQ |
RSL_MT_LOCATION_INFO |
RSL_MT_IPAC_DIR_RETR_ENQ |
RSL_MT_IPAC_PDCH_ACT |
RSL_MT_IPAC_PDCH_ACT_ACK |
RSL_MT_IPAC_PDCH_ACT_NACK |
RSL_MT_IPAC_PDCH_DEACT |
RSL_MT_IPAC_PDCH_DEACT_ACK |
RSL_MT_IPAC_PDCH_DEACT_NACK |
RSL_MT_IPAC_CONNECT_MUX |
RSL_MT_IPAC_CONNECT_MUX_ACK |
RSL_MT_IPAC_CONNECT_MUX_NACK |
RSL_MT_IPAC_BIND_MUX |
RSL_MT_IPAC_BIND_MUX_ACK |
RSL_MT_IPAC_BIND_MUX_NACK |
RSL_MT_IPAC_DISC_MUX |
RSL_MT_IPAC_DISC_MUX_ACK |
RSL_MT_IPAC_DISC_MUX_NACK |
RSL_MT_IPAC_MEAS_PREPROC_DFT |
RSL_MT_IPAC_HO_CAN_ENQ |
RSL_MT_IPAC_HO_CAN_RES |
RSL_MT_IPAC_CRCX |
RSL_MT_IPAC_CRCX_ACK |
RSL_MT_IPAC_CRCX_NACK |
RSL_MT_IPAC_MDCX |
RSL_MT_IPAC_MDCX_ACK |
RSL_MT_IPAC_MDCX_NACK |
RSL_MT_IPAC_DLCX_IND |
RSL_MT_IPAC_DLCX |
RSL_MT_IPAC_DLCX_ACK |
RSL_MT_IPAC_DLCX_NACK |
RSL_MT_OSMO_ETWS_CMD |

## ◆ abis_rsl_msgtype_ericsson

enum abis_rsl_msgtype_ericsson

Ericsson vendor-specific RSL message types.

Enumerator
RSL_MT_ERICSSON_IMM_ASS_SENT |

## ◆ abis_rsl_msgtype_siemens

enum abis_rsl_msgtype_siemens

Siemens vendor-specific RSL message types.

Enumerator
RSL_MT_SIEMENS_MRPCI |
RSL_MT_SIEMENS_INTRAC_HO_COND_IND |
RSL_MT_SIEMENS_INTERC_HO_COND_IND |
RSL_MT_SIEMENS_FORCED_HO_REQ |
RSL_MT_SIEMENS_PREF_AREA_REQ |
RSL_MT_SIEMENS_PREF_AREA |
RSL_MT_SIEMENS_START_TRACE |
RSL_MT_SIEMENS_START_TRACE_ACK |
RSL_MT_SIEMENS_STOP_TRACE |
RSL_MT_SIEMENS_TRMR |
RSL_MT_SIEMENS_HO_FAIL_IND |
RSL_MT_SIEMENS_STOP_TRACE_ACK |
RSL_MT_SIEMENS_UPLF |
RSL_MT_SIEMENS_UPLB |
RSL_MT_SIEMENS_SET_SYS_INFO_10 |
RSL_MT_SIEMENS_MODIF_COND_IND |

## ◆ rsl_cmod_crt

enum rsl_cmod_crt

Channel rate and type.

Enumerator
RSL_CMOD_CRT_SDCCH |
RSL_CMOD_CRT_TCH_Bm |
RSL_CMOD_CRT_TCH_Lm |
RSL_CMOD_CRT_TCH_BI_Bm |
RSL_CMOD_CRT_TCH_UNI_Bm |
RSL_CMOD_CRT_TCH_GROUP_Bm |
RSL_CMOD_CRT_TCH_GROUP_Lm |
RSL_CMOD_CRT_TCH_BCAST_Bm |
RSL_CMOD_CRT_TCH_BCAST_Lm |
RSL_CMOD_CRT_OSMO_TCH_VAMOS_Bm |
RSL_CMOD_CRT_OSMO_TCH_VAMOS_Lm |

## ◆ rsl_cmod_csd_nt

enum rsl_cmod_csd_nt

Non-transparent data.

Enumerator
RSL_CMOD_CSD_NTA_43k5_14k5 |
RSL_CMOD_CSD_NTA_29k0_14k5 |
RSL_CMOD_CSD_NTA_43k5_29k0 |
RSL_CMOD_CSD_NTA_14k5_43k5 |
RSL_CMOD_CSD_NTA_14k5_29k0 |
RSL_CMOD_CSD_NTA_29k0_43k5 |
RSL_CMOD_CSD_NT_43k5 |
RSL_CMOD_CSD_NT_28k8 |
RSL_CMOD_CSD_NT_14k5 |
RSL_CMOD_CSD_NT_12k0 |
RSL_CMOD_CSD_NT_6k0 |

## ◆ rsl_cmod_csd_t

enum rsl_cmod_csd_t

Transparent data.

Enumerator
RSL_CMOD_CSD_T_32k0 |
RSL_CMOD_CSD_T_29k0 |
RSL_CMOD_CSD_T_14k4 |
RSL_CMOD_CSD_T_9k6 |
RSL_CMOD_CSD_T_4k8 |
RSL_CMOD_CSD_T_2k4 |
RSL_CMOD_CSD_T_1k2 |
RSL_CMOD_CSD_T_600 |
RSL_CMOD_CSD_T_1200_75 |

## ◆ rsl_cmod_sp

enum rsl_cmod_sp

Speech.

Enumerator
RSL_CMOD_SP_GSM1 |
RSL_CMOD_SP_GSM2 |
RSL_CMOD_SP_GSM3 |
RSL_CMOD_SP_GSM4 |
RSL_CMOD_SP_GSM5 |
RSL_CMOD_SP_GSM6 |

## ◆ rsl_cmod_spd

enum rsl_cmod_spd

Enumerator
RSL_CMOD_SPD_SPEECH |
RSL_CMOD_SPD_DATA |
RSL_CMOD_SPD_SIGN |

## ◆ rsl_ipac_embedded_ie

enum rsl_ipac_embedded_ie

ip.access specific embedded information elements

Enumerator
RSL_IPAC_EIE_RXLEV |
RSL_IPAC_EIE_RXQUAL |
RSL_IPAC_EIE_FREQ_ERR |
RSL_IPAC_EIE_TIMING_ERR |
RSL_IPAC_EIE_MEAS_AVG_CFG |
RSL_IPAC_EIE_BS_PWR_CTL |
RSL_IPAC_EIE_MS_PWR_CTL |
RSL_IPAC_EIE_HANDO_THRESH |
RSL_IPAC_EIE_NCELL_DEFAULTS |
RSL_IPAC_EIE_NCELL_LIST |
RSL_IPAC_EIE_PC_THRESH_COMP |
RSL_IPAC_EIE_HO_THRESH_COMP |
RSL_IPAC_EIE_HO_CAUSE |
RSL_IPAC_EIE_HO_CANDIDATES |
RSL_IPAC_EIE_NCELL_BA_CHG_LIST |
RSL_IPAC_EIE_NUM_OF_MS |
RSL_IPAC_EIE_HO_CAND_EXT |
RSL_IPAC_EIE_NCELL_DEF_EXT |
RSL_IPAC_EIE_NCELL_LIST_EXT |
RSL_IPAC_EIE_MASTER_KEY |
RSL_IPAC_EIE_MASTER_SALT |
RSL_IPAC_EIE_MEAS_TRANS_RES |
RSL_IPAC_EIE_3G_HO_PARAM |
RSL_IPAC_EIE_3G_NCELL_LIST |
RSL_IPAC_EIE_SDCCH_CTL_PARAM |
RSL_IPAC_EIE_AMR_CONV_THRESH |
RSL_IPAC_EIE_OSMO_MEAS_AVG_CFG |
RSL_IPAC_EIE_OSMO_MS_PWR_CTL |
RSL_IPAC_EIE_OSMO_PC_THRESH_COMP |

## ◆ rsl_ipac_rtp_csd_format_d

enum rsl_ipac_rtp_csd_format_d

Enumerator
RSL_IPAC_RTP_CSD_EXT_TRAU | TRAU-like RTP format, without leading zero-bits.
RSL_IPAC_RTP_CSD_NON_TRAU | packed 16k (252/288 bit) / 8k (126 bit) in RTP
RSL_IPAC_RTP_CSD_TRAU_BTS | TRAU in BTS; V.110 in RTP/CLEARMODE.
RSL_IPAC_RTP_CSD_IWF_FREE | unknown proprietary IWF-free BTS-BTS data

## ◆ rsl_ipac_rtp_csd_format_ir

enum rsl_ipac_rtp_csd_format_ir

Enumerator
RSL_IPAC_RTP_CSD_IR_8k |
RSL_IPAC_RTP_CSD_IR_16k |
RSL_IPAC_RTP_CSD_IR_32k |
RSL_IPAC_RTP_CSD_IR_64k |

## ◆ rsl_ipac_rtp_payload

enum rsl_ipac_rtp_payload

Enumerator
RSL_IPAC_RTP_GSM |
RSL_IPAC_RTP_EFR |
RSL_IPAC_RTP_AMR |
RSL_IPAC_RTP_CSD |
RSL_IPAC_RTP_MUX |

## ◆ rsl_ipac_speech_mode_m

enum rsl_ipac_speech_mode_m

Enumerator
RSL_IPAC_SPEECH_M_RXTX |
RSL_IPAC_SPEECH_M_RX |
RSL_IPAC_SPEECH_M_TX |

## ◆ rsl_ipac_speech_mode_s

enum rsl_ipac_speech_mode_s

Enumerator
RSL_IPAC_SPEECH_GSM_FR |
RSL_IPAC_SPEECH_GSM_EFR |
RSL_IPAC_SPEECH_GSM_AMR_FR |
RSL_IPAC_SPEECH_GSM_HR |
RSL_IPAC_SPEECH_GSM_AMR_HR |
RSL_IPAC_SPEECH_AS_RTP |

## ◆ rsl_mrpci_phase

enum rsl_mrpci_phase

Enumerator
RSL_MRPCI_PHASE_1 |
RSL_MRPCI_PHASE_2 |
RSL_MRPCI_PHASE_2PLUS |

## ◆ rsl_mrpci_pwrclass

enum rsl_mrpci_pwrclass

Enumerator
RSL_MRPCI_PWRC_1 |
RSL_MRPCI_PWRC_2 |
RSL_MRPCI_PWRC_3 |
RSL_MRPCI_PWRC_4 |
RSL_MRPCI_PWRC_5 |

## ◆ rsl_rel_mode

enum rsl_rel_mode

Enumerator
RSL_REL_NORMAL |
RSL_REL_LOCAL_END |

## Function Documentation

## ◆ __attribute__()

union abis_rsl_chan_nr __attribute__ | ( | (packed) |  | ) |

## ◆ rsl_act_type_name()

static const char * rsl_act_type_name | ( | uint8_t | act_type | ) |
| inline static

Return a human readable name for GSM 08.58 RSL_ACT_* constants.

References get_value_string(), and rsl_act_type_names.

## ◆ rsl_ccch_conf_to_bs_cc_chans()

int rsl_ccch_conf_to_bs_cc_chans | ( | int | ccch_conf | ) |

References RSL_BCCH_CCCH_CONF_1_C, RSL_BCCH_CCCH_CONF_1_NC, RSL_BCCH_CCCH_CONF_2_NC, RSL_BCCH_CCCH_CONF_3_NC, and RSL_BCCH_CCCH_CONF_4_NC.

Referenced by gsm0502_calc_paging_group().

## ◆ rsl_ccch_conf_to_bs_ccch_sdcch_comb()

int rsl_ccch_conf_to_bs_ccch_sdcch_comb | ( | int | ccch_conf | ) |

References RSL_BCCH_CCCH_CONF_1_C, RSL_BCCH_CCCH_CONF_1_NC, RSL_BCCH_CCCH_CONF_2_NC, RSL_BCCH_CCCH_CONF_3_NC, and RSL_BCCH_CCCH_CONF_4_NC.

## ◆ rsl_chan_nr_str()

const char * rsl_chan_nr_str | ( | uint8_t | chan_nr | ) |

Get human-readable string for RSL channel number, in static buffer.

Parameters

  [in] | chan_nr | channel number to be stringified

Returns
  buf with string

References chan_nr, and rsl_chan_nr_str_buf().

## ◆ rsl_chan_nr_str_buf()

char * rsl_chan_nr_str_buf | ( | char * | buf,
|  | size_t | buf_len,
|  | uint8_t | chan_nr
| ) |  |

Get human-readable string for RSL channel number, in caller-provided buffer.

Parameters

  [out] | buf | caller-provided output buffer
  [in] | buf_len | size of buf in bytes
  [in] | chan_nr | channel number to be stringified

Returns
  buf with string

References ABIS_RSL_CHAN_NR_CBITS_BCCH, ABIS_RSL_CHAN_NR_CBITS_Bm_ACCHs, ABIS_RSL_CHAN_NR_CBITS_Lm_ACCHs, ABIS_RSL_CHAN_NR_CBITS_OSMO_CBCH4, ABIS_RSL_CHAN_NR_CBITS_OSMO_CBCH8, ABIS_RSL_CHAN_NR_CBITS_OSMO_PDCH, ABIS_RSL_CHAN_NR_CBITS_OSMO_VAMOS_Bm_ACCHs, ABIS_RSL_CHAN_NR_CBITS_OSMO_VAMOS_Lm_ACCHs, ABIS_RSL_CHAN_NR_CBITS_PCH_AGCH, ABIS_RSL_CHAN_NR_CBITS_RACH, ABIS_RSL_CHAN_NR_CBITS_SDCCH4_ACCH, ABIS_RSL_CHAN_NR_CBITS_SDCCH8_ACCH, chan_nr, and ts.

Referenced by rsl_chan_nr_str(), and rsl_chan_nr_str_c().

## ◆ rsl_chan_nr_str_c()

char * rsl_chan_nr_str_c | ( | const void * | ctx,
|  | uint8_t | chan_nr
| ) |  |

Get human-readable string for RSL channel number, in dynamically-allocated buffer.

Parameters

  [in] | ctx | talloc context from which to allocate output buffer
  [in] | chan_nr | channel number to be stringified

Returns
  dynamically-allocated buffer with string representation

References chan_nr, and rsl_chan_nr_str_buf().

## ◆ rsl_dec_chan_nr()

int rsl_dec_chan_nr | ( | uint8_t | chan_nr,
|  | uint8_t * | type,
|  | uint8_t * | subch,
|  | uint8_t * | timeslot
| ) |  |

Decode RSL channel number.

Parameters

  [in] | chan_nr | Channel Number
  [out] | type | Channel Type
  [out] | subch | Sub-channel Number
  [out] | timeslot | Timeslot

References chan_nr, RSL_CHAN_BCCH, RSL_CHAN_Bm_ACCHs, RSL_CHAN_Lm_ACCHs, RSL_CHAN_NR_MASK, RSL_CHAN_OSMO_CBCH4, RSL_CHAN_OSMO_CBCH8, RSL_CHAN_OSMO_PDCH, RSL_CHAN_OSMO_VAMOS_Bm_ACCHs, RSL_CHAN_OSMO_VAMOS_Lm_ACCHs, RSL_CHAN_PCH_AGCH, RSL_CHAN_RACH, RSL_CHAN_SDCCH4_ACCH, RSL_CHAN_SDCCH8_ACCH, timeslot, and type.

## ◆ rsl_enc_chan_nr()

uint8_t rsl_enc_chan_nr | ( | uint8_t | type,
|  | uint8_t | subch,
|  | uint8_t | timeslot
| ) |  |

Encode channel number as per Section 9.3.1.

Parameters

  [in] | Channel | Type (RSL_CHAN_...)
  [in] | subch | Sub-Channel within Channel
  [in] | timeslot | Air interface timeslot

Returns
  RSL Channel Number (TS 08.58 9.3.1)

References RSL_CHAN_Lm_ACCHs, RSL_CHAN_OSMO_VAMOS_Lm_ACCHs, RSL_CHAN_SDCCH4_ACCH, RSL_CHAN_SDCCH8_ACCH, timeslot, and type.

## ◆ rsl_err_name()

const char * rsl_err_name | ( | uint8_t | err | ) |

Get human-readable name for RSL Error.

References get_value_string(), and rsl_err_vals.

## ◆ rsl_init_cchan_hdr()

void rsl_init_cchan_hdr | ( | struct abis_rsl_cchan_hdr * | ch,
|  | uint8_t | msg_type
| ) |  |

Initialize a RSL Common Channel header.

Parameters

  [out] | ch | Caller-allocated RSL Common Channel Header
  [in] | msg_type | Message Type

References ABIS_RSL_MDISC_COM_CHAN, abis_rsl_cchan_hdr::c, abis_rsl_cchan_hdr::ie_chan, abis_rsl_common_hdr::msg_discr, msg_type, abis_rsl_common_hdr::msg_type, and RSL_IE_CHAN_NR.

Referenced by l2_ph_chan_conf(), and l2_ph_rach_ind().

## ◆ rsl_init_rll_hdr()

void rsl_init_rll_hdr | ( | struct abis_rsl_rll_hdr * | dh,
|  | uint8_t | msg_type
| ) |  |

Initialize a RSL RLL header.

Parameters

  [out] | dh | Caller-allocated RSL RLL header
  [in] | msg_type | Message Type

References ABIS_RSL_MDISC_RLL, abis_rsl_rll_hdr::c, abis_rsl_rll_hdr::ie_chan, abis_rsl_rll_hdr::ie_link_id, abis_rsl_common_hdr::msg_discr, msg_type, abis_rsl_common_hdr::msg_type, RSL_IE_CHAN_NR, and RSL_IE_LINK_IDENT.

Referenced by rsl_rll_push_hdr(), and rsl_rll_simple().

## ◆ rsl_ipac_msg_name()

const char * rsl_ipac_msg_name | ( | uint8_t | msg_type | ) |

Get human-readable name of ip.access RSL msg type.

References get_value_string(), msg_type, and rsl_ipac_msgt_names.

Referenced by rsl_or_ipac_msg_name().

## ◆ rsl_msg_name()

const char * rsl_msg_name | ( | uint8_t | err | ) |

Get human-readable string for RSL Message Type.

References get_value_string(), msg_type, and rsl_msgt_names.

Referenced by rslms_rx_rll().

## ◆ rsl_or_ipac_msg_name()

const char * rsl_or_ipac_msg_name | ( | uint8_t | msg_type | ) |

Get human-readable name of standard or ip.access RSL msg type.

If msg_type is a standard RSL message type, return its human-readable name. Otherwise return rsl_ipac_msg_name(msg_type).

References get_value_string_or_null(), msg_type, rsl_ipac_msg_name(), rsl_msgt_names, and value_string::str.

## ◆ rsl_rll_push_hdr()

void rsl_rll_push_hdr | ( | struct msgb * | msg,
|  | uint8_t | msg_type,
|  | uint8_t | chan_nr,
|  | uint8_t | link_id,
|  | int | transparent
| ) |  |

Push a RSL RLL header onto an existing msgb.

Parameters

  | msg | Message Buffer to which RLL header shall be pushed
  [in] | msg_type | RSL Message Type
  [in] | chan_nr | RSL Channel Number
  [in] | link_id | RSL Link Identifier
  [in] | transparent | Transparent to BTS (1) or not (0)

References ABIS_RSL_MDISC_TRANSP, abis_rsl_rll_hdr::c, chan_nr, abis_rsl_rll_hdr::chan_nr, link_id, abis_rsl_rll_hdr::link_id, msg, abis_rsl_common_hdr::msg_discr, msg_type, msgb_push(), and rsl_init_rll_hdr().

Referenced by rsl_rll_push_l3(), and send_rslms_rll_l3_ui().

## ◆ rsl_rll_push_l3()

void rsl_rll_push_l3 | ( | struct msgb * | msg,
|  | uint8_t | msg_type,
|  | uint8_t | chan_nr,
|  | uint8_t | link_id,
|  | int | transparent
| ) |  |

Wrap msgb in L3 Info IE and push a RSL RLL header.

Parameters

  [in] | msg | Message Buffer to which L3 Header shall be appended
  [in] | msg_type | RSL Message Type
  [in] | chan_hr | RSL Channel Number
  [in] | link_id | Link Identififer
  [in] | transparent | Transparent to BTS (1) or not (0)

References chan_nr, link_id, msg, msg_type, msgb_l3, msgb_tv16_push(), RSL_IE_L3_INFO, and rsl_rll_push_hdr().

Referenced by send_rslms_rll_l3().

## ◆ rsl_rll_simple()

struct msgb * rsl_rll_simple | ( | uint8_t | msg_type,
|  | uint8_t | chan_nr,
|  | uint8_t | link_id,
|  | int | transparent
| ) |  |

Create msgb with RSL RLL header.

Parameters

  [in] | msg_type | RSL Message Type
  [in] | chan_nr | RSL Channel Number
  [in] | link_id | RSL Link Identifier
  [in] | transparent | Transparent to BTS (1) or not (0)

Returns
  callee-allocated msgb; NULL on error

References ABIS_RSL_MDISC_TRANSP, abis_rsl_rll_hdr::c, chan_nr, abis_rsl_rll_hdr::chan_nr, link_id, abis_rsl_rll_hdr::link_id, msg, abis_rsl_common_hdr::msg_discr, msg_type, msgb_alloc_headroom(), msgb_put(), RSL_ALLOC_HEADROOM, RSL_ALLOC_SIZE, and rsl_init_rll_hdr().

Referenced by rsl_rll_error(), and send_rll_simple().

## ◆ rsl_rlm_cause_name()

const char * rsl_rlm_cause_name | ( | uint8_t | err | ) |

Get human-readable string for RLM cause.

References get_value_string(), and rsl_rlm_cause_strs.

## Variable Documentation

## ◆ __attribute__

struct ipac_preproc_cfg __attribute__

## ◆ rsl_act_type_names [1/2]

const struct value_string rsl_act_type_names[]
| extern

String names of RSL Channel Activation Types.

Referenced by rsl_act_type_name().

## ◆ rsl_act_type_names [2/2]

const struct value_string rsl_act_type_names[]

Initial value:
= {
{ RSL_ACT_TYPE_INITIAL, "INITIAL" },
{ RSL_ACT_TYPE_REACT, "REACT" },
{ RSL_ACT_INTRA_IMM_ASS, "INTRA_IMM_ASS" },
{ RSL_ACT_INTRA_NORM_ASS, "INTRA_NORM_ASS" },
{ RSL_ACT_INTER_ASYNC, "INTER_ASYNC" },
{ RSL_ACT_INTER_SYNC, "INTER_SYNC" },
{ RSL_ACT_SECOND_ADD, "SECOND_ADD" },
{ RSL_ACT_SECOND_MULTI, "SECOND_MULTI" },
{ RSL_ACT_OSMO_PDCH, "OSMO_PDCH" },
{ 0, NULL }
}
RSL_ACT_SECOND_MULTI
#define RSL_ACT_SECOND_MULTI
Definition: gsm_08_58.h:488
RSL_ACT_TYPE_REACT
#define RSL_ACT_TYPE_REACT
Definition: gsm_08_58.h:482
RSL_ACT_OSMO_PDCH
#define RSL_ACT_OSMO_PDCH
Definition: gsm_08_58.h:489
RSL_ACT_INTER_ASYNC
#define RSL_ACT_INTER_ASYNC
Definition: gsm_08_58.h:485
RSL_ACT_INTRA_NORM_ASS
#define RSL_ACT_INTRA_NORM_ASS
Definition: gsm_08_58.h:484
RSL_ACT_TYPE_INITIAL
#define RSL_ACT_TYPE_INITIAL
Definition: gsm_08_58.h:481
RSL_ACT_INTRA_IMM_ASS
#define RSL_ACT_INTRA_IMM_ASS
Definition: gsm_08_58.h:483
RSL_ACT_SECOND_ADD
#define RSL_ACT_SECOND_ADD
Definition: gsm_08_58.h:487
RSL_ACT_INTER_SYNC
#define RSL_ACT_INTER_SYNC
Definition: gsm_08_58.h:486

String names of RSL Channel Activation Types.

Referenced by rsl_act_type_name().

## ◆ rsl_att_tlvdef [1/2]

const struct tlv_definition rsl_att_tlvdef
| extern

## ◆ rsl_att_tlvdef [2/2]

const struct tlv_definition rsl_att_tlvdef

## ◆ rsl_err_vals

const struct value_string rsl_err_vals[]
| static

Referenced by rsl_err_name().

## ◆ rsl_ipac_eie_tlvdef [1/2]

const struct tlv_definition rsl_ipac_eie_tlvdef
| extern

TLV parser definitions for IPA embedded IEs.

## ◆ rsl_ipac_eie_tlvdef [2/2]

const struct tlv_definition rsl_ipac_eie_tlvdef

TLV parser definitions for IPA embedded IEs.

## ◆ rsl_ipac_msgt_names

const struct value_string rsl_ipac_msgt_names[]
| static

Initial value:
= {
{ RSL_MT_IPAC_PDCH_ACT, "IPAC_PDCH_ACT" },
{ RSL_MT_IPAC_PDCH_ACT_ACK, "IPAC_PDCH_ACT_ACK" },
{ RSL_MT_IPAC_PDCH_ACT_NACK, "IPAC_PDCH_ACT_NACK" },
{ RSL_MT_IPAC_PDCH_DEACT, "IPAC_PDCH_DEACT" },
{ RSL_MT_IPAC_PDCH_DEACT_ACK, "IPAC_PDCH_DEACT_ACK" },
{ RSL_MT_IPAC_PDCH_DEACT_NACK, "IPAC_PDCH_DEACT_NACK" },
{ RSL_MT_IPAC_CONNECT_MUX, "IPAC_CONNECT_MUX" },
{ RSL_MT_IPAC_CONNECT_MUX_ACK, "IPAC_CONNECT_MUX_ACK" },
{ RSL_MT_IPAC_CONNECT_MUX_NACK, "IPAC_CONNECT_MUX_NACK" },
{ RSL_MT_IPAC_BIND_MUX, "IPAC_BIND_MUX" },
{ RSL_MT_IPAC_BIND_MUX_ACK, "IPAC_BIND_MUX_ACK" },
{ RSL_MT_IPAC_BIND_MUX_NACK, "IPAC_BIND_MUX_NACK" },
{ RSL_MT_IPAC_DISC_MUX, "IPAC_DISC_MUX" },
{ RSL_MT_IPAC_DISC_MUX_ACK, "IPAC_DISC_MUX_ACK" },
{ RSL_MT_IPAC_DISC_MUX_NACK, "IPAC_DISC_MUX_NACK" },
{ RSL_MT_IPAC_CRCX, "IPAC_CRCX" },
{ RSL_MT_IPAC_CRCX_ACK, "IPAC_CRCX_ACK" },
{ RSL_MT_IPAC_CRCX_NACK, "IPAC_CRCX_NACK" },
{ RSL_MT_IPAC_MDCX, "IPAC_MDCX" },
{ RSL_MT_IPAC_MDCX_ACK, "IPAC_MDCX_ACK" },
{ RSL_MT_IPAC_MDCX_NACK, "IPAC_MDCX_NACK" },
{ RSL_MT_IPAC_DLCX_IND, "IPAC_DLCX_IND" },
{ RSL_MT_IPAC_DLCX, "IPAC_DLCX" },
{ RSL_MT_IPAC_DLCX_ACK, "IPAC_DLCX_ACK" },
{ RSL_MT_IPAC_DLCX_NACK, "IPAC_DLCX_NACK" },
{ RSL_MT_IPAC_DIR_RETR_ENQ, "IPAC_DIR_RETR_ENQ" },
{ 0, NULL }
}
RSL_MT_IPAC_CONNECT_MUX_ACK
@ RSL_MT_IPAC_CONNECT_MUX_ACK
Definition: gsm_08_58.h:249
RSL_MT_IPAC_DISC_MUX
@ RSL_MT_IPAC_DISC_MUX
Definition: gsm_08_58.h:254
RSL_MT_IPAC_CRCX_ACK
@ RSL_MT_IPAC_CRCX_ACK
Definition: gsm_08_58.h:261
RSL_MT_IPAC_BIND_MUX
@ RSL_MT_IPAC_BIND_MUX
Definition: gsm_08_58.h:251
RSL_MT_IPAC_CRCX_NACK
@ RSL_MT_IPAC_CRCX_NACK
Definition: gsm_08_58.h:262
RSL_MT_IPAC_PDCH_DEACT
@ RSL_MT_IPAC_PDCH_DEACT
Definition: gsm_08_58.h:245
RSL_MT_IPAC_DIR_RETR_ENQ
@ RSL_MT_IPAC_DIR_RETR_ENQ
Definition: gsm_08_58.h:241
RSL_MT_IPAC_PDCH_ACT_NACK
@ RSL_MT_IPAC_PDCH_ACT_NACK
Definition: gsm_08_58.h:244
RSL_MT_IPAC_PDCH_ACT
@ RSL_MT_IPAC_PDCH_ACT
Definition: gsm_08_58.h:242
RSL_MT_IPAC_DLCX_ACK
@ RSL_MT_IPAC_DLCX_ACK
Definition: gsm_08_58.h:268
RSL_MT_IPAC_PDCH_ACT_ACK
@ RSL_MT_IPAC_PDCH_ACT_ACK
Definition: gsm_08_58.h:243
RSL_MT_IPAC_MDCX_NACK
@ RSL_MT_IPAC_MDCX_NACK
Definition: gsm_08_58.h:265
RSL_MT_IPAC_DLCX_IND
@ RSL_MT_IPAC_DLCX_IND
Definition: gsm_08_58.h:266
RSL_MT_IPAC_DISC_MUX_ACK
@ RSL_MT_IPAC_DISC_MUX_ACK
Definition: gsm_08_58.h:255
RSL_MT_IPAC_DLCX_NACK
@ RSL_MT_IPAC_DLCX_NACK
Definition: gsm_08_58.h:269
RSL_MT_IPAC_MDCX
@ RSL_MT_IPAC_MDCX
Definition: gsm_08_58.h:263
RSL_MT_IPAC_DISC_MUX_NACK
@ RSL_MT_IPAC_DISC_MUX_NACK
Definition: gsm_08_58.h:256
RSL_MT_IPAC_CONNECT_MUX
@ RSL_MT_IPAC_CONNECT_MUX
Definition: gsm_08_58.h:248
RSL_MT_IPAC_CRCX
@ RSL_MT_IPAC_CRCX
Definition: gsm_08_58.h:260
RSL_MT_IPAC_BIND_MUX_NACK
@ RSL_MT_IPAC_BIND_MUX_NACK
Definition: gsm_08_58.h:253
RSL_MT_IPAC_MDCX_ACK
@ RSL_MT_IPAC_MDCX_ACK
Definition: gsm_08_58.h:264
RSL_MT_IPAC_CONNECT_MUX_NACK
@ RSL_MT_IPAC_CONNECT_MUX_NACK
Definition: gsm_08_58.h:250
RSL_MT_IPAC_BIND_MUX_ACK
@ RSL_MT_IPAC_BIND_MUX_ACK
Definition: gsm_08_58.h:252
RSL_MT_IPAC_PDCH_DEACT_ACK
@ RSL_MT_IPAC_PDCH_DEACT_ACK
Definition: gsm_08_58.h:246
RSL_MT_IPAC_PDCH_DEACT_NACK
@ RSL_MT_IPAC_PDCH_DEACT_NACK
Definition: gsm_08_58.h:247
RSL_MT_IPAC_DLCX
@ RSL_MT_IPAC_DLCX
Definition: gsm_08_58.h:267

ip.access specific

Referenced by rsl_ipac_msg_name().

## ◆ rsl_msgt_names

const struct value_string rsl_msgt_names[]
| static

Referenced by rsl_msg_name(), and rsl_or_ipac_msg_name().

## ◆ rsl_rlm_cause_strs

const struct value_string rsl_rlm_cause_strs[]
| static

Initial value:
= {
{ RLL_CAUSE_T200_EXPIRED, "Timer T200 expired (N200+1) times" },
{ RLL_CAUSE_REEST_REQ, "Re-establishment request" },
{ RLL_CAUSE_UNSOL_UA_RESP, "Unsolicited UA response" },
{ RLL_CAUSE_UNSOL_DM_RESP, "Unsolicited DM response" },
{ RLL_CAUSE_UNSOL_DM_RESP_MF, "Unsolicited DM response, multiple frame" },
{ RLL_CAUSE_UNSOL_SPRV_RESP, "Unsolicited supervisory response" },
{ RLL_CAUSE_SEQ_ERR, "Sequence Error" },
{ RLL_CAUSE_UFRM_INC_PARAM, "U-Frame with incorrect parameters" },
{ RLL_CAUSE_SFRM_INC_PARAM, "S-Frame with incorrect parameters" },
{ RLL_CAUSE_IFRM_INC_MBITS, "I-Frame with incorrect use of M bit" },
{ RLL_CAUSE_IFRM_INC_LEN, "I-Frame with incorrect length" },
{ RLL_CAUSE_FRM_UNIMPL, "Frame not implemented" },
{ RLL_CAUSE_SABM_MF, "SABM command, multiple frame established state" },
{ RLL_CAUSE_SABM_INFO_NOTALL, "SABM frame with information not allowed in this state" },
{ 0, NULL },
}
RLL_CAUSE_UNSOL_DM_RESP_MF
#define RLL_CAUSE_UNSOL_DM_RESP_MF
Definition: gsm_08_58.h:588
RLL_CAUSE_UNSOL_UA_RESP
#define RLL_CAUSE_UNSOL_UA_RESP
Definition: gsm_08_58.h:586
RLL_CAUSE_SEQ_ERR
#define RLL_CAUSE_SEQ_ERR
Definition: gsm_08_58.h:590
RLL_CAUSE_SFRM_INC_PARAM
#define RLL_CAUSE_SFRM_INC_PARAM
Definition: gsm_08_58.h:592
RLL_CAUSE_UFRM_INC_PARAM
#define RLL_CAUSE_UFRM_INC_PARAM
Definition: gsm_08_58.h:591
RLL_CAUSE_REEST_REQ
#define RLL_CAUSE_REEST_REQ
Definition: gsm_08_58.h:585
RLL_CAUSE_T200_EXPIRED
#define RLL_CAUSE_T200_EXPIRED
Definition: gsm_08_58.h:584
RLL_CAUSE_SABM_INFO_NOTALL
#define RLL_CAUSE_SABM_INFO_NOTALL
Definition: gsm_08_58.h:597
RLL_CAUSE_UNSOL_DM_RESP
#define RLL_CAUSE_UNSOL_DM_RESP
Definition: gsm_08_58.h:587
RLL_CAUSE_IFRM_INC_MBITS
#define RLL_CAUSE_IFRM_INC_MBITS
Definition: gsm_08_58.h:593
RLL_CAUSE_SABM_MF
#define RLL_CAUSE_SABM_MF
Definition: gsm_08_58.h:596
RLL_CAUSE_IFRM_INC_LEN
#define RLL_CAUSE_IFRM_INC_LEN
Definition: gsm_08_58.h:594
RLL_CAUSE_UNSOL_SPRV_RESP
#define RLL_CAUSE_UNSOL_SPRV_RESP
Definition: gsm_08_58.h:589
RLL_CAUSE_FRM_UNIMPL
#define RLL_CAUSE_FRM_UNIMPL
Definition: gsm_08_58.h:595

Referenced by rsl_rlm_cause_name().