libosmoisdn 1.13.1.1-afb4 Osmocom ISDN library

Data Fields
v110_ta_state Struct Reference

## Data Fields
unsigned int | v24_flags
| V.24 status flags shared between DTE (user) and DCE (TA, us) More...
struct {
enum v110_ta_d_bit_mode d_bit_mode
ubit_t s_bits
ubit_t x_bits
} | tx
struct {
enum v110_ta_d_bit_mode d_bit_mode
} | rx

## Field Documentation

## ◆ d_bit_mode

enum v110_ta_d_bit_mode v110_ta_state::d_bit_mode

## ◆

struct { ... } v110_ta_state::rx

## ◆ s_bits

ubit_t v110_ta_state::s_bits

## ◆

struct { ... } v110_ta_state::tx

## ◆ v24_flags

unsigned int v110_ta_state::v24_flags

V.24 status flags shared between DTE (user) and DCE (TA, us)

Referenced by osmo_v110_ta_get_circuit(), osmo_v110_ta_get_status(), osmo_v110_ta_set_circuit(), v110_ta_flags_update(), v110_ta_fsm_connect_ta_to_line(), v110_ta_fsm_data_transfer(), v110_ta_fsm_data_transfer_onenter(), v110_ta_fsm_disconnect_onenter(), v110_ta_fsm_idle_ready_onenter(), v110_ta_fsm_resyncing(), and v110_ta_set_status().

## ◆ x_bits

ubit_t v110_ta_state::x_bits

The documentation for this struct was generated from the following file:

- src/isdn/v110_ta.c