libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Fields
bsslap_ta_response Struct Reference
3GPP TS 48.071 BSS LCS Assistance Protocol (BSSLAP).

`#include <gsm_48_071.h>`

## Data Fields
uint16_t | cell_id
uint8_t | ta
bool | more_items
| always set this to false More...

## Field Documentation

## ◆ cell_id

uint16_t bsslap_ta_response::cell_id

Referenced by osmo_bsslap_dec(), and osmo_bsslap_enc().

## ◆ more_items

bool bsslap_ta_response::more_items

always set this to false

## ◆ ta

uint8_t bsslap_ta_response::ta

Referenced by osmo_bsslap_dec(), and osmo_bsslap_enc().

The documentation for this struct was generated from the following file:

- include/osmocom/gsm/protocol/gsm_48_071.h