libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Fields
osmo_gsm48_si_dtm_support Struct Reference

`#include <gsm48_rest_octets.h>`

## Data Fields
bool | present
uint8_t | rac
uint8_t | max_lapdm

## Field Documentation

## ◆ max_lapdm

uint8_t osmo_gsm48_si_dtm_support::max_lapdm

Referenced by osmo_gsm48_rest_octets_si6_encode().

## ◆ present

bool osmo_gsm48_si_dtm_support::present

Referenced by osmo_gsm48_rest_octets_si6_encode().

## ◆ rac

uint8_t osmo_gsm48_si_dtm_support::rac

Referenced by osmo_gsm48_rest_octets_si6_encode().

The documentation for this struct was generated from the following file:

- include/osmocom/gsm/gsm48_rest_octets.h