libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - r -

- r_gsm_assoc_radio_cap : gsm48_classmark3
- r_support : gsm48_classmark3
- ra : ph_rach_ind_param, ph_rach_req_param
- ra_colour : osmo_gsm48_si3_gprs_ind
- ra_id : gsm48_gprs_susp_req
- rac : gprs_ra_id, gsm48_ra_id, osmo_gsm48_si13_info, osmo_gsm48_si_dtm_support, osmo_routing_area_id
- rach_control : gsm48_system_information_type_1, gsm48_system_information_type_2, gsm48_system_information_type_2bis, gsm48_system_information_type_3, gsm48_system_information_type_4
- rach_ind : osmo_phsap_prim
- rach_req : osmo_phsap_prim
- radio : gsm_mncc_bearer_cap
- rai : osmo_cell_global_id_ps
- rand : osmo_auth_vector, osmo_gsup_message, osmo_oap_message
- rand_present : osmo_oap_message
- rate_adaption : gsm_mncc_bearer_cap
- rate_control : osmo_iuup_rnl_status
- rc : osmo_bssap_le_err, osmo_bsslap_err, osmo_bssmap_le_err, osmo_gad_err, osmo_iuup_instance
- rec : gsm_mncc_cause
- rec_val : gsm_mncc_cause
- recovery_ind : osmo_cbsp_restart
- registration_failures : osmo_oap_client_state
- reject : bsslap_pdu
- rejected_talker_priority : gsm0808_uplink_reject_cmd
- rejected_talker_priority_present : gsm0808_uplink_reject_cmd
- reliab_class : gsm48_qos
- rep_period : osmo_cbsp_write_replace
- repeated_acch_capability : gsm48_classmark3
- repetition_period : osmo_cbsp_keep_alive
- req_llc_sapi : gsm48_act_pdp_ctx_req
- req_nsapi : gsm48_act_pdp_ctx_req
- req_ref : gsm0408_vgcs_ul_grant, gsm48_imm_ass
- req_ref1 : gsm48_imm_ass_ext, gsm48_imm_ass_rej
- req_ref2 : gsm48_imm_ass_ext, gsm48_imm_ass_rej
- req_ref3 : gsm48_imm_ass_rej
- req_ref4 : gsm48_imm_ass_rej
- res : osmo_auth_vector
- res_len : osmo_auth_vector
- reset : bsslap_pdu, bssmap_le_pdu, osmo_cbsp_decoded
- reset_compl : osmo_cbsp_decoded
- reset_fail : osmo_cbsp_decoded
- reset_retries : abis_nm_ipacc_att_ns_cfg
- reset_timer : abis_nm_ipacc_att_ns_cfg
- resid_ber : gsm48_qos
- rest : gsm48_imm_ass_rej
- rest_octets : gsm48_system_information_type_13, gsm48_system_information_type_1, gsm48_system_information_type_2bis, gsm48_system_information_type_2quater, gsm48_system_information_type_2ter, gsm48_system_information_type_3
- restart : osmo_cbsp_decoded
- retrans_itp : osmo_timer_nt
- rf_pwr_cap_1 : gsm48_classmark3
- rf_pwr_cap_2 : gsm48_classmark3
- rfci : osmo_iuup_rnl_config, osmo_iuup_rnl_data, osmo_iuup_rnl_status
- rl_recv : gsm411_smr_inst
- rlc_cv_countdown : abis_nm_ipacc_att_rlc_cfg
- rnc_id : osmo_rnc_id
- rout : smcdatastate, smcdownstate, smrdatastate, smrdownstate
- rp_state : gsm411_smr_inst
- rp_timer : gsm411_smr_inst
- rr_cause : gsm0808_handover_complete, gsm0808_handover_failure, gsm48_ass_cpl, gsm48_ass_fail, gsm48_chan_rel, gsm48_ho_cpl, gsm48_ho_fail, gsm48_rr_status, gsm48_uplink_release
- rr_cause_present : gsm0808_handover_complete, gsm0808_handover_failure
- rssi : ph_data_param, ph_rach_ind_param, ph_tch_param
- run : gprs_cipher_impl
- rx_lev : gsm_rx_lev_qual
- rx_qual : gsm_rx_lev_qual
- rxlev_buckets : rxlev_stats