libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Structures | Functions | Variables
gad.h File Reference
3GPP TS 23.032 GAD: Universal Geographical Area Description.

Message encoding and decoding for 3GPP TS 23.032 GAD: Universal Geographical Area Description. More...

`#include <osmocom/gsm/protocol/gsm_23_032.h>`
`#include <osmocom/core/utils.h>`

Go to the source code of this file.

## Data Structures
struct | osmo_gad_ell_point
struct | osmo_gad_ell_point_unc_circle
struct | osmo_gad_ell_point_unc_ellipse
struct | osmo_gad_polygon
struct | osmo_gad_ell_point_alt
struct | osmo_gad_ell_point_alt_unc_ell
struct | osmo_gad_ell_arc
struct | osmo_gad_ha_ell_point_alt_unc_ell
struct | osmo_gad
struct | osmo_gad_err

## Functions
static const char * | osmo_gad_type_name (enum gad_type val)
int | osmo_gad_raw_write (struct msgb *msg, const union gad_raw *gad_raw)
| Append a GAD PDU to the msgb. More...
int | osmo_gad_raw_read (union gad_raw *gad_raw, struct osmo_gad_err **err, void *err_ctx, const uint8_t *data, uint8_t len)
| Read a GAD PDU and validate structure. More...
int | osmo_gad_enc (union gad_raw *gad_raw, const struct osmo_gad *gad)
| Write GAD values with consistent units to raw GAD PDU representation. More...
int | osmo_gad_dec (struct osmo_gad *gad, struct osmo_gad_err **err, void *err_ctx, const union gad_raw *raw)
| Decode GAD raw PDU to values with consistent units. More...
int | osmo_gad_to_str_buf (char *buf, size_t buflen, const struct osmo_gad *gad)
| Return a human readable representation of GAD (location estimate) values. More...
char * | osmo_gad_to_str_c (void *ctx, const struct osmo_gad *gad)
| Return a human readable representation of GAD (location estimate) values. More...
uint32_t | osmo_gad_enc_lat (int32_t deg_1e6)
| Encode a latitude value according to 3GPP TS 23.032. More...
int32_t | osmo_gad_dec_lat (uint32_t lat)
| Decode a latitude value according to 3GPP TS 23.032. More...
uint32_t | osmo_gad_enc_lon (int32_t deg_1e6)
| Encode a longitude value according to 3GPP TS 23.032. More...
int32_t | osmo_gad_dec_lon (uint32_t lon)
| Decode a longitude value according to 3GPP TS 23.032. More...
uint8_t | osmo_gad_enc_unc (uint32_t mm)
| Encode an uncertainty circle value according to 3GPP TS 23.032. More...
uint32_t | osmo_gad_dec_unc (uint8_t unc)
| Decode an uncertainty circle value according to 3GPP TS 23.032. More...

## Variables
const struct value_string | osmo_gad_type_names []

## Detailed Description

Message encoding and decoding for 3GPP TS 23.032 GAD: Universal Geographical Area Description.