libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Fields
abis_om_hdr Struct Reference
A-bis OML

generic header in front of every OML message according to TS 08.59 More...

`#include <gsm_12_21.h>`

## Data Fields
uint8_t | mdisc
| Message Discriminator abis_oml_mdisc. More...
uint8_t | placement
| Placement (like ABIS_OM_PLACEMENT_ONLY) More...
uint8_t | sequence
| Sequence Number (if ABIS_OM_PLACEMENT_MIDDLE) More...
uint8_t | length
| Length in octets. More...
uint8_t | data [0]
| actual payload data More...

## Detailed Description

generic header in front of every OML message according to TS 08.59

## Field Documentation

## ◆ data

uint8_t abis_om_hdr::data[0]

actual payload data

## ◆ length

uint8_t abis_om_hdr::length

Length in octets.

## ◆ mdisc

uint8_t abis_om_hdr::mdisc

Message Discriminator abis_oml_mdisc.

## ◆ placement

uint8_t abis_om_hdr::placement

Placement (like ABIS_OM_PLACEMENT_ONLY)

## ◆ sequence

uint8_t abis_om_hdr::sequence

Sequence Number (if ABIS_OM_PLACEMENT_MIDDLE)

The documentation for this struct was generated from the following file:

- include/osmocom/gsm/protocol/gsm_12_21.h