libosmosim 1.13.1.1-afb4 Osmocom SIM library

Data Fields
pcsc_reader_state Struct Reference

## Data Fields
SCARDCONTEXT | hContext
SCARDHANDLE | hCard
DWORD | dwActiveProtocol
const SCARD_IO_REQUEST * | pioSendPci
SCARD_IO_REQUEST | pioRecvPci
char * | name

## Field Documentation

## ◆ dwActiveProtocol

DWORD pcsc_reader_state::dwActiveProtocol

Referenced by pcsc_card_open(), pcsc_card_reset(), and pcsc_reader_open().

## ◆ hCard

SCARDHANDLE pcsc_reader_state::hCard

Referenced by pcsc_card_close(), pcsc_card_open(), pcsc_card_reset(), pcsc_get_atr(), and pcsc_transceive().

## ◆ hContext

SCARDCONTEXT pcsc_reader_state::hContext

Referenced by pcsc_card_open(), and pcsc_reader_open().

## ◆ name

char* pcsc_reader_state::name

Referenced by pcsc_card_open(), and pcsc_reader_open().

## ◆ pioRecvPci

SCARD_IO_REQUEST pcsc_reader_state::pioRecvPci

Referenced by pcsc_transceive().

## ◆ pioSendPci

const SCARD_IO_REQUEST* pcsc_reader_state::pioSendPci

Referenced by pcsc_card_open(), and pcsc_transceive().

The documentation for this struct was generated from the following file:

- src/sim/reader_pcsc.c