libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - o -

- obj_class : abis_om_fom_hdr
- obj_inst : abis_om_fom_hdr
- oct3 : rsl_ie_chan_ident
- oct4 : rsl_ie_chan_ident
- offset : ph_rach_req_param
- offset_required : gsm48_classmark3
- ofs_angle : osmo_gad_ell_arc
- old_bss_to_new_bss_info : gsm0808_handover_request, gsm0808_handover_required
- old_bss_to_new_bss_info_present : gsm0808_handover_request, gsm0808_handover_required
- old_bss_to_new_bss_info_raw : gsm0808_handover_request
- old_bss_to_new_bss_info_raw_len : gsm0808_handover_request
- old_serial_nr : osmo_cbsp_error_ind, osmo_cbsp_kill, osmo_cbsp_kill_complete, osmo_cbsp_kill_failure, osmo_cbsp_msg_status_query, osmo_cbsp_msg_status_query_complete, osmo_cbsp_msg_status_query_failure, osmo_cbsp_write_replace, osmo_cbsp_write_replace_complete, osmo_cbsp_write_replace_failure
- opc : osmo_sub_auth_data2, osmo_sub_auth_data
- opc_is_op : osmo_sub_auth_data2, osmo_sub_auth_data
- opc_len : osmo_sub_auth_data2
- opcode : ss_request
- oph : osmo_iuup_rnl_prim, osmo_iuup_tnl_prim, osmo_phsap_prim
- options : gsm48_gprs_susp_req
- OSMO_OAP_DISABLED : osmo_oap_client_state
- OSMO_OAP_INITIALIZED : osmo_oap_client_state
- OSMO_OAP_REGISTERED : osmo_oap_client_state
- OSMO_OAP_REQUESTED_CHALLENGE : osmo_oap_client_state
- OSMO_OAP_SENT_CHALLENGE_RESULT : osmo_oap_client_state
- OSMO_OAP_UNINITIALIZED : osmo_oap_client_state