libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Fields
rsl_ie_chan_mode Struct Reference
A-bis RSL

RSL Channel Mode IF (Chapter 9.3.6) More...

`#include <gsm_08_58.h>`

## Data Fields
uint8_t | dtx_dtu
uint8_t | spd_ind
uint8_t | chan_rt
uint8_t | chan_rate

## Detailed Description

RSL Channel Mode IF (Chapter 9.3.6)

## Field Documentation

## ◆ chan_rate

uint8_t rsl_ie_chan_mode::chan_rate

## ◆ chan_rt

uint8_t rsl_ie_chan_mode::chan_rt

## ◆ dtx_dtu

uint8_t rsl_ie_chan_mode::dtx_dtu

## ◆ spd_ind

uint8_t rsl_ie_chan_mode::spd_ind

The documentation for this struct was generated from the following file:

- include/osmocom/gsm/protocol/gsm_08_58.h