libosmogb 1.13.1.1-afb4 Osmocom Gb library

### - _ -

- __attribute__ : gsm_08_16.h, gsm_08_18.h, gprs_ns2_frgre.c

### - b -

- binds : gprs_ns2_vty.c
- block_ack_ies : gprs_bssgp_util.c
- block_ies : gprs_bssgp_util.c
- bssgp_bvc_ctxts : gprs_bssgp.h
- bssgp_bvc_fsm : bssgp_bvc_fsm.c
- bssgp_bvc_fsm_states : bssgp_bvc_fsm.c
- bssgp_bvc_fsm_tdefs : bssgp_bvc_fsm.c
- bssgp_cause_strings : gprs_bssgp_util.c
- bssgp_cell_id : gprs_msgb.h
- bssgp_ctr_description : gprs_bssgp.c
- bssgp_ctrg_desc : gprs_bssgp.c
- bssgp_fc_gran_tbl : gprs_bssgp2.c
- bssgp_nacc_cause_strs : gprs_bssgp_rim.h, gprs_bssgp_rim.c
- bssgp_node : gprs_bssgp_vty.c
- bssgp_ns_send : gprs_bssgp.c, gprs_bssgp_internal.h
- bssgp_ns_send_data : gprs_bssgp.c, gprs_bssgp_internal.h
- bssgp_nsi : gprs_bssgp.h, gprs_bssgp_util.c
- bssgp_pdu_strings : gprs_bssgp_util.c
- bssgp_ran_inf_app_id_strs : gprs_bssgp_rim.h, gprs_bssgp_rim.c
- bssgp_rim_routing_info_discr_strs : gprs_bssgp_rim.h, gprs_bssgp_rim.c
- bssgp_tall_ctx : gprs_bssgp.c
- bssgph : gprs_msgb.h
- bvci : gprs_msgb.h

### - c -

- call_ref : frame_relay.c
- crt_bss_pfc_ack_ies : gprs_bssgp_util.c
- crt_bss_pfc_ies : gprs_bssgp_util.c
- crt_bss_pfc_nack_ies : gprs_bssgp_util.c

### - d -

- d_pag_ps_ies : gprs_bssgp_util.c
- d_pag_ps_rej_ies : gprs_bssgp_util.c
- d_pag_ps_resp_ies : gprs_bssgp_util.c
- data : gsm_08_16.h, gsm_08_18.h
- data_weight : gsm_08_16.h
- del_bss_pfc_ack_ies : gprs_bssgp_util.c
- del_bss_pfc_ies : gprs_bssgp_util.c
- del_bss_pfc_req_ies : gprs_bssgp_util.c
- dl_bss_pfc_ies : gprs_bssgp_util.c
- dl_mb_ud_ies : gprs_bssgp_util.c
- dl_ud_ies : gprs_bssgp_util.c
- DNS : common_vty.c, common_vty.h

### - f -

- fc_bvc_ack_ies : gprs_bssgp_util.c
- fc_bvc_ies : gprs_bssgp_util.c
- fc_ms_ack_ies : gprs_bssgp_util.c
- fc_ms_ies : gprs_bssgp_util.c
- fc_pfc_ack_ies : gprs_bssgp_util.c
- fc_pfc_ies : gprs_bssgp_util.c
- flags : gprs_ns2_frgre.c, gprs_ns_frgre.c
- flush_ll_ack_ies : gprs_bssgp_util.c
- flush_ll_ies : gprs_bssgp_util.c
- fr_tdefs : frame_relay.c

### - g -

- gprs_ns2_aff_cause_prim_strs : gprs_ns2.c, gprs_ns2.h
- gprs_ns2_cause_strs : gprs_ns2.h, gprs_ns2.c
- gprs_ns2_lltype_strs : gprs_ns2.h, gprs_ns2.c
- gprs_ns2_prim_strs : gprs_ns2.h, gprs_ns2.c
- gprs_ns2_sns_bss_fsm : gprs_ns2_sns.c
- gprs_ns2_sns_sgsn_fsm : gprs_ns2_sns.c
- gprs_ns_pdu_strings : gsm_08_16.h, gprs_ns.c
- gprs_ns_signal_ns_names : gprs_ns.h, gprs_ns.c
- gprs_ns_timer_strs : gprs_ns2_vty.c, gprs_ns_vty.c
- gprs_sns_bss_fsm : gprs_ns_sns.c
- gprs_sns_bss_states : gprs_ns_sns.c
- gprs_sns_event_names : gprs_ns2_sns.c, gprs_ns_sns.c
- gprs_sns_fsm_registered : gprs_ns.c

### - i -

- inv_trc_ies : gprs_bssgp_util.c
- ip_addr : gsm_08_16.h
- ip_sns_default_binds : gprs_ns2_vty.c

### - l -

- llc_disc_ies : gprs_bssgp_util.c
- llch : gprs_msgb.h

### - m -

- mod_bss_pfc_ack_ies : gprs_bssgp_util.c
- mod_bss_pfc_ies : gprs_bssgp_util.c
- ms_reg_enq_ies : gprs_bssgp_util.c
- ms_reg_enq_res_ies : gprs_bssgp_util.c
- msg_type : frame_relay.c

### - n -

- ns2_sns_bss_states : gprs_ns2_sns.c
- ns2_sns_sgsn_states : gprs_ns2_sns.c
- ns2_vc_event_names : gprs_ns2_vc_fsm.c
- ns2_vc_fsm : gprs_ns2_vc_fsm.c
- ns2_vc_states : gprs_ns2_vc_fsm.c
- ns_att_tlvdef : gprs_ns.c
- ns_att_tlvdef1 : gprs_ns2.c
- ns_att_tlvdef2 : gprs_ns2.c
- ns_bind_node : gprs_ns2_vty.c
- ns_cause_str : gprs_ns.c
- ns_ctr_description : gprs_ns2.c
- ns_node : gprs_ns2_vty.c, gprs_ns_vty.c
- ns_nse_node : gprs_ns2_vty.c
- nsbind_stat_description : gprs_ns2.c
- nsbind_statg_desc : gprs_ns2.c
- nse_ctrg_desc : gprs_ns2.c
- nsei : gprs_msgb.h
- nses : gprs_ns2_vty.c
- nsvc_ctr_description : gprs_ns.c
- nsvc_ctrg_desc : gprs_ns.c, gprs_ns2.c
- nsvc_stat_description : gprs_ns.c, gprs_ns2.c
- nsvc_statg_desc : gprs_ns.c, gprs_ns2.c

### - o -

- osmo_fr_role_names : frame_relay.h, frame_relay.c
- osmo_pdef_bssgp : gprs_bssgp.h, gprs_bssgp_util.c
- overload_ies : gprs_bssgp_util.c

### - p -

- pag_cs_ies : gprs_bssgp_util.c
- pag_ps_ies : gprs_bssgp_util.c
- pdu_type : gsm_08_16.h, gsm_08_18.h
- prot_disc : frame_relay.c
- ps_ho_cancel_ies : gprs_bssgp_util.c
- ps_ho_compl_ack_ies : gprs_bssgp_util.c
- ps_ho_compl_ies : gprs_bssgp_util.c
- ps_ho_request_ack_ies : gprs_bssgp_util.c
- ps_ho_request_ies : gprs_bssgp_util.c
- ps_ho_request_nack_ies : gprs_bssgp_util.c
- ps_ho_required_ack_ies : gprs_bssgp_util.c
- ps_ho_required_ies : gprs_bssgp_util.c
- ps_ho_required_nack_ies : gprs_bssgp_util.c
- ptp_bvc_event_names : bssgp_bvc_fsm.c
- ptype : gprs_ns2_frgre.c, gprs_ns_frgre.c

### - q -

- q933_att_tlvdef : frame_relay.c
- qos_profile : gsm_08_18.h

### - r -

- ra_cap_ies : gprs_bssgp_util.c
- ra_cap_upd_ack_ies : gprs_bssgp_util.c
- ra_cap_upd_ies : gprs_bssgp_util.c
- rad_sts_ies : gprs_bssgp_util.c
- reset_ack_ies : gprs_bssgp_util.c
- reset_ies : gprs_bssgp_util.c
- resume_ack_ies : gprs_bssgp_util.c
- resume_ies : gprs_bssgp_util.c
- resume_nack_ies : gprs_bssgp_util.c
- rinfo_ack_ies : gprs_bssgp_util.c
- rinfo_aerr_ies : gprs_bssgp_util.c
- rinfo_err_ies : gprs_bssgp_util.c
- rinfo_ies : gprs_bssgp_util.c
- rinfo_req_ies : gprs_bssgp_util.c

### - s -

- sig_weight : gsm_08_16.h
- status_ies : gprs_bssgp_util.c
- suspend_ack_ies : gprs_bssgp_util.c
- suspend_ies : gprs_bssgp_util.c
- suspend_nack_ies : gprs_bssgp_util.c

### - t -

- timer_mode_strs : gprs_ns.c
- timer_mode_tout : gprs_ns.c
- tlli : gprs_msgb.h, gsm_08_18.h

### - u -

- udp_port : gsm_08_16.h
- ul_mb_ud_ies : gprs_bssgp_util.c
- ul_ud_ies : gprs_bssgp_util.c
- unblock_ack_ies : gprs_bssgp_util.c
- unblock_ies : gprs_bssgp_util.c

### - v -

- vc_driver_fr : gprs_ns2_fr.c
- vc_driver_frgre : gprs_ns2_frgre.c
- vc_driver_ip : gprs_ns2_udp.c
- vty_fr_network : gprs_ns2_vty.c
- vty_fr_role_names : gprs_ns2_vty.c
- vty_ll_names : gprs_ns2_vty.c
- vty_nsi : gprs_ns2_vty.c, gprs_ns_vty.c