libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Structures | Macros | Functions | Variables
bssmap_le.c File Reference
3GPP TS 49.031 BSSMAP-LE.

Message encoding and decoding for 3GPP TS 49.031 BSSMAP-LE. More...

`#include <string.h>`
`#include <osmocom/core/byteswap.h>`
`#include <osmocom/core/endian.h>`
`#include <osmocom/core/msgb.h>`
`#include <osmocom/gsm/bssmap_le.h>`
`#include <osmocom/gsm/bsslap.h>`
`#include <osmocom/gsm/gad.h>`
`#include <osmocom/gsm/gsm48.h>`
`#include <osmocom/gsm/gsm0808.h>`

## Data Structures
struct | osmo_bssap_le_header

## Macros
#define | BSSAP_LE_MSG_SIZE BSSMAP_MSG_SIZE
#define | BSSAP_LE_MSG_HEADROOM BSSMAP_MSG_HEADROOM
#define | DEC_ERR_NO_RETURN(RC, MSG_TYPE, IEI, CAUSE, fmt, args...)
#define | DEC_ERR(RC, MSG_TYPE, IEI, CAUSE, fmt, args...)
#define | DEC_IE_MANDATORY(MSG_TYPE, IEI, DEC_FUN, DEC_FUN_ARG)
#define | DEC_IE_OPTIONAL_FLAG(MSG_TYPE, IEI, DEC_FUN, DEC_FUN_ARG, PRESENCE_FLAG)
#define | DEC_IE_OPTIONAL(MSG_TYPE, IEI, DEC_FUN, DEC_FUN_ARG)
#define | BSSAP_LE_DEC_ERR(RC, fmt, args...)

## Functions
uint8_t | osmo_bssmap_le_ie_enc_location_type (struct msgb *msg, const struct bssmap_le_location_type *location_type)
| Encode full BSSMAP-LE Location Type IE, including IEI tag and length. More...
int | osmo_bssmap_le_ie_dec_location_type (struct bssmap_le_location_type *lt, enum bssmap_le_msgt msgt, enum bssmap_le_iei iei, struct osmo_bssmap_le_err **err, void *err_ctx, const uint8_t *elem, uint8_t len)
| Decode BSSMAP-LE Location Type IE value part. More...
static uint8_t | osmo_bssmap_le_ie_enc_lcs_client_type (struct msgb *msg, enum bssmap_le_lcs_client_type client_type)
| Encode full BSSMAP-LE LCS Client Type IE, including IEI tag and length. More...
static int | osmo_bssmap_le_ie_dec_lcs_client_type (enum bssmap_le_lcs_client_type *client_type, enum bssmap_le_msgt msgt, enum bssmap_le_iei iei, struct osmo_bssmap_le_err **err, void *err_ctx, const uint8_t *elem, uint8_t len)
static uint8_t | osmo_bssmap_le_ie_enc_lcs_priority (struct msgb *msg, uint8_t priority)
| Encode full BSSMAP-LE LCS Priority IE, including IEI tag and length. More...
static int | osmo_bssmap_le_ie_dec_lcs_priority (uint8_t *priority, enum bssmap_le_msgt msgt, enum bssmap_le_iei iei, struct osmo_bssmap_le_err **err, void *err_ctx, const uint8_t *elem, uint8_t len)
static uint8_t | osmo_bssmap_le_ie_enc_lcs_qos (struct msgb *msg, const struct osmo_bssmap_le_lcs_qos *qos)
| Encode full BSSMAP-LE LCS QoS IE, including IEI tag and length. More...
static int | osmo_bssmap_le_ie_dec_lcs_qos (struct osmo_bssmap_le_lcs_qos *qos, enum bssmap_le_msgt msgt, enum bssmap_le_iei iei, struct osmo_bssmap_le_err **err, void *err_ctx, const uint8_t *elem, uint8_t len)
int | osmo_lcs_cause_enc (struct msgb *msg, const struct lcs_cause_ie *lcs_cause)
| Encode the value part of 3GPP TS 49.031 10.13 LCS Cause, without IEI and len. More...
int | osmo_lcs_cause_dec (struct lcs_cause_ie *lcs_cause, enum bssmap_le_msgt msgt, enum bssmap_le_iei iei, struct osmo_bssmap_le_err **err, void *err_ctx, const uint8_t *data, uint8_t len)
| Decode the value part of 3GPP TS 49.031 10.13 LCS Cause, without IEI and len. More...
static int | osmo_bssmap_le_ie_enc_apdu (struct msgb *msg, const struct bsslap_pdu *bsslap)
static int | osmo_bssmap_le_ie_dec_apdu (struct bsslap_pdu *bsslap, enum bssmap_le_msgt msgt, enum bssmap_le_iei iei, struct osmo_bssmap_le_err **err, void *err_ctx, const uint8_t *data, size_t len)
static int | osmo_bssmap_le_ie_dec_cell_id (struct gsm0808_cell_id *cell_id, enum bssmap_le_msgt msgt, enum bssmap_le_iei iei, struct osmo_bssmap_le_err **err, void *err_ctx, const uint8_t *elem, uint8_t len)
static int | osmo_bssmap_le_ie_dec_imsi (struct osmo_mobile_identity *imsi, enum bssmap_le_msgt msgt, enum bssmap_le_iei iei, struct osmo_bssmap_le_err **err, void *err_ctx, const uint8_t *elem, uint8_t len)
static int | osmo_bssmap_le_ie_dec_imei (struct osmo_mobile_identity *imei, enum bssmap_le_msgt msgt, enum bssmap_le_iei iei, struct osmo_bssmap_le_err **err, void *err_ctx, const uint8_t *elem, uint8_t len)
static int | osmo_bssmap_le_ie_dec_gad (union gad_raw *gad, enum bssmap_le_msgt msgt, enum bssmap_le_iei iei, struct osmo_bssmap_le_err **err, void *err_ctx, const uint8_t *elem, uint8_t len)
struct osmo_bssmap_le_lcs_qos | __attribute__ ((packed))
enum bssmap_le_msgt | osmo_bssmap_le_msgt (const uint8_t *data, uint8_t len)
| Return the BSSMAP-LE msg_type from a BSSAP-LE PDU, e.g. More...
static int | osmo_bssmap_le_enc_reset (struct msgb *msg, enum gsm0808_cause cause)
static int | osmo_bssmap_le_dec_reset (enum gsm0808_cause *cause, enum bssmap_le_msgt msgt, struct osmo_bssmap_le_err **err, void *err_ctx, const struct tlv_parsed *tp)
static int | osmo_bssmap_le_enc_perform_loc_req (struct msgb *msg, const struct bssmap_le_perform_loc_req *params)
static int | osmo_bssmap_le_dec_perform_loc_req (struct bssmap_le_perform_loc_req *params, enum bssmap_le_msgt msgt, struct osmo_bssmap_le_err **err, void *err_ctx, const struct tlv_parsed *tp)
static int | osmo_bssmap_le_enc_perform_loc_resp (struct msgb *msg, const struct bssmap_le_perform_loc_resp *params)
static int | osmo_bssmap_le_dec_perform_loc_resp (struct bssmap_le_perform_loc_resp *params, enum bssmap_le_msgt msgt, struct osmo_bssmap_le_err **err, void *err_ctx, const struct tlv_parsed *tp)
static int | osmo_bssmap_le_enc_perform_loc_abort (struct msgb *msg, const struct lcs_cause_ie *params)
static int | osmo_bssmap_le_dec_perform_loc_abort (struct lcs_cause_ie *params, enum bssmap_le_msgt msgt, struct osmo_bssmap_le_err **err, void *err_ctx, const struct tlv_parsed *tp)
static int | osmo_bssmap_le_enc_conn_oriented_info (struct msgb *msg, const struct bssmap_le_conn_oriented_info *params)
static int | osmo_bssmap_le_dec_conn_oriented_info (struct bssmap_le_conn_oriented_info *params, enum bssmap_le_msgt msgt, struct osmo_bssmap_le_err **err, void *err_ctx, const struct tlv_parsed *tp)
static int | osmo_bssmap_le_enc (struct msgb *msg, const struct bssmap_le_pdu *pdu)
| Encode BSSMAP-LE PDU and add to msgb (3GPP TS 49.031). More...
static int | osmo_bssmap_le_dec (struct bssmap_le_pdu *pdu, struct osmo_bssmap_le_err **err, void *err_ctx, const uint8_t *data, size_t len)
| Decode BSSMAP-LE PDU (3GPP TS 49.031). More...
struct msgb * | osmo_bssap_le_enc (const struct bssap_le_pdu *pdu)
| Encode BSSAP-LE PDU returned in new msgb (3GPP TS 49.031). More...
int | osmo_bssap_le_dec (struct bssap_le_pdu *pdu, struct osmo_bssap_le_err **err, void *err_ctx, struct msgb *msg)
| Decode BSSAP-LE PDU (3GPP TS 49.031). More...
int | osmo_bssap_le_pdu_to_str_buf (char *buf, size_t buflen, const struct bssap_le_pdu *bssap_le)
| Return a human readable string describing a BSSAP-LE PDU. More...
char * | osmo_bssap_le_pdu_to_str_c (void *ctx, const struct bssap_le_pdu *bssap_le)
| Return a human readable string describing a BSSAP-LE PDU. More...

## Variables
static const struct tlv_definition | osmo_bssmap_le_tlvdef
uint8_t | type
uint8_t | length
uint8_t | data [0]
const struct value_string | osmo_bssmap_le_msgt_names []
const struct value_string | osmo_bssmap_le_iei_names []

## Detailed Description

Message encoding and decoding for 3GPP TS 49.031 BSSMAP-LE.

## Macro Definition Documentation

## ◆ BSSAP_LE_DEC_ERR

#define BSSAP_LE_DEC_ERR | ( |  | RC,
|  |  | fmt,
|  |  | args...
| ) |  |

Value:
do { \
if (err && !*err) { \
*err = talloc_zero(err_ctx, struct osmo_bssap_le_err); \
**err = (struct osmo_bssap_le_err){ \
.rc = (RC), \
.logmsg = talloc_asprintf(*err, "Error decoding BSSAP-LE: " fmt, ##args), \
}; \
} \
return RC; \
} while(0)
osmo_bssap_le_err
Definition: bssmap_le.h:42
osmo_bssap_le_err::logmsg
char * logmsg
Definition: bssmap_le.h:46

## Variable Documentation

## ◆ data

uint8_t data[0]

Referenced by osmo_bssmap_le_dec(), osmo_bssmap_le_ie_dec_apdu(), osmo_bssmap_le_msgt(), and osmo_lcs_cause_dec().

## ◆ length

uint8_t length

## ◆ type

uint8_t type