* Freescale Multi Master Multi Memory Interface (M4IF) module

Required properties:
- compatible : Should be "fsl,imx51-m4if"
- reg : Address and length of the register set for the device

Example:

m4if: m4if@83fd8000 {
	compatible = "fsl,imx51-m4if";
	reg = <0x83fd8000 0x1000>;
};
