IFI CANFD controller
--------------------

Required properties:
  - compatible: Should be "ifi,canfd-1.0"
  - reg: Should contain CAN controller registers location and length
  - interrupts: Should contain IRQ line for the CAN controller

Example:

	canfd0: canfd@ff220000 {
		compatible = "ifi,canfd-1.0";
		reg = <0xff220000 0x00001000>;
		interrupts = <0 43 0>;
	};
