* PXA MMC drivers

Driver bindings for the PXA MCI (MMC/SDIO) interfaces

Required properties:
- compatible: Should be "marvell,pxa-mmc".
- vmmc-supply: A regulator for VMMC

Optional properties:
- marvell,detect-delay-ms: sets the detection delay timeout in ms.

In addition to the properties described in this document, the details
described in mmc.txt are supported.

Examples:

mmc0: mmc@41100000 {
	compatible = "marvell,pxa-mmc";
	reg = <0x41100000 0x1000>;
	interrupts = <23>;
	vmmc-supply = <&mmc_regulator>;
	cd-gpios = <&gpio 23 0>;
	wp-gpios = <&gpio 24 0>;
};

