Microsemi Ocelot reset controller

The DEVCPU_GCB:CHIP_REGS have a SOFT_RST register that can be used to reset the
SoC core.

The reset registers are both present in the MSCC vcoreiii MIPS and
microchip Sparx5 armv8 SoC's.

Required Properties:

 - compatible: "mscc,ocelot-chip-reset", "mscc,luton-chip-reset",
   "mscc,jaguar2-chip-reset" or "microchip,sparx5-chip-reset"

Example:
	reset@1070008 {
		compatible = "mscc,ocelot-chip-reset";
		reg = <0x1070008 0x4>;
	};

