SPEAr13XX PCIe DT detail:
================================

SPEAr13XX uses the Synopsys DesignWare PCIe controller and ST MiPHY as PHY
controller.

Required properties:
- compatible	    : should be "st,spear1340-pcie", "snps,dw-pcie".
- phys		    : phandle to PHY node associated with PCIe controller
- phy-names	    : must be "pcie-phy"
- All other definitions as per generic PCI bindings

 Optional properties:
- st,pcie-is-gen1 indicates that forced gen1 initialization is needed.
