Motorola CPCAP PMIC RTC
-----------------------

This module is part of the CPCAP. For more details about the whole
chip see Documentation/devicetree/bindings/mfd/motorola-cpcap.txt.

Requires node properties:
- compatible: should contain "motorola,cpcap-rtc"
- interrupts: An interrupt specifier for alarm and 1 Hz irq

Example:

&cpcap {
	cpcap_rtc: rtc {
		compatible = "motorola,cpcap-rtc";
		interrupts = <39 IRQ_TYPE_NONE>, <26 IRQ_TYPE_NONE>;
	};
};
