===========================================
C-SKY Multi-processors Interrupt Controller
===========================================

C-SKY Multi-processors Interrupt Controller is designed for ck807/ck810/ck860
SMP soc, and it also could be used in non-SMP system.

Interrupt number definition:
  0-15  : software irq, and we use 15 as our IPI_IRQ.
 16-31  : private  irq, and we use 16 as the co-processor timer.
 31-1024: common irq for soc ip.

Interrupt trigger mode: (Defined in dt-bindings/interrupt-controller/irq.h)
 IRQ_TYPE_LEVEL_HIGH (default)
 IRQ_TYPE_LEVEL_LOW
 IRQ_TYPE_EDGE_RISING
 IRQ_TYPE_EDGE_FALLING

=============================
intc node bindings definition
=============================

	Description: Describes SMP interrupt controller

	PROPERTIES

	- compatible
		Usage: required
		Value type: <string>
		Definition: must be "csky,mpintc"
	- #interrupt-cells
		Usage: required
		Value type: <u32>
		Definition: <2>
	- interrupt-controller:
		Usage: required

Examples: ("interrupts = <irq_num IRQ_TYPE_XXX>")
---------
#include <dt-bindings/interrupt-controller/irq.h>

	intc: interrupt-controller {
		compatible = "csky,mpintc";
		#interrupt-cells = <2>;
		interrupt-controller;
	};

	device: device-example {
		...
		interrupts = <34 IRQ_TYPE_EDGE_RISING>;
		interrupt-parent = <&intc>;
	};
