* ST-Ericsson DB8500 Thermal

** Thermal node properties:

- compatible : "stericsson,db8500-thermal";
- reg : address range of the thermal sensor registers;
- interrupts : interrupts generated from PRCMU;
- interrupt-names : "IRQ_HOTMON_LOW" and "IRQ_HOTMON_HIGH";
- num-trips : number of total trip points, this is required, set it 0 if none,
  if greater than 0, the following properties must be defined;
- tripN-temp : temperature of trip point N, should be in ascending order;
- tripN-type : type of trip point N, should be one of "active" "passive" "hot"
  "critical";
- tripN-cdev-num : number of the cooling devices which can be bound to trip
  point N, this is required if trip point N is defined, set it 0 if none,
  otherwise the following cooling device names must be defined;
- tripN-cdev-nameM : name of the No. M cooling device of trip point N;

Usually the num-trips and tripN-*** are separated in board related dts files.

Example:
thermal@801573c0 {
	compatible = "stericsson,db8500-thermal";
	reg = <0x801573c0 0x40>;
	interrupts = <21 0x4>, <22 0x4>;
	interrupt-names = "IRQ_HOTMON_LOW", "IRQ_HOTMON_HIGH";

	num-trips = <3>;

	trip0-temp = <75000>;
	trip0-type = "active";
	trip0-cdev-num = <1>;
	trip0-cdev-name0 = "thermal-cpufreq-0";

	trip1-temp = <80000>;
	trip1-type = "active";
	trip1-cdev-num = <2>;
	trip1-cdev-name0 = "thermal-cpufreq-0";
	trip1-cdev-name1 = "thermal-fan";

	trip2-temp = <85000>;
	trip2-type = "critical";
	trip2-cdev-num = <0>;
}
