This binding is based on the matrix-keymap binding with the following
changes:

keypad,num-rows and keypad,num-columns are required.

Required properties:
- compatible: "ti,tca8418"
- reg: the I2C address
- interrupts: IRQ line number, should trigger on falling edge
- linux,keymap: Keys definitions, see keypad-matrix.
