* Device tree bindings for Texas Instruments keystone device state control

The Keystone II devices have a set of registers that are used to control
the status of its peripherals. This node is intended to allow access to
this functionality.

Required properties:

- compatible:		"ti,keystone-devctrl", "syscon"

- reg:			contains offset/length value for device state control
			registers space.

Example:

devctrl: device-state-control@02620000 {
	compatible = "ti,keystone-devctrl", "syscon";
	reg = <0x02620000 0x1000>;
};
