DA8XX USB OHCI controller

Required properties:

 - compatible: Should be "ti,da830-ohci"
 - reg:        Should contain one register range i.e. start and length
 - interrupts: Description of the interrupt line
 - phys:       Phandle for the PHY device
 - phy-names:  Should be "usb-phy"

Optional properties:
 - vbus-supply: phandle of regulator that controls vbus power / over-current

Example:

ohci: usb@225000 {
        compatible = "ti,da830-ohci";
        reg = <0x225000 0x1000>;
        interrupts = <59>;
        phys = <&usb_phy 1>;
        phy-names = "usb-phy";
        vbus-supply = <&reg_usb_ohci>;
};
