Motorola CPCAP PMIC LEDs
------------------------

This module is part of the CPCAP. For more details about the whole
chip see Documentation/devicetree/bindings/mfd/motorola-cpcap.txt.

Requires node properties:
- compatible: should be one of
   * "motorola,cpcap-led-mdl"		(Main Display Lighting)
   * "motorola,cpcap-led-kl"		(Keyboard Lighting)
   * "motorola,cpcap-led-adl"		(Aux Display Lighting)
   * "motorola,cpcap-led-red"		(Red Triode)
   * "motorola,cpcap-led-green"		(Green Triode)
   * "motorola,cpcap-led-blue"		(Blue Triode)
   * "motorola,cpcap-led-cf"		(Camera Flash)
   * "motorola,cpcap-led-bt"		(Bluetooth)
   * "motorola,cpcap-led-cp"		(Camera Privacy LED)
- label: see Documentation/devicetree/bindings/leds/common.txt
- vdd-supply: A phandle to the regulator powering the LED

Example:

&cpcap {
	cpcap_led_red: red-led {
		compatible = "motorola,cpcap-led-red";
		label = "cpcap:red";
		vdd-supply = <&sw5>;
	};
};
