MediaTek Gen2 PCIe controller

Required properties:
- compatible: Should contain one of the following strings:
	"mediatek,mt2701-pcie"
	"mediatek,mt2712-pcie"
	"mediatek,mt7622-pcie"
	"mediatek,mt7623-pcie"
	"mediatek,mt7629-pcie"
	"airoha,en7523-pcie"
- device_type: Must be "pci"
- reg: Base addresses and lengths of the root ports.
- reg-names: Names of the above areas to use during resource lookup.
- #address-cells: Address representation for root ports (must be 3)
- #size-cells: Size representation for root ports (must be 2)
- clocks: Must contain an entry for each entry in clock-names.
  See ../clocks/clock-bindings.txt for details.
- clock-names:
  Mandatory entries:
   - sys_ckN :transaction layer and data link layer clock
  Required entries for MT2701/MT7623:
   - free_ck :for reference clock of PCIe subsys
  Required entries for MT2712/MT7622:
   - ahb_ckN :AHB slave interface operating clock for CSR access and RC
	      initiated MMIO access
  Required entries for MT7622:
   - axi_ckN :application layer MMIO channel operating clock
   - aux_ckN :pe2_mac_bridge and pe2_mac_core operating clock when
	      pcie_mac_ck/pcie_pipe_ck is turned off
   - obff_ckN :OBFF functional block operating clock
   - pipe_ckN :LTSSM and PHY/MAC layer operating clock
  where N starting from 0 to one less than the number of root ports.
- phys: List of PHY specifiers (used by generic PHY framework).
- phy-names : Must be "pcie-phy0", "pcie-phy1", "pcie-phyN".. based on the
  number of PHYs as specified in *phys* property.
- power-domains: A phandle and power domain specifier pair to the power domain
  which is responsible for collapsing and restoring power to the peripheral.
- bus-range: Range of bus numbers associated with this controller.
- ranges: Ranges for the PCI memory and I/O regions.

Required properties for MT7623/MT2701:
- #interrupt-cells: Size representation for interrupts (must be 1)
- interrupt-map-mask and interrupt-map: Standard PCI IRQ mapping properties
  Please refer to the standard PCI bus binding document for a more detailed
  explanation.
- resets: Must contain an entry for each entry in reset-names.
  See ../reset/reset.txt for details.
- reset-names: Must be "pcie-rst0", "pcie-rst1", "pcie-rstN".. based on the
  number of root ports.

Required properties for MT2712/MT7622/MT7629:
-interrupts: A list of interrupt outputs of the controller, must have one
	     entry for each PCIe port
- interrupt-names: Must include the following entries:
	- "pcie_irq": The interrupt that is asserted when an MSI/INTX is received
- linux,pci-domain: PCI domain ID. Should be unique for each host controller

In addition, the device tree node must have sub-nodes describing each
PCIe port interface, having the following mandatory properties:

Required properties:
- device_type: Must be "pci"
- reg: Only the first four bytes are used to refer to the correct bus number
  and device number.
- #address-cells: Must be 3
- #size-cells: Must be 2
- #interrupt-cells: Must be 1
- interrupt-map-mask and interrupt-map: Standard PCI IRQ mapping properties
  Please refer to the standard PCI bus binding document for a more detailed
  explanation.
- ranges: Sub-ranges distributed from the PCIe controller node. An empty
  property is sufficient.

Examples for MT7623:

	hifsys: syscon@1a000000 {
		compatible = "mediatek,mt7623-hifsys",
			     "mediatek,mt2701-hifsys",
			     "syscon";
		reg = <0 0x1a000000 0 0x1000>;
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	pcie: pcie@1a140000 {
		compatible = "mediatek,mt7623-pcie";
		device_type = "pci";
		reg = <0 0x1a140000 0 0x1000>, /* PCIe shared registers */
		      <0 0x1a142000 0 0x1000>, /* Port0 registers */
		      <0 0x1a143000 0 0x1000>, /* Port1 registers */
		      <0 0x1a144000 0 0x1000>; /* Port2 registers */
		reg-names = "subsys", "port0", "port1", "port2";
		#address-cells = <3>;
		#size-cells = <2>;
		#interrupt-cells = <1>;
		interrupt-map-mask = <0xf800 0 0 0>;
		interrupt-map = <0x0000 0 0 0 &sysirq GIC_SPI 193 IRQ_TYPE_LEVEL_LOW>,
				<0x0800 0 0 0 &sysirq GIC_SPI 194 IRQ_TYPE_LEVEL_LOW>,
				<0x1000 0 0 0 &sysirq GIC_SPI 195 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&topckgen CLK_TOP_ETHIF_SEL>,
			 <&hifsys CLK_HIFSYS_PCIE0>,
			 <&hifsys CLK_HIFSYS_PCIE1>,
			 <&hifsys CLK_HIFSYS_PCIE2>;
		clock-names = "free_ck", "sys_ck0", "sys_ck1", "sys_ck2";
		resets = <&hifsys MT2701_HIFSYS_PCIE0_RST>,
			 <&hifsys MT2701_HIFSYS_PCIE1_RST>,
			 <&hifsys MT2701_HIFSYS_PCIE2_RST>;
		reset-names = "pcie-rst0", "pcie-rst1", "pcie-rst2";
		phys = <&pcie0_phy PHY_TYPE_PCIE>, <&pcie1_phy PHY_TYPE_PCIE>,
		       <&pcie2_phy PHY_TYPE_PCIE>;
		phy-names = "pcie-phy0", "pcie-phy1", "pcie-phy2";
		power-domains = <&scpsys MT2701_POWER_DOMAIN_HIF>;
		bus-range = <0x00 0xff>;
		ranges = <0x81000000 0 0x1a160000 0 0x1a160000 0 0x00010000	/* I/O space */
			  0x83000000 0 0x60000000 0 0x60000000 0 0x10000000>;	/* memory space */

		pcie@0,0 {
			reg = <0x0000 0 0 0 0>;
			#address-cells = <3>;
			#size-cells = <2>;
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 0>;
			interrupt-map = <0 0 0 0 &sysirq GIC_SPI 193 IRQ_TYPE_LEVEL_LOW>;
			ranges;
		};

		pcie@1,0 {
			reg = <0x0800 0 0 0 0>;
			#address-cells = <3>;
			#size-cells = <2>;
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 0>;
			interrupt-map = <0 0 0 0 &sysirq GIC_SPI 194 IRQ_TYPE_LEVEL_LOW>;
			ranges;
		};

		pcie@2,0 {
			reg = <0x1000 0 0 0 0>;
			#address-cells = <3>;
			#size-cells = <2>;
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 0>;
			interrupt-map = <0 0 0 0 &sysirq GIC_SPI 195 IRQ_TYPE_LEVEL_LOW>;
			ranges;
		};
	};

Examples for MT2712:

	pcie1: pcie@112ff000 {
		compatible = "mediatek,mt2712-pcie";
		device_type = "pci";
		reg = <0 0x112ff000 0 0x1000>;
		reg-names = "port1";
		linux,pci-domain = <1>;
		#address-cells = <3>;
		#size-cells = <2>;
		interrupts = <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "pcie_irq";
		clocks = <&topckgen CLK_TOP_PE2_MAC_P1_SEL>,
			 <&pericfg CLK_PERI_PCIE1>;
		clock-names = "sys_ck1", "ahb_ck1";
		phys = <&u3port1 PHY_TYPE_PCIE>;
		phy-names = "pcie-phy1";
		bus-range = <0x00 0xff>;
		ranges = <0x82000000 0 0x11400000  0x0 0x11400000  0 0x300000>;
		status = "disabled";

		#interrupt-cells = <1>;
		interrupt-map-mask = <0 0 0 7>;
		interrupt-map = <0 0 0 1 &pcie_intc1 0>,
				<0 0 0 2 &pcie_intc1 1>,
				<0 0 0 3 &pcie_intc1 2>,
				<0 0 0 4 &pcie_intc1 3>;
		pcie_intc1: interrupt-controller {
			interrupt-controller;
			#address-cells = <0>;
			#interrupt-cells = <1>;
		};
	};

	pcie0: pcie@11700000 {
		compatible = "mediatek,mt2712-pcie";
		device_type = "pci";
		reg = <0 0x11700000 0 0x1000>;
		reg-names = "port0";
		linux,pci-domain = <0>;
		#address-cells = <3>;
		#size-cells = <2>;
		interrupts = <GIC_SPI 115 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "pcie_irq";
		clocks = <&topckgen CLK_TOP_PE2_MAC_P0_SEL>,
			 <&pericfg CLK_PERI_PCIE0>;
		clock-names = "sys_ck0", "ahb_ck0";
		phys = <&u3port0 PHY_TYPE_PCIE>;
		phy-names = "pcie-phy0";
		bus-range = <0x00 0xff>;
		ranges = <0x82000000 0 0x20000000 0x0 0x20000000 0 0x10000000>;
		status = "disabled";

		#interrupt-cells = <1>;
		interrupt-map-mask = <0 0 0 7>;
		interrupt-map = <0 0 0 1 &pcie_intc0 0>,
				<0 0 0 2 &pcie_intc0 1>,
				<0 0 0 3 &pcie_intc0 2>,
				<0 0 0 4 &pcie_intc0 3>;
		pcie_intc0: interrupt-controller {
			interrupt-controller;
			#address-cells = <0>;
			#interrupt-cells = <1>;
		};
	};

Examples for MT7622:

	pcie0: pcie@1a143000 {
		compatible = "mediatek,mt7622-pcie";
		device_type = "pci";
		reg = <0 0x1a143000 0 0x1000>;
		reg-names = "port0";
		linux,pci-domain = <0>;
		#address-cells = <3>;
		#size-cells = <2>;
		interrupts = <GIC_SPI 228 IRQ_TYPE_LEVEL_LOW>;
		interrupt-names = "pcie_irq";
		clocks = <&pciesys CLK_PCIE_P0_MAC_EN>,
			 <&pciesys CLK_PCIE_P0_AHB_EN>,
			 <&pciesys CLK_PCIE_P0_AUX_EN>,
			 <&pciesys CLK_PCIE_P0_AXI_EN>,
			 <&pciesys CLK_PCIE_P0_OBFF_EN>,
			 <&pciesys CLK_PCIE_P0_PIPE_EN>;
		clock-names = "sys_ck0", "ahb_ck0", "aux_ck0",
			      "axi_ck0", "obff_ck0", "pipe_ck0";

		power-domains = <&scpsys MT7622_POWER_DOMAIN_HIF0>;
		bus-range = <0x00 0xff>;
		ranges = <0x82000000 0 0x20000000  0x0 0x20000000  0 0x8000000>;
		status = "disabled";

		#interrupt-cells = <1>;
		interrupt-map-mask = <0 0 0 7>;
		interrupt-map = <0 0 0 1 &pcie_intc0 0>,
				<0 0 0 2 &pcie_intc0 1>,
				<0 0 0 3 &pcie_intc0 2>,
				<0 0 0 4 &pcie_intc0 3>;
		pcie_intc0: interrupt-controller {
			interrupt-controller;
			#address-cells = <0>;
			#interrupt-cells = <1>;
		};
	};

	pcie1: pcie@1a145000 {
		compatible = "mediatek,mt7622-pcie";
		device_type = "pci";
		reg = <0 0x1a145000 0 0x1000>;
		reg-names = "port1";
		linux,pci-domain = <1>;
		#address-cells = <3>;
		#size-cells = <2>;
		interrupts = <GIC_SPI 229 IRQ_TYPE_LEVEL_LOW>;
		interrupt-names = "pcie_irq";
		clocks = <&pciesys CLK_PCIE_P1_MAC_EN>,
			 /* designer has connect RC1 with p0_ahb clock */
			 <&pciesys CLK_PCIE_P0_AHB_EN>,
			 <&pciesys CLK_PCIE_P1_AUX_EN>,
			 <&pciesys CLK_PCIE_P1_AXI_EN>,
			 <&pciesys CLK_PCIE_P1_OBFF_EN>,
			 <&pciesys CLK_PCIE_P1_PIPE_EN>;
		clock-names = "sys_ck1", "ahb_ck1", "aux_ck1",
			      "axi_ck1", "obff_ck1", "pipe_ck1";

		power-domains = <&scpsys MT7622_POWER_DOMAIN_HIF0>;
		bus-range = <0x00 0xff>;
		ranges = <0x82000000 0 0x28000000  0x0 0x28000000  0 0x8000000>;
		status = "disabled";

		#interrupt-cells = <1>;
		interrupt-map-mask = <0 0 0 7>;
		interrupt-map = <0 0 0 1 &pcie_intc1 0>,
				<0 0 0 2 &pcie_intc1 1>,
				<0 0 0 3 &pcie_intc1 2>,
				<0 0 0 4 &pcie_intc1 3>;
		pcie_intc1: interrupt-controller {
			interrupt-controller;
			#address-cells = <0>;
			#interrupt-cells = <1>;
		};
	};
