*  Adaptrum Anarion ethernet controller

This device is a platform glue layer for stmmac.
Please see stmmac.txt for the other unchanged properties.

Required properties:
 - compatible:  Should be "adaptrum,anarion-gmac", "snps,dwmac"
 - phy-mode:    Should be "rgmii". Other modes are not currently supported.


Examples:

	gmac1: ethernet@f2014000 {
		compatible = "adaptrum,anarion-gmac", "snps,dwmac";
		reg = <0xf2014000 0x4000>, <0xf2018100 8>;

		interrupt-parent = <&core_intc>;
		interrupts = <21>;
		interrupt-names = "macirq";

		clocks = <&core_clk>;
		clock-names = "stmmaceth";

		phy-mode = "rgmii";
	};
