* MELFAS MIP4 Touchscreen

Required properties:
- compatible: must be "melfas,mip4_ts"
- reg: I2C slave address of the chip (0x48 or 0x34)
- interrupts: interrupt to which the chip is connected

Optional properties:
- ce-gpios: GPIO connected to the CE (chip enable) pin of the chip

Example:
	i2c@00000000 {
		touchscreen: melfas_mip4@48 {
			compatible = "melfas,mip4_ts";
			reg = <0x48>;
			interrupt-parent = <&gpio>;
			interrupts = <0 IRQ_TYPE_EDGE_FALLING>;
			ce-gpios = <&gpio 0 GPIO_ACTIVE_HIGH>;
		};
	};
