Broadcom BCM63138 Processor Monitor Bus binding
===============================================

Please also refer to reset.txt in this directory for common reset
controller binding usage.

Require properties:

- compatible: must be "brcm,bcm63138-pmb"
- reg: base register address and size for this bus controller
- #reset-cells: must be 2 first cell is the address within the bus instance designated
  by the phandle, and the second is the number of zones for this peripheral

Example:
	pmb0: reset-controller@4800c0 {
		compatible = "brcm,bcm63138-pmb";
		reg = <0x4800c0 0x10>;
		#reset-cells = <2>;
	};
