* Freescale Tigerp platform module

Required properties:
- compatible : Should be "fsl,imx51-tigerp"
- reg : Address and length of the register set for the device

Example:

tigerp: tigerp@83fa0000 {
	compatible = "fsl,imx51-tigerp";
	reg = <0x83fa0000 0x28>;
};
