// SPDX-License-Identifier: GPL-2.0-only
/*
 * support fot the imx6 based aristainetos board
 *
 * Copyright (C) 2014 Heiko Schocher <hs@denx.de>
 */
/dts-v1/;
#include "imx6dl.dtsi"
#include "imx6qdl-aristainetos.dtsi"

/ {
	model = "aristainetos i.MX6 Dual Lite Board 4";
	compatible = "abb,aristainetos-imx6dl-4", "fsl,imx6dl";

	backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm1 0 5000000 0>;
		brightness-levels = <0 4 8 16 32 64 128 255>;
		default-brightness-level = <7>;
		enable-gpios = <&gpio1 2 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_backlight>;
		status = "okay";
	};

	memory@10000000 {
		device_type = "memory";
		reg = <0x10000000 0x40000000>;
	};

	display0: disp0 {
		compatible = "fsl,imx-parallel-display";
		interface-pix-fmt = "rgb24";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_ipu_disp>;
		status = "okay";

		display-timings {
			native-mode = <&timing0>;
			timing0: timing-480x800p60 {
				clock-frequency = <30000000>;
				hactive = <480>;
				vactive = <800>;
				hfront-porch = <59>;
				hback-porch = <10>;
				hsync-len = <10>;
				vback-porch = <15>;
				vfront-porch = <15>;
				vsync-len = <15>;
				hsync-active = <1>;
				vsync-active = <1>;
			};
		};

		port {
			display0_in: endpoint {
				remote-endpoint = <&ipu1_di0_disp0>;
			};
		};
	};
};

&ecspi2 {
	cs-gpios = <&gpio3 24 GPIO_ACTIVE_LOW>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_ecspi2>;
	status = "okay";
};

&i2c2 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c2>;
	status = "okay";
};

&ipu1_di0_disp0 {
	remote-endpoint = <&display0_in>;
};

&pwm1 {
	status = "okay";
};
