// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * at91-sama5d4_xplained.dts - Device Tree file for SAMA5D4 Xplained board
 *
 *  Copyright (C) 2015 Atmel,
 *                2015 Josh Wu <josh.wu@atmel.com>
 */
/dts-v1/;
#include "sama5d4.dtsi"
#include <dt-bindings/input/input.h>

/ {
	model = "Atmel SAMA5D4 Xplained";
	compatible = "atmel,sama5d4-xplained", "atmel,sama5d4", "atmel,sama5";

	chosen {
		stdout-path = "serial0:115200n8";
	};

	memory@20000000 {
		reg = <0x20000000 0x20000000>;
	};

	clocks {
		slow_xtal {
			clock-frequency = <32768>;
		};

		main_xtal {
			clock-frequency = <12000000>;
		};
	};

	ahb {
		apb {
			uart0: serial@f8004000 {
				atmel,use-dma-rx;
				atmel,use-dma-tx;
				status = "okay";
			};

			i2c0: i2c@f8014000 {
				i2c-digital-filter;
				status = "okay";
			};

			macb0: ethernet@f8020000 {
				phy-mode = "rmii";
				status = "okay";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_macb0_rmii &pinctrl_macb0_phy_irq>;

				phy0: ethernet-phy@1 {
					interrupt-parent = <&pioE>;
					interrupts = <1 IRQ_TYPE_LEVEL_LOW>;
					reg = <1>;
				};
			};

			mmc1: mmc@fc000000 {
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_mmc1_clk_cmd_dat0 &pinctrl_mmc1_dat1_3 &pinctrl_mmc1_cd>;
				vmmc-supply = <&vcc_mmc1_reg>;
				vqmmc-supply = <&vcc_3v3_reg>;
				status = "okay";
				slot@0 {
					reg = <0>;
					bus-width = <4>;
					cd-gpios = <&pioE 3 0>;
				};
			};

			usart3: serial@fc00c000 {
				atmel,use-dma-rx;
				atmel,use-dma-tx;
				status = "okay";
			};

			usart4: serial@fc010000 {
				status = "okay";
			};

			spi1: spi@fc018000 {
				pinctrl-names = "default", "cs";
				pinctrl-1 = <&pinctrl_spi1_cs>;
				cs-gpios = <&pioB 21 0>;
				status = "okay";
			};

			tcb2: timer@fc024000 {
				timer0: timer@0 {
					compatible = "atmel,tcb-timer";
					reg = <0>;
				};

				timer1: timer@1 {
					compatible = "atmel,tcb-timer";
					reg = <1>;
				};
			};

			adc0: adc@fc034000 {
				pinctrl-names = "default";
				pinctrl-0 = <
					/* external trigger conflicts with USBA_VBUS */
					&pinctrl_adc0_ad0
					&pinctrl_adc0_ad1
					&pinctrl_adc0_ad2
					&pinctrl_adc0_ad3
					&pinctrl_adc0_ad4
					>;
				atmel,adc-vref = <3300>;
				status = "okay";
			};

			watchdog@fc068640 {
				status = "okay";
			};

			pinctrl@fc06a000 {
				board {
					pinctrl_mmc1_cd: mmc1_cd {
						atmel,pins =
							<AT91_PIOE 3 AT91_PERIPH_GPIO AT91_PINCTRL_PULL_UP_DEGLITCH>;
					};
					pinctrl_usba_vbus: usba_vbus {
						atmel,pins =
							<AT91_PIOE 31 AT91_PERIPH_GPIO AT91_PINCTRL_DEGLITCH>;
					};
					pinctrl_usb_default: usb_default {
						atmel,pins =
							<AT91_PIOE 11 AT91_PERIPH_GPIO AT91_PINCTRL_NONE
							 AT91_PIOE 14 AT91_PERIPH_GPIO AT91_PINCTRL_NONE>;
					};
					pinctrl_key_gpio: key_gpio_0 {
						atmel,pins =
							<AT91_PIOE 8 AT91_PERIPH_GPIO AT91_PINCTRL_PULL_UP_DEGLITCH>;
					};
					pinctrl_macb0_phy_irq: macb0_phy_irq_0 {
						atmel,pins =
							<AT91_PIOE 1 AT91_PERIPH_GPIO AT91_PINCTRL_PULL_UP_DEGLITCH>;
					};
					pinctrl_spi1_cs: spi1_cs_default {
						atmel,pins =
							<AT91_PIOB 21 AT91_PERIPH_GPIO AT91_PINCTRL_NONE>;
					};
					pinctrl_gpio_leds: gpio_leds_default {
						atmel,pins =
							<AT91_PIOD 30 AT91_PERIPH_GPIO AT91_PINCTRL_NONE
							 AT91_PIOE 15 AT91_PERIPH_GPIO AT91_PINCTRL_NONE>;
					};
					pinctrl_vcc_mmc1_reg: vcc_mmc1_reg {
						atmel,pins =
							<AT91_PIOE 4 AT91_PERIPH_GPIO AT91_PINCTRL_NONE>;
					};
				};
			};
		};

		usb0: gadget@400000 {
			atmel,vbus-gpio = <&pioE 31 GPIO_ACTIVE_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_usba_vbus>;
			status = "okay";
		};

		usb1: ohci@500000 {
			num-ports = <3>;
			atmel,vbus-gpio = <0
					   &pioE 11 GPIO_ACTIVE_HIGH
					   &pioE 14 GPIO_ACTIVE_HIGH
					  >;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_usb_default>;
			status = "okay";
		};

		usb2: ehci@600000 {
			status = "okay";
		};

		ebi: ebi@10000000 {
			pinctrl-0 = <&pinctrl_ebi_cs3 &pinctrl_ebi_nrd_nandoe
				     &pinctrl_ebi_nwe_nandwe &pinctrl_ebi_nandrdy
				     &pinctrl_ebi_data_0_7 &pinctrl_ebi_nand_addr>;
			pinctrl-names = "default";
			status = "okay";

			nand_controller: nand-controller {
				status = "okay";

				nand@3 {
					reg = <0x3 0x0 0x2>;
					atmel,rb = <0>;
					nand-bus-width = <8>;
					nand-ecc-mode = "hw";
					nand-on-flash-bbt;
					label = "atmel_nand";

					partitions {
						compatible = "fixed-partitions";
						#address-cells = <1>;
						#size-cells = <1>;

						at91bootstrap@0 {
							label = "at91bootstrap";
							reg = <0x0 0x40000>;
						};

						bootloader@40000 {
							label = "bootloader";
							reg = <0x40000 0xc0000>;
						};

						bootloaderenvred@100000 {
							label = "bootloader env redundant";
							reg = <0x100000 0x40000>;
						};

						bootloaderenv@140000 {
							label = "bootloader env";
							reg = <0x140000 0x40000>;
						};

						dtb@180000 {
							label = "device tree";
							reg = <0x180000 0x80000>;
						};

						kernel@200000 {
							label = "kernel";
							reg = <0x200000 0x600000>;
						};

						rootfs@800000 {
							label = "rootfs";
							reg = <0x800000 0x1f800000>;
						};
					};
				};
			};
		};
	};

	gpio-keys {
		compatible = "gpio-keys";

		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_key_gpio>;

		button {
			label = "pb_user1";
			gpios = <&pioE 8 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_PROG1>;
			wakeup-source;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_gpio_leds>;
		status = "okay";

		led-d8 {
			label = "d8";
			gpios = <&pioD 30 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};

		led-d10 {
			label = "d10";
			gpios = <&pioE 15 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "heartbeat";
		};
	};

	vcc_3v3_reg: fixedregulator_3v3 {
		compatible = "regulator-fixed";
		regulator-name = "VCC 3V3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-boot-on;
		regulator-always-on;
	};

	vcc_mmc1_reg: fixedregulator_mmc1 {
		compatible = "regulator-fixed";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_vcc_mmc1_reg>;
		gpio = <&pioE 4 GPIO_ACTIVE_LOW>;
		regulator-name = "VDD MCI1";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&vcc_3v3_reg>;
		regulator-always-on;
	};
};
