/*
 *  BSD LICENSE
 *
 *  Copyright(c) 2015 Broadcom Corporation.  All rights reserved.
 *
 *  Redistribution and use in source and binary forms, with or without
 *  modification, are permitted provided that the following conditions
 *  are met:
 *
 *    * Redistributions of source code must retain the above copyright
 *      notice, this list of conditions and the following disclaimer.
 *    * Redistributions in binary form must reproduce the above copyright
 *      notice, this list of conditions and the following disclaimer in
 *      the documentation and/or other materials provided with the
 *      distribution.
 *    * Neither the name of Broadcom Corporation nor the names of its
 *      contributors may be used to endorse or promote products derived
 *      from this software without specific prior written permission.
 *
 *  THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
 *  "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
 *  LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
 *  A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
 *  OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
 *  SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
 *  LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
 *  DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
 *  THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
 *  (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
 *  OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
 */

#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/clock/bcm-nsp.h>

/ {
	#address-cells = <1>;
	#size-cells = <1>;
	compatible = "brcm,nsp";
	model = "Broadcom Northstar Plus SoC";
	interrupt-parent = <&gic>;

	aliases {
		serial0 = &uart0;
		serial1 = &uart1;
		ethernet0 = &amac0;
		ethernet1 = &amac1;
		ethernet2 = &amac2;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a9";
			next-level-cache = <&L2>;
			reg = <0x0>;
		};

		cpu1: cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a9";
			next-level-cache = <&L2>;
			enable-method = "brcm,bcm-nsp-smp";
			secondary-boot-reg = <0xffff0fec>;
			reg = <0x1>;
		};
	};

	pmu {
		compatible = "arm,cortex-a9-pmu";
		interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-affinity = <&cpu0>, <&cpu1>;
	};

	mpcore-bus@19000000 {
		compatible = "simple-bus";
		ranges = <0x00000000 0x19000000 0x00023000>;
		#address-cells = <1>;
		#size-cells = <1>;

		a9pll: arm_clk@0 {
			#clock-cells = <0>;
			compatible = "brcm,nsp-armpll";
			clocks = <&osc>;
			reg = <0x00000 0x1000>;
		};

		timer@20200 {
			compatible = "arm,cortex-a9-global-timer";
			reg = <0x20200 0x100>;
			interrupts = <GIC_PPI 11 IRQ_TYPE_EDGE_RISING>;
			clocks = <&periph_clk>;
		};

		twd-timer@20600 {
			compatible = "arm,cortex-a9-twd-timer";
			reg = <0x20600 0x20>;
			interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(2) |
						  IRQ_TYPE_EDGE_RISING)>;
			clocks = <&periph_clk>;
		};

		twd-watchdog@20620 {
			compatible = "arm,cortex-a9-twd-wdt";
			reg = <0x20620 0x20>;
			interrupts = <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(2) |
						  IRQ_TYPE_LEVEL_HIGH)>;
			clocks = <&periph_clk>;
		};

		gic: interrupt-controller@21000 {
			compatible = "arm,cortex-a9-gic";
			#interrupt-cells = <3>;
			#address-cells = <0>;
			interrupt-controller;
			reg = <0x21000 0x1000>,
			      <0x20100 0x100>;
		};

		L2: cache-controller@22000 {
			compatible = "arm,pl310-cache";
			reg = <0x22000 0x1000>;
			cache-unified;
			cache-level = <2>;
		};
	};

	clocks {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		osc: oscillator {
			#clock-cells = <0>;
			compatible = "fixed-clock";
			clock-frequency = <25000000>;
		};

		iprocmed: iprocmed {
			#clock-cells = <0>;
			compatible = "fixed-factor-clock";
			clocks = <&genpll BCM_NSP_GENPLL_IPROCFAST_CLK>;
			clock-div = <2>;
			clock-mult = <1>;
		};

		iprocslow: iprocslow {
			#clock-cells = <0>;
			compatible = "fixed-factor-clock";
			clocks = <&genpll BCM_NSP_GENPLL_IPROCFAST_CLK>;
			clock-div = <4>;
			clock-mult = <1>;
		};

		periph_clk: periph_clk {
			#clock-cells = <0>;
			compatible = "fixed-factor-clock";
			clocks = <&a9pll>;
			clock-div = <2>;
			clock-mult = <1>;
		};
	};

	axi: axi@18000000 {
		compatible = "simple-bus";
		ranges = <0x00000000 0x18000000 0x0011c40c>;
		#address-cells = <1>;
		#size-cells = <1>;

		gpioa: gpio@20 {
			compatible = "brcm,nsp-gpio-a";
			reg = <0x0020 0x70>,
			      <0x3f1c4 0x1c>;
			#gpio-cells = <2>;
			gpio-controller;
			ngpios = <32>;
			interrupt-controller;
			#interrupt-cells = <2>;
			interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
			gpio-ranges = <&pinctrl 0 0 32>;
		};

		uart0: serial@300 {
			compatible = "ns16550a";
			reg = <0x0300 0x100>;
			interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&osc>;
			status = "disabled";
		};

		uart1: serial@400 {
			compatible = "ns16550a";
			reg = <0x0400 0x100>;
			interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&osc>;
			status = "disabled";
		};

		dma: dma@20000 {
			compatible = "arm,pl330", "arm,primecell";
			reg = <0x20000 0x1000>;
			interrupts = <GIC_SPI 47 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 48 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 50 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 51 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 52 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 53 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 54 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 63 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&iprocslow>;
			clock-names = "apb_pclk";
			#dma-cells = <1>;
			dma-coherent;
			status = "disabled";
		};

		sdio: mmc@21000 {
			compatible = "brcm,sdhci-iproc-cygnus";
			reg = <0x21000 0x100>;
			interrupts = <GIC_SPI 145 IRQ_TYPE_LEVEL_HIGH>;
			sdhci,auto-cmd12;
			clocks = <&lcpll0 BCM_NSP_LCPLL0_SDIO_CLK>;
			dma-coherent;
			status = "disabled";
		};

		amac0: ethernet@22000 {
			compatible = "brcm,nsp-amac";
			reg = <0x022000 0x1000>,
			      <0x110000 0x1000>;
			reg-names = "amac_base", "idm_base";
			interrupts = <GIC_SPI 147 IRQ_TYPE_LEVEL_HIGH>;
			dma-coherent;
			status = "disabled";
		};

		amac1: ethernet@23000 {
			compatible = "brcm,nsp-amac";
			reg = <0x023000 0x1000>,
			      <0x111000 0x1000>;
			reg-names = "amac_base", "idm_base";
			interrupts = <GIC_SPI 148 IRQ_TYPE_LEVEL_HIGH>;
			dma-coherent;
			status = "disabled";
		};

		amac2: ethernet@24000 {
			compatible = "brcm,nsp-amac";
			reg = <0x024000 0x1000>,
			      <0x112000 0x1000>;
			reg-names = "amac_base", "idm_base";
			interrupts = <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>;
			dma-coherent;
			status = "disabled";
		};

		mailbox: mailbox@25c00 {
			compatible = "brcm,iproc-fa2-mbox";
			reg = <0x25c00 0x400>;
			interrupts = <GIC_SPI 151 IRQ_TYPE_LEVEL_HIGH>;
			#mbox-cells = <1>;
			brcm,rx-status-len = <32>;
			brcm,use-bcm-hdr;
			dma-coherent;
		};

		nand_controller: nand-controller@26000 {
			compatible = "brcm,nand-iproc", "brcm,brcmnand-v6.1";
			reg = <0x026000 0x600>,
			      <0x11b408 0x600>,
			      <0x026f00 0x20>;
			reg-names = "nand", "iproc-idm", "iproc-ext";
			interrupts = <GIC_SPI 68 IRQ_TYPE_LEVEL_HIGH>;

			#address-cells = <1>;
			#size-cells = <0>;

			brcm,nand-has-wp;
		};

		qspi: spi@27200 {
			compatible = "brcm,spi-nsp-qspi", "brcm,spi-bcm-qspi";
			reg = <0x027200 0x184>,
			      <0x027000 0x124>,
			      <0x11c408 0x004>,
			      <0x0273a0 0x01c>;
			reg-names = "mspi", "bspi", "intr_regs",
				    "intr_status_reg";
			interrupts = <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 76 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 77 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 78 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "spi_lr_fullness_reached",
					  "spi_lr_session_aborted",
					  "spi_lr_impatient",
					  "spi_lr_session_done",
					  "spi_lr_overhead",
					  "mspi_done",
					  "mspi_halted";
			clocks = <&iprocmed>;
			clock-names = "iprocmed";
			num-cs = <2>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		xhci: usb@29000 {
			compatible = "generic-xhci";
			reg = <0x29000 0x1000>;
			interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>;
			phys = <&usb3_phy>;
			phy-names = "usb3-phy";
			dma-coherent;
			status = "disabled";
		};

		ehci0: usb@2a000 {
			compatible = "generic-ehci";
			reg = <0x2a000 0x100>;
			interrupts = <GIC_SPI 79 IRQ_TYPE_LEVEL_HIGH>;
			dma-coherent;
			status = "disabled";
		};

		ohci0: usb@2b000 {
			compatible = "generic-ohci";
			reg = <0x2b000 0x100>;
			interrupts = <GIC_SPI 79 IRQ_TYPE_LEVEL_HIGH>;
			dma-coherent;
			status = "disabled";
		};

		crypto@2f000 {
			compatible = "brcm,spum-nsp-crypto";
			reg = <0x2f000 0x900>;
			mboxes = <&mailbox 0>;
		};

		gpiob: gpio@30000 {
			compatible = "brcm,iproc-nsp-gpio", "brcm,iproc-gpio";
			reg = <0x30000 0x50>;
			#gpio-cells = <2>;
			gpio-controller;
			ngpios = <4>;
			interrupt-controller;
			#interrupt-cells = <2>;
			interrupts = <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>;
		};

		pwm: pwm@31000 {
			compatible = "brcm,iproc-pwm";
			reg = <0x31000 0x28>;
			clocks = <&osc>;
			#pwm-cells = <3>;
			status = "disabled";
		};

		mdio: mdio@32000 {
			compatible = "brcm,iproc-mdio";
			reg = <0x32000 0x8>;
			#size-cells = <0>;
			#address-cells = <1>;
		};

		mdio-mux@32000 {
			compatible = "mdio-mux-mmioreg", "mdio-mux";
			reg = <0x32000 0x4>;
			mux-mask = <0x200>;
			#address-cells = <1>;
			#size-cells = <0>;
			mdio-parent-bus = <&mdio>;

			mdio_int: mdio@0 {
				reg = <0x0>;
				#address-cells = <1>;
				#size-cells = <0>;

				usb3_phy: usb3-phy@10 {
					compatible = "brcm,ns-bx-usb3-phy";
					reg = <0x10>;
					usb3-dmp-syscon = <&usb3_dmp>;
					#phy-cells = <0>;
					status = "disabled";
				};
			};

			mdio_ext: mdio@200 {
				reg = <0x200>;
				#address-cells = <1>;
				#size-cells = <0>;
			};
		};

		rng: rng@33000 {
			compatible = "brcm,bcm-nsp-rng";
			reg = <0x33000 0x14>;
		};

		ccbtimer0: timer@34000 {
			compatible = "arm,sp804", "arm,primecell";
			reg = <0x34000 0x1000>;
			interrupts = <GIC_SPI 90 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&iprocslow>;
			clock-names = "apb_pclk";
		};

		ccbtimer1: timer@35000 {
			compatible = "arm,sp804", "arm,primecell";
			reg = <0x35000 0x1000>;
			interrupts = <GIC_SPI 92 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&iprocslow>;
			clock-names = "apb_pclk";
		};

		srab: ethernet-switch@36000 {
			compatible = "brcm,nsp-srab";
			reg = <0x36000 0x1000>,
			      <0x3f308 0x8>,
			      <0x3f410 0xc>;
			reg-names = "srab", "mux_config", "sgmii_config";
			interrupts = <GIC_SPI 95 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 99 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 105 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 106 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 107 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "link_state_p0",
					  "link_state_p1",
					  "link_state_p2",
					  "link_state_p3",
					  "link_state_p4",
					  "link_state_p5",
					  "link_state_p7",
					  "link_state_p8",
					  "phy",
					  "ts",
					  "imp_sleep_timer_p5",
					  "imp_sleep_timer_p7",
					  "imp_sleep_timer_p8";
			status = "disabled";

			/* ports are defined in board DTS */
			ports {
				#address-cells = <1>;
				#size-cells = <0>;
			};
		};

		i2c0: i2c@38000 {
			compatible = "brcm,iproc-i2c";
			reg = <0x38000 0x50>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>;
			clock-frequency = <100000>;
			dma-coherent;
			status = "disabled";
		};

		watchdog@39000 {
			compatible = "arm,sp805", "arm,primecell";
			reg = <0x39000 0x1000>;
			interrupts = <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&iprocslow>, <&iprocslow>;
			clock-names = "wdog_clk", "apb_pclk";
		};

		lcpll0: lcpll0@3f100 {
			#clock-cells = <1>;
			compatible = "brcm,nsp-lcpll0";
			reg = <0x3f100 0x14>;
			clocks = <&osc>;
			clock-output-names = "lcpll0", "pcie_phy", "sdio",
					     "ddr_phy";
		};

		genpll: genpll@3f140 {
			#clock-cells = <1>;
			compatible = "brcm,nsp-genpll";
			reg = <0x3f140 0x24>;
			clocks = <&osc>;
			clock-output-names = "genpll", "phy", "ethernetclk",
					     "usbclk", "iprocfast", "sata1",
					     "sata2";
		};

		pinctrl: pinctrl@3f1c0 {
			compatible = "brcm,nsp-pinmux";
			reg = <0x3f1c0 0x04>,
			      <0x30028 0x04>,
			      <0x3f408 0x04>;
		};

		thermal: thermal@3f2c0 {
			compatible = "brcm,ns-thermal";
			reg = <0x3f2c0 0x10>;
			#thermal-sensor-cells = <0>;
		};

		sata_phy: sata_phy@40100 {
			compatible = "brcm,iproc-nsp-sata-phy";
			reg = <0x40100 0x340>;
			reg-names = "phy";
			#address-cells = <1>;
			#size-cells = <0>;

			sata_phy0: sata-phy@0 {
				reg = <0>;
				#phy-cells = <0>;
				status = "disabled";
			};

			sata_phy1: sata-phy@1 {
				reg = <1>;
				#phy-cells = <0>;
				status = "disabled";
			};
		};

		sata: sata@41000 {
			compatible = "brcm,bcm-nsp-ahci";
			reg-names = "ahci", "top-ctrl";
			reg = <0x41000 0x1000>, <0x40020 0x1c>;
			interrupts = <GIC_SPI 159 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <0>;
			dma-coherent;
			status = "disabled";

			sata0: sata-port@0 {
				reg = <0>;
				phys = <&sata_phy0>;
				phy-names = "sata-phy";
			};

			sata1: sata-port@1 {
				reg = <1>;
				phys = <&sata_phy1>;
				phy-names = "sata-phy";
			};
		};

		usb3_dmp: syscon@104000 {
			reg = <0x104000 0x1000>;
		};
	};

	pcie0: pcie@18012000 {
		compatible = "brcm,iproc-pcie";
		reg = <0x18012000 0x1000>;

		#interrupt-cells = <1>;
		interrupt-map-mask = <0 0 0 0>;
		interrupt-map = <0 0 0 0 &gic GIC_SPI 131 IRQ_TYPE_LEVEL_HIGH>;

		linux,pci-domain = <0>;

		bus-range = <0x00 0xff>;

		#address-cells = <3>;
		#size-cells = <2>;
		device_type = "pci";

		/* Note: The HW does not support I/O resources.  So,
		 * only the memory resource range is being specified.
		 */
		ranges = <0x82000000 0 0x08000000 0x08000000 0 0x8000000>;

		dma-coherent;
		status = "disabled";

		msi-parent = <&msi0>;
		msi0: msi {
			compatible = "brcm,iproc-msi";
			msi-controller;
			interrupt-parent = <&gic>;
			interrupts = <GIC_SPI 127 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 128 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 129 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 130 IRQ_TYPE_LEVEL_HIGH>;
			brcm,pcie-msi-inten;
		};
	};

	pcie1: pcie@18013000 {
		compatible = "brcm,iproc-pcie";
		reg = <0x18013000 0x1000>;

		#interrupt-cells = <1>;
		interrupt-map-mask = <0 0 0 0>;
		interrupt-map = <0 0 0 0 &gic GIC_SPI 137 IRQ_TYPE_LEVEL_HIGH>;

		linux,pci-domain = <1>;

		bus-range = <0x00 0xff>;

		#address-cells = <3>;
		#size-cells = <2>;
		device_type = "pci";

		/* Note: The HW does not support I/O resources.  So,
		 * only the memory resource range is being specified.
		 */
		ranges = <0x82000000 0 0x40000000 0x40000000 0 0x8000000>;

		dma-coherent;
		status = "disabled";

		msi-parent = <&msi1>;
		msi1: msi {
			compatible = "brcm,iproc-msi";
			msi-controller;
			interrupt-parent = <&gic>;
			interrupts = <GIC_SPI 133 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 134 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 135 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 136 IRQ_TYPE_LEVEL_HIGH>;
			brcm,pcie-msi-inten;
		};
	};

	pcie2: pcie@18014000 {
		compatible = "brcm,iproc-pcie";
		reg = <0x18014000 0x1000>;

		#interrupt-cells = <1>;
		interrupt-map-mask = <0 0 0 0>;
		interrupt-map = <0 0 0 0 &gic GIC_SPI 143 IRQ_TYPE_LEVEL_HIGH>;

		linux,pci-domain = <2>;

		bus-range = <0x00 0xff>;

		#address-cells = <3>;
		#size-cells = <2>;
		device_type = "pci";

		/* Note: The HW does not support I/O resources.  So,
		 * only the memory resource range is being specified.
		 */
		ranges = <0x82000000 0 0x48000000 0x48000000 0 0x8000000>;

		dma-coherent;
		status = "disabled";

		msi-parent = <&msi2>;
		msi2: msi {
			compatible = "brcm,iproc-msi";
			msi-controller;
			interrupt-parent = <&gic>;
			interrupts = <GIC_SPI 139 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 140 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 141 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 142 IRQ_TYPE_LEVEL_HIGH>;
			brcm,pcie-msi-inten;
		};
	};

	thermal-zones {
		cpu-thermal {
			polling-delay-passive = <0>;
			polling-delay = <1000>;
			coefficients = <(-556) 418000>;
			thermal-sensors = <&thermal>;

			trips {
				cpu-crit {
					temperature     = <125000>;
					hysteresis      = <0>;
					type            = "critical";
				};
			};

			cooling-maps {
			};
		};
	};
};
