/*
 * support for the imx6 based aristainetos2 board
 *
 * Copyright (C) 2015 Heiko Schocher <hs@denx.de>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License
 *     version 2 as published by the Free Software Foundation.
 *
 *     This file is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */
/dts-v1/;
#include "imx6dl.dtsi"
#include "imx6qdl-aristainetos2.dtsi"

/ {
	model = "aristainetos2 i.MX6 Dual Lite Board 4";
	compatible = "abb,aristainetos2-imx6dl-4", "fsl,imx6dl";

	memory@10000000 {
		device_type = "memory";
		reg = <0x10000000 0x40000000>;
	};

	display0: disp0 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "fsl,imx-parallel-display";
		interface-pix-fmt = "rgb24";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_ipu_disp>;

		port@0 {
			reg = <0>;
			display0_in: endpoint {
				remote-endpoint = <&ipu1_di0_disp0>;
			};
		};

		port@1 {
			reg = <1>;
			display_out: endpoint {
				remote-endpoint = <&panel_in>;
			};
		};
	};
};

&ecspi1 {
	lcd_panel: display@0 {
		compatible = "lg,lg4573";
		spi-max-frequency = <10000000>;
		reg = <0>;

		display-timings {
			native-mode = <&timing0>;
			timing0: timing-480x800p57 {
				clock-frequency = <27000027>;
				hactive = <480>;
				vactive = <800>;
				hfront-porch = <10>;
				hback-porch = <59>;
				hsync-len = <10>;
				vback-porch = <15>;
				vfront-porch = <15>;
				vsync-len = <15>;
				hsync-active = <1>;
				vsync-active = <1>;
			};
		};

		port {
			panel_in: endpoint {
				remote-endpoint = <&display_out>;
			};
		};
	};
};

&i2c3 {
	touch: touch@4b {
		compatible = "atmel,maxtouch";
		reg = <0x4b>;
		interrupt-parent = <&gpio2>;
		interrupts = <9 8>;
	};
};

&ipu1_di0_disp0 {
	remote-endpoint = <&display0_in>;
};

&iomuxc {
	pinctrl_ipu_disp: ipudisp1grp {
		fsl,pins = <
			MX6QDL_PAD_DI0_DISP_CLK__IPU1_DI0_DISP_CLK 0x31
			MX6QDL_PAD_DI0_PIN15__IPU1_DI0_PIN15       0xE1
			MX6QDL_PAD_DI0_PIN2__IPU1_DI0_PIN02        0x10
			MX6QDL_PAD_DI0_PIN3__IPU1_DI0_PIN03        0x10
			MX6QDL_PAD_DISP0_DAT0__IPU1_DISP0_DATA00   0xE1
			MX6QDL_PAD_DISP0_DAT1__IPU1_DISP0_DATA01   0xE1
			MX6QDL_PAD_DISP0_DAT2__IPU1_DISP0_DATA02   0xE1
			MX6QDL_PAD_DISP0_DAT3__IPU1_DISP0_DATA03   0xE1
			MX6QDL_PAD_DISP0_DAT4__IPU1_DISP0_DATA04   0xE1
			MX6QDL_PAD_DISP0_DAT5__IPU1_DISP0_DATA05   0xE1
			MX6QDL_PAD_DISP0_DAT6__IPU1_DISP0_DATA06   0xE1
			MX6QDL_PAD_DISP0_DAT7__IPU1_DISP0_DATA07   0xE1
			MX6QDL_PAD_DISP0_DAT8__IPU1_DISP0_DATA08   0xE1
			MX6QDL_PAD_DISP0_DAT9__IPU1_DISP0_DATA09   0xE1
			MX6QDL_PAD_DISP0_DAT10__IPU1_DISP0_DATA10  0xE1
			MX6QDL_PAD_DISP0_DAT11__IPU1_DISP0_DATA11  0xE1
			MX6QDL_PAD_DISP0_DAT12__IPU1_DISP0_DATA12  0xE1
			MX6QDL_PAD_DISP0_DAT13__IPU1_DISP0_DATA13  0xE1
			MX6QDL_PAD_DISP0_DAT14__IPU1_DISP0_DATA14  0xe1
			MX6QDL_PAD_DISP0_DAT15__IPU1_DISP0_DATA15  0xE1
			MX6QDL_PAD_DISP0_DAT16__IPU1_DISP0_DATA16  0xE1
			MX6QDL_PAD_DISP0_DAT17__IPU1_DISP0_DATA17  0xE1
			MX6QDL_PAD_DISP0_DAT18__IPU1_DISP0_DATA18  0xE1
			MX6QDL_PAD_DISP0_DAT19__IPU1_DISP0_DATA19  0xE1
			MX6QDL_PAD_DISP0_DAT20__IPU1_DISP0_DATA20  0xE1
			MX6QDL_PAD_DISP0_DAT21__IPU1_DISP0_DATA21  0xE1
			MX6QDL_PAD_DISP0_DAT22__IPU1_DISP0_DATA22  0xE1
			MX6QDL_PAD_DISP0_DAT23__IPU1_DISP0_DATA23  0xE1
		>;
	};
};
