// SPDX-License-Identifier: GPL-2.0-only
/*
 * Copyright (C) 2013 Texas Instruments Incorporated - https://www.ti.com/
 */

/* AM43x EPOS EVM */

/dts-v1/;

#include "am4372.dtsi"
#include <dt-bindings/pinctrl/am43xx.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pwm/pwm.h>
#include <dt-bindings/sound/tlv320aic31xx.h>

/ {
	model = "TI AM43x EPOS EVM";
	compatible = "ti,am43x-epos-evm","ti,am438x","ti,am43";

	aliases {
		display0 = &lcd0;
	};

	chosen {
		stdout-path = &uart0;
	};

	vmmcsd_fixed: fixedregulator-sd {
		compatible = "regulator-fixed";
		regulator-name = "vmmcsd_fixed";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		enable-active-high;
	};

	vbat: fixedregulator0 {
		compatible = "regulator-fixed";
		regulator-name = "vbat";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-boot-on;
	};

	lcd0: display {
		compatible = "osddisplays,osd070t1718-19ts", "panel-dpi";
		label = "lcd";

		backlight = <&lcd_bl>;

		port {
			lcd_in: endpoint {
				remote-endpoint = <&dpi_out>;
			};
		};
	};

	matrix_keypad: matrix_keypad0 {
		compatible = "gpio-matrix-keypad";
		debounce-delay-ms = <5>;
		col-scan-delay-us = <2>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&matrix_keypad_default>;
		pinctrl-1 = <&matrix_keypad_sleep>;
		wakeup-source;

		row-gpios = <&gpio0 12 GPIO_ACTIVE_HIGH		/* Bank0, pin12 */
			     &gpio0 13 GPIO_ACTIVE_HIGH		/* Bank0, pin13 */
			     &gpio0 14 GPIO_ACTIVE_HIGH		/* Bank0, pin14 */
			     &gpio0 15 GPIO_ACTIVE_HIGH>;	/* Bank0, pin15 */

		col-gpios = <&gpio3 9 GPIO_ACTIVE_HIGH		/* Bank3, pin9 */
			     &gpio3 10 GPIO_ACTIVE_HIGH		/* Bank3, pin10 */
			     &gpio2 18 GPIO_ACTIVE_HIGH		/* Bank2, pin18 */
			     &gpio2 19 GPIO_ACTIVE_HIGH>;	/* Bank2, pin19 */

		linux,keymap = <0x00000201	/* P1 */
			0x01000204	/* P4 */
			0x02000207	/* P7 */
			0x0300020a	/* NUMERIC_STAR */
			0x00010202	/* P2 */
			0x01010205	/* P5 */
			0x02010208	/* P8 */
			0x03010200	/* P0 */
			0x00020203	/* P3 */
			0x01020206	/* P6 */
			0x02020209	/* P9 */
			0x0302020b	/* NUMERIC_POUND */
			0x00030067	/* UP */
			0x0103006a	/* RIGHT */
			0x0203006c	/* DOWN */
			0x03030069>;	/* LEFT */
	};

	lcd_bl: backlight {
		compatible = "pwm-backlight";
		pwms = <&ecap0 0 50000 PWM_POLARITY_INVERTED>;
		brightness-levels = <0 51 53 56 62 75 101 152 255>;
		default-brightness-level = <8>;
	};

	sound0: sound0 {
		compatible = "simple-audio-card";
		simple-audio-card,name = "AM43-EPOS-EVM";
		simple-audio-card,widgets =
			"Microphone", "Microphone Jack",
			"Headphone", "Headphone Jack",
			"Speaker", "Speaker";
		simple-audio-card,routing =
			"MIC1LP", "Microphone Jack",
			"MIC1RP", "Microphone Jack",
			"MIC1LP", "MICBIAS",
			"MIC1RP", "MICBIAS",
			"Headphone Jack", "HPL",
			"Headphone Jack", "HPR",
			"Speaker", "SPL",
			"Speaker", "SPR";
		simple-audio-card,format = "dsp_b";
		simple-audio-card,bitclock-master = <&sound0_master>;
		simple-audio-card,frame-master = <&sound0_master>;
		simple-audio-card,bitclock-inversion;

		simple-audio-card,cpu {
			sound-dai = <&mcasp1>;
			system-clock-frequency = <12000000>;
		};

		sound0_master: simple-audio-card,codec {
			sound-dai = <&tlv320aic3111>;
			system-clock-frequency = <12000000>;
		};
	};

	audio_mstrclk: clock {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <12000000>;
	};
};

&am43xx_pinmux {
		pinctrl-names = "default";
		pinctrl-0 = <&unused_pins>;

		unused_pins: unused-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x848, DS0_PIN_OUTPUT_PULLUP | PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x850, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x858, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x860, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x864, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x868, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x86c, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x878, DS0_PIN_OUTPUT_PULLUP | PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x908, DS0_PIN_INPUT_PULLDOWN | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x91c, DS0_PIN_OUTPUT_PULLDOWN | PIN_OUTPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x920, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x9e0, DS0_PIN_INPUT_PULLDOWN | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA0c, DS0_PIN_OUTPUT_PULLDOWN | PIN_OUTPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA38, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA3c, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA40, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA44, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA48, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA4c, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA50, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA54, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA58, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA5c, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA60, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA64, DS0_PIN_OUTPUT_PULLUP | PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0xA68, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA6C, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA74, DS0_PIN_INPUT_PULLDOWN | PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0xA78, DS0_PIN_INPUT | PIN_INPUT_PULLDOWN | MUX_MODE7)
			>;
		};

		cpsw_default: cpsw-default-pins {
			pinctrl-single,pins = <
				/* Slave 1 */
				AM4372_IOPAD(0x90c, PIN_INPUT_PULLDOWN | MUX_MODE1)	/* mii1_crs.rmii1_crs */
				AM4372_IOPAD(0x910, PIN_INPUT_PULLDOWN | MUX_MODE1)	/* mii1_rxerr.rmii1_rxerr */
				AM4372_IOPAD(0x914, PIN_OUTPUT_PULLDOWN | MUX_MODE1)	/* mii1_txen.rmii1_txen */
				AM4372_IOPAD(0x918, PIN_INPUT_PULLDOWN | MUX_MODE1)	/* mii1_rxdv.rmii1_rxdv */
				AM4372_IOPAD(0x924, PIN_OUTPUT_PULLDOWN | MUX_MODE1)	/* mii1_txd1.rmii1_txd1 */
				AM4372_IOPAD(0x928, PIN_OUTPUT_PULLDOWN | MUX_MODE1)	/* mii1_txd0.rmii1_txd0 */
				AM4372_IOPAD(0x93c, PIN_INPUT_PULLDOWN | MUX_MODE1)	/* mii1_rxd1.rmii1_rxd1 */
				AM4372_IOPAD(0x940, PIN_INPUT_PULLDOWN | MUX_MODE1)	/* mii1_rxd0.rmii1_rxd0 */
				AM4372_IOPAD(0x944, PIN_INPUT_PULLDOWN | MUX_MODE0)	/* rmii1_refclk.rmii1_refclk */
			>;
		};

		cpsw_sleep: cpsw-sleep-pins {
			pinctrl-single,pins = <
				/* Slave 1 reset value */
				AM4372_IOPAD(0x90c, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x910, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x914, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x918, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x924, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x928, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x93c, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x940, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x944, PIN_INPUT_PULLDOWN | MUX_MODE7)
			>;
		};

		davinci_mdio_default: davinci-mdio-default-pins {
			pinctrl-single,pins = <
				/* MDIO */
				AM4372_IOPAD(0x948, PIN_INPUT_PULLUP | SLEWCTRL_FAST | MUX_MODE0)	/* mdio_data.mdio_data */
				AM4372_IOPAD(0x94c, PIN_OUTPUT_PULLUP | MUX_MODE0)			/* mdio_clk.mdio_clk */
			>;
		};

		davinci_mdio_sleep: davinci-mdio-sleep-pins {
			pinctrl-single,pins = <
				/* MDIO reset value */
				AM4372_IOPAD(0x948, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x94c, PIN_INPUT_PULLDOWN | MUX_MODE7)
			>;
		};

		i2c0_pins: i2c0-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x988, PIN_INPUT_PULLUP | SLEWCTRL_FAST | MUX_MODE0)	/* i2c0_sda.i2c0_sda */
				AM4372_IOPAD(0x98c, PIN_INPUT_PULLUP | SLEWCTRL_FAST | MUX_MODE0)	/* i2c0_scl.i2c0_scl */
			>;
		};

		nand_flash_x8_default: nand-flash-x8-default-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x840, PIN_OUTPUT_PULLDOWN | MUX_MODE7)	/* gpmc_a0.SELQSPIorNAND/GPIO */
				AM4372_IOPAD(0x800, PIN_INPUT_PULLDOWN | MUX_MODE0)	/* gpmc_ad0.gpmc_ad0 */
				AM4372_IOPAD(0x804, PIN_INPUT_PULLDOWN | MUX_MODE0)	/* gpmc_ad1.gpmc_ad1 */
				AM4372_IOPAD(0x808, PIN_INPUT_PULLDOWN | MUX_MODE0)	/* gpmc_ad2.gpmc_ad2 */
				AM4372_IOPAD(0x80c, PIN_INPUT_PULLDOWN | MUX_MODE0)	/* gpmc_ad3.gpmc_ad3 */
				AM4372_IOPAD(0x810, PIN_INPUT_PULLDOWN | MUX_MODE0)	/* gpmc_ad4.gpmc_ad4 */
				AM4372_IOPAD(0x814, PIN_INPUT_PULLDOWN | MUX_MODE0)	/* gpmc_ad5.gpmc_ad5 */
				AM4372_IOPAD(0x818, PIN_INPUT_PULLDOWN | MUX_MODE0)	/* gpmc_ad6.gpmc_ad6 */
				AM4372_IOPAD(0x81c, PIN_INPUT_PULLDOWN | MUX_MODE0)	/* gpmc_ad7.gpmc_ad7 */
				AM4372_IOPAD(0x870, PIN_INPUT_PULLUP | MUX_MODE0)	/* gpmc_wait0.gpmc_wait0 */
				AM4372_IOPAD(0x874, PIN_OUTPUT_PULLUP | MUX_MODE7)	/* gpmc_wpn.gpmc_wpn */
				AM4372_IOPAD(0x87c, PIN_OUTPUT | MUX_MODE0)		/* gpmc_csn0.gpmc_csn0  */
				AM4372_IOPAD(0x890, PIN_OUTPUT | MUX_MODE0)		/* gpmc_advn_ale.gpmc_advn_ale */
				AM4372_IOPAD(0x894, PIN_OUTPUT | MUX_MODE0)		/* gpmc_oen_ren.gpmc_oen_ren */
				AM4372_IOPAD(0x898, PIN_OUTPUT | MUX_MODE0)		/* gpmc_wen.gpmc_wen */
				AM4372_IOPAD(0x89c, PIN_OUTPUT | MUX_MODE0)		/* gpmc_be0n_cle.gpmc_be0n_cle */
			>;
		};

		nand_flash_x8_sleep: nand-flash-x8-sleep-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x840, DS0_PIN_OUTPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x800, DS0_PIN_OUTPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x804, DS0_PIN_OUTPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x808, DS0_PIN_OUTPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x80c, DS0_PIN_OUTPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x810, DS0_PIN_OUTPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x814, DS0_PIN_OUTPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x818, DS0_PIN_OUTPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x81c, DS0_PIN_OUTPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x870, DS0_PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x874, DS0_PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x87c, DS0_PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x890, DS0_PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x894, DS0_PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x898, DS0_PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x89c, DS0_PIN_OUTPUT_PULLUP | MUX_MODE7)
			>;
		};

		ecap0_pins_default: backlight-default-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x964, MUX_MODE0)         /* eCAP0_in_PWM0_out.eCAP0_in_PWM0_out MODE0 */
			>;
		};

		ecap0_pins_sleep: backlight-sleep-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x964, DS0_PIN_OUTPUT_PULLUP | MUX_MODE7)
			>;
		};

		i2c2_pins: i2c2-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x9c0, PIN_INPUT_PULLUP | SLEWCTRL_FAST | MUX_MODE8)    /* i2c2_sda.i2c2_sda */
				AM4372_IOPAD(0x9c4, PIN_INPUT_PULLUP | SLEWCTRL_FAST | MUX_MODE8)    /* i2c2_scl.i2c2_scl */
			>;
		};

		spi0_pins_default: spi0-default-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x950, PIN_INPUT | MUX_MODE0)           /* spi0_clk.spi0_clk */
				AM4372_IOPAD(0x954, PIN_OUTPUT | MUX_MODE0)           /* spi0_d0.spi0_d0 */
				AM4372_IOPAD(0x958, PIN_INPUT | MUX_MODE0)           /* spi0_d1.spi0_d1 */
				AM4372_IOPAD(0x95c, PIN_OUTPUT | MUX_MODE0)          /* spi0_cs0.spi0_cs0 */
			>;
		};

		spi0_pins_sleep: spi0-sleep-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x950, DS0_PIN_OUTPUT_PULLUP | PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x954, DS0_PIN_OUTPUT_PULLUP | PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x958, DS0_PIN_OUTPUT_PULLUP | PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x95c, DS0_PIN_OUTPUT_PULLUP | PIN_OUTPUT_PULLUP | MUX_MODE7)
			>;
		};

		spi1_pins_default: spi1-default-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x990, PIN_INPUT | MUX_MODE3)           /* mcasp0_aclkx.spi1_clk */
				AM4372_IOPAD(0x994, PIN_OUTPUT | MUX_MODE3)           /* mcasp0_fsx.spi1_d0 */
				AM4372_IOPAD(0x998, PIN_INPUT | MUX_MODE3)           /* mcasp0_axr0.spi1_d1 */
				AM4372_IOPAD(0x99c, PIN_OUTPUT | MUX_MODE3)          /* mcasp0_ahclkr.spi1_cs0 */
			>;
		};

		spi1_pins_sleep: spi1-sleep-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x990, DS0_PIN_OUTPUT_PULLDOWN | PIN_OUTPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x994, DS0_PIN_OUTPUT_PULLDOWN | PIN_OUTPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x998, DS0_PIN_OUTPUT_PULLDOWN | PIN_OUTPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x99c, DS0_PIN_OUTPUT_PULLDOWN | PIN_OUTPUT_PULLDOWN | MUX_MODE7)
			>;
		};

		mmc1_pins_default: mmc1-default-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x960, PIN_INPUT | MUX_MODE7) /* spi0_cs1.gpio0_6 */
			>;
		};

		mmc1_pins_sleep: mmc1-sleep-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x960, DS0_PIN_OUTPUT_PULLUP | PIN_INPUT | MUX_MODE7)
			>;
		};

		matrix_keypad_default: matrix-keypad-default-pins {
			pinctrl-single,pins = <
				 AM4372_IOPAD(0x92c, PIN_OUTPUT | MUX_MODE7)          /* mii1_tx_clk.gpio3_9 */
				 AM4372_IOPAD(0x930, PIN_OUTPUT | MUX_MODE7)          /* mii1_rx_clk.gpio3_10 */
				 AM4372_IOPAD(0x934, PIN_OUTPUT | MUX_MODE7)          /* mii1_rxd3.gpio2_18 */
				 AM4372_IOPAD(0x938, PIN_OUTPUT | MUX_MODE7)          /* mii1_rxd2.gpio2_19 */
				 AM4372_IOPAD(0x978, PIN_INPUT_PULLDOWN | MUX_MODE7)  /* uart1_ctsn.gpio0_12 */
				 AM4372_IOPAD(0x97C, PIN_INPUT_PULLDOWN | MUX_MODE7)  /* uart1_rtsn.gpio0_13 */
				 AM4372_IOPAD(0x980, PIN_INPUT_PULLDOWN | MUX_MODE7)  /* uart1_rxd.gpio0_14 */
				 AM4372_IOPAD(0x984, PIN_INPUT_PULLDOWN | MUX_MODE7)  /* uart1_txd.gpio0_15 */
			>;
		};

		matrix_keypad_sleep: matrix-keypad-sleep-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x92c, PIN_INPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x930, PIN_INPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x934, PIN_INPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x938, PIN_INPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x978, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x97C, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x980, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x984, PIN_INPUT_PULLDOWN | MUX_MODE7)
			>;
		};

		qspi1_pins_default: qspi1-default-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x87c, PIN_INPUT_PULLUP | MUX_MODE3)
				AM4372_IOPAD(0x888, PIN_INPUT_PULLUP | MUX_MODE2)
				AM4372_IOPAD(0x890, PIN_INPUT_PULLUP | MUX_MODE3)
				AM4372_IOPAD(0x894, PIN_INPUT_PULLUP | MUX_MODE3)
				AM4372_IOPAD(0x898, PIN_INPUT_PULLUP | MUX_MODE3)
				AM4372_IOPAD(0x89c, PIN_INPUT_PULLUP | MUX_MODE3)
			>;
		};

		qspi1_pins_sleep: qspi1-sleep-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x87c, DS0_PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x888, DS0_PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x890, DS0_PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x894, DS0_PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x898, DS0_PIN_OUTPUT_PULLUP | MUX_MODE7)
				AM4372_IOPAD(0x89c, DS0_PIN_OUTPUT_PULLUP | MUX_MODE7)
			>;
		};

		pixcir_ts_pins_default: pixcir-ts-default-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x844, PIN_INPUT_PULLUP | MUX_MODE7)	/* gpmc_a1.gpio1_17 */
			>;
		};

		pixcir_ts_pins_sleep: pixcir-ts-sleep-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x844, DS0_PIN_OUTPUT_PULLUP | PIN_OUTPUT_PULLUP | MUX_MODE7)	/* gpmc_a1.gpio1_17 */
			>;
		};

		hdq_pins: hdq-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0xa34, PIN_INPUT_PULLUP | MUX_MODE1)    /* cam1_wen.hdq_gpio */
			>;
		};

		dss_pins: dss-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x820, PIN_OUTPUT_PULLUP | MUX_MODE1) /*gpmc ad 8 -> DSS DATA 23 */
				AM4372_IOPAD(0x824, PIN_OUTPUT_PULLUP | MUX_MODE1)
				AM4372_IOPAD(0x828, PIN_OUTPUT_PULLUP | MUX_MODE1)
				AM4372_IOPAD(0x82c, PIN_OUTPUT_PULLUP | MUX_MODE1)
				AM4372_IOPAD(0x830, PIN_OUTPUT_PULLUP | MUX_MODE1)
				AM4372_IOPAD(0x834, PIN_OUTPUT_PULLUP | MUX_MODE1)
				AM4372_IOPAD(0x838, PIN_OUTPUT_PULLUP | MUX_MODE1)
				AM4372_IOPAD(0x83c, PIN_OUTPUT_PULLUP | MUX_MODE1) /*gpmc ad 15 -> DSS DATA 16 */
				AM4372_IOPAD(0x8a0, PIN_OUTPUT_PULLUP | MUX_MODE0) /* DSS DATA 0 */
				AM4372_IOPAD(0x8a4, PIN_OUTPUT_PULLUP | MUX_MODE0)
				AM4372_IOPAD(0x8a8, PIN_OUTPUT_PULLUP | MUX_MODE0)
				AM4372_IOPAD(0x8ac, PIN_OUTPUT_PULLUP | MUX_MODE0)
				AM4372_IOPAD(0x8b0, PIN_OUTPUT_PULLUP | MUX_MODE0)
				AM4372_IOPAD(0x8b4, PIN_OUTPUT_PULLUP | MUX_MODE0)
				AM4372_IOPAD(0x8B8, PIN_OUTPUT_PULLUP | MUX_MODE0)
				AM4372_IOPAD(0x8bc, PIN_OUTPUT_PULLUP | MUX_MODE0)
				AM4372_IOPAD(0x8c0, PIN_OUTPUT_PULLUP | MUX_MODE0)
				AM4372_IOPAD(0x8c4, PIN_OUTPUT_PULLUP | MUX_MODE0)
				AM4372_IOPAD(0x8c8, PIN_OUTPUT_PULLUP | MUX_MODE0)
				AM4372_IOPAD(0x8cc, PIN_OUTPUT_PULLUP | MUX_MODE0)
				AM4372_IOPAD(0x8d0, PIN_OUTPUT_PULLUP | MUX_MODE0)
				AM4372_IOPAD(0x8d4, PIN_OUTPUT_PULLUP | MUX_MODE0)
				AM4372_IOPAD(0x8d8, PIN_OUTPUT_PULLUP | MUX_MODE0)
				AM4372_IOPAD(0x8dc, PIN_OUTPUT_PULLUP | MUX_MODE0) /* DSS DATA 15 */
				AM4372_IOPAD(0x8e0, PIN_OUTPUT_PULLUP | MUX_MODE0) /* DSS VSYNC */
				AM4372_IOPAD(0x8e4, PIN_OUTPUT_PULLUP | MUX_MODE0) /* DSS HSYNC */
				AM4372_IOPAD(0x8e8, PIN_OUTPUT_PULLUP | MUX_MODE0) /* DSS PCLK */
				AM4372_IOPAD(0x8ec, PIN_OUTPUT_PULLUP | MUX_MODE0) /* DSS AC BIAS EN */
			>;
		};

		display_mux_pins: display-mux-pins {
			pinctrl-single,pins = <
				/* GPMC CLK -> GPIO 2_1 to select LCD / HDMI */
				AM4372_IOPAD(0x88C, PIN_OUTPUT_PULLUP | MUX_MODE7)
			>;
		};

		vpfe1_pins_default: vpfe1-default-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x9cc, PIN_INPUT_PULLUP | MUX_MODE0)  /* cam1_data9 mode 0 */
				AM4372_IOPAD(0x9d0, PIN_INPUT_PULLUP | MUX_MODE0)  /* cam1_data8 mode 0 */
				AM4372_IOPAD(0x9d4, PIN_INPUT_PULLUP | MUX_MODE0)  /* cam1_hd mode 0 */
				AM4372_IOPAD(0x9d8, PIN_INPUT_PULLUP | MUX_MODE0)  /* cam1_vd mode 0 */
				AM4372_IOPAD(0x9dc, PIN_INPUT_PULLUP | MUX_MODE0)  /* cam1_pclk mode 0 */
				AM4372_IOPAD(0x9e8, PIN_INPUT_PULLUP | MUX_MODE0)  /* cam1_data0 mode 0 */
				AM4372_IOPAD(0x9ec, PIN_INPUT_PULLUP | MUX_MODE0)  /* cam1_data1 mode 0 */
				AM4372_IOPAD(0x9f0, PIN_INPUT_PULLUP | MUX_MODE0)  /* cam1_data2 mode 0 */
				AM4372_IOPAD(0x9f4, PIN_INPUT_PULLUP | MUX_MODE0)  /* cam1_data3 mode 0 */
				AM4372_IOPAD(0x9f8, PIN_INPUT_PULLUP | MUX_MODE0)  /* cam1_data4 mode 0 */
				AM4372_IOPAD(0x9fc, PIN_INPUT_PULLUP | MUX_MODE0)  /* cam1_data5 mode 0 */
				AM4372_IOPAD(0xa00, PIN_INPUT_PULLUP | MUX_MODE0)  /* cam1_data6 mode 0 */
				AM4372_IOPAD(0xa04, PIN_INPUT_PULLUP | MUX_MODE0)  /* cam1_data7 mode 0 */
			>;
		};

		vpfe1_pins_sleep: vpfe1-sleep-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x9cc, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
				AM4372_IOPAD(0x9d0, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
				AM4372_IOPAD(0x9d4, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
				AM4372_IOPAD(0x9d8, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
				AM4372_IOPAD(0x9dc, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
				AM4372_IOPAD(0x9e8, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
				AM4372_IOPAD(0x9ec, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
				AM4372_IOPAD(0x9f0, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
				AM4372_IOPAD(0x9f4, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
				AM4372_IOPAD(0x9f8, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
				AM4372_IOPAD(0x9fc, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
				AM4372_IOPAD(0xa00, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
				AM4372_IOPAD(0xa04, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
			>;
		};

		uart0_pins_default: uart0-default-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x968, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE0) /* uart0_ctsn.uart0_ctsn */
				AM4372_IOPAD(0x96C, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE0) /* uart0_rtsn.uart0_rtsn */
				AM4372_IOPAD(0x970, PIN_INPUT_PULLUP | SLEWCTRL_FAST | DS0_PULL_UP_DOWN_EN | MUX_MODE0)	/* uart0_rxd.uart0_rxd */
				AM4372_IOPAD(0x974, PIN_INPUT | SLEWCTRL_FAST | DS0_PULL_UP_DOWN_EN | MUX_MODE0)	/* uart0_txd.uart0_txd */
			>;
		};

		uart0_pins_sleep: uart0-sleep-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x968, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
				AM4372_IOPAD(0x96C, DS0_PULL_UP_DOWN_EN | INPUT_EN | MUX_MODE7)
				AM4372_IOPAD(0x970, PIN_INPUT_PULLUP | SLEWCTRL_FAST | DS0_PULL_UP_DOWN_EN | MUX_MODE0)
				AM4372_IOPAD(0x974, PIN_INPUT | SLEWCTRL_FAST | DS0_PULL_UP_DOWN_EN | MUX_MODE0)
			>;
		};

		usb2_phy1_default: usb2-phy1-default-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0xac0, PIN_INPUT_PULLDOWN | MUX_MODE0)
			>;
		};

		usb2_phy1_sleep: usb2-phy1-sleep-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0xac0, DS0_PULL_UP_DOWN_EN | PIN_INPUT_PULLDOWN | MUX_MODE7)
			>;
		};

		usb2_phy2_default: usb2-phy2-default-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0xac4, PIN_INPUT_PULLDOWN | MUX_MODE0)
			>;
		};

		usb2_phy2_sleep: usb2-phy2-sleep-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0xac4, DS0_PULL_UP_DOWN_EN | PIN_INPUT_PULLDOWN | MUX_MODE7)
			>;
		};

		mcasp1_pins: mcasp1-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x9a0, PIN_INPUT_PULLDOWN | MUX_MODE3) /* MCASP0_ACLKR/MCASP1_ACLKX */
				AM4372_IOPAD(0x9a4, PIN_INPUT_PULLDOWN | MUX_MODE3) /* MCASP0_FSR/MCASP1_FSX */
				AM4372_IOPAD(0x9a8, PIN_OUTPUT_PULLDOWN | MUX_MODE3)/* MCASP0_AXR1/MCASP1_AXR0 */
				AM4372_IOPAD(0x9ac, PIN_INPUT_PULLDOWN | MUX_MODE3) /* MCASP0_AHCLKX/MCASP1_AXR1 */
			>;
		};

		mcasp1_sleep_pins: mcasp1-sleep-pins {
			pinctrl-single,pins = <
				AM4372_IOPAD(0x9a0, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x9a4, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x9a8, PIN_INPUT_PULLDOWN | MUX_MODE7)
				AM4372_IOPAD(0x9ac, PIN_INPUT_PULLDOWN | MUX_MODE7)
			>;
		};
};

&mmc1 {
	status = "okay";
	vmmc-supply = <&vmmcsd_fixed>;
	bus-width = <4>;
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&mmc1_pins_default>;
	pinctrl-1 = <&mmc1_pins_sleep>;
	cd-gpios = <&gpio0 6 GPIO_ACTIVE_LOW>;
};

&mac_sw {
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&cpsw_default>;
	pinctrl-1 = <&cpsw_sleep>;
	status = "okay";
};

&davinci_mdio_sw {
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&davinci_mdio_default>;
	pinctrl-1 = <&davinci_mdio_sleep>;

	ethphy0: ethernet-phy@16 {
		reg = <16>;
	};
};

&cpsw_port1 {
	phy-handle = <&ethphy0>;
	phy-mode = "rmii";
	phys = <&phy_gmii_sel 1 1>;
	ti,dual-emac-pvid = <1>;
};

&cpsw_port2 {
	status = "disabled";
};

&i2c0 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0_pins>;
	clock-frequency = <100000>;

	tps65218: tps65218@24 {
		reg = <0x24>;
		compatible = "ti,tps65218";
		interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>; /* NMIn */
		interrupt-controller;
		#interrupt-cells = <2>;

		dcdc1: regulator-dcdc1 {
			regulator-name = "vdd_core";
			regulator-min-microvolt = <912000>;
			regulator-max-microvolt = <1144000>;
			regulator-boot-on;
			regulator-always-on;
		};

		dcdc2: regulator-dcdc2 {
			regulator-name = "vdd_mpu";
			regulator-min-microvolt = <912000>;
			regulator-max-microvolt = <1378000>;
			regulator-boot-on;
			regulator-always-on;
		};

		dcdc3: regulator-dcdc3 {
			regulator-name = "vdcdc3";
			regulator-boot-on;
			regulator-always-on;
			regulator-state-mem {
				regulator-on-in-suspend;
			};
			regulator-state-disk {
				regulator-off-in-suspend;
			};
		};

		dcdc4: regulator-dcdc4 {
			regulator-name = "vdcdc4";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			regulator-boot-on;
			regulator-always-on;
		};

		dcdc5: regulator-dcdc5 {
			regulator-name = "v1_0bat";
			regulator-min-microvolt = <1000000>;
			regulator-max-microvolt = <1000000>;
			regulator-boot-on;
			regulator-always-on;
		};

		dcdc6: regulator-dcdc6 {
			regulator-name = "v1_8bat";
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1800000>;
			regulator-boot-on;
			regulator-always-on;
		};

		ldo1: regulator-ldo1 {
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1800000>;
			regulator-boot-on;
			regulator-always-on;
		};
	};

	at24@50 {
		compatible = "atmel,24c256";
		pagesize = <64>;
		reg = <0x50>;
	};

	pixcir_ts@5c {
		compatible = "pixcir,pixcir_tangoc";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&pixcir_ts_pins_default>;
		pinctrl-1 = <&pixcir_ts_pins_sleep>;

		reg = <0x5c>;
		interrupt-parent = <&gpio1>;
		interrupts = <17 IRQ_TYPE_EDGE_FALLING>;

		attb-gpio = <&gpio1 17 GPIO_ACTIVE_HIGH>;

		touchscreen-size-x = <1024>;
		touchscreen-size-y = <600>;
	};

	tlv320aic3111: tlv320aic3111@18 {
		#sound-dai-cells = <0>;
		compatible = "ti,tlv320aic3111";
		reg = <0x18>;
		status = "okay";

		ai31xx-micbias-vg = <MICBIAS_2_0V>;

		/* Regulators */
		HPVDD-supply = <&dcdc4>; /* v3_3AUD -> V3_3D -> DCDC4 */
		SPRVDD-supply = <&vbat>; /* vbat */
		SPLVDD-supply = <&vbat>; /* vbat */
		AVDD-supply = <&dcdc4>; /* v3_3AUD -> V3_3D -> DCDC4 */
		IOVDD-supply = <&dcdc4>; /* V3_3D -> DCDC4 */
		DVDD-supply = <&ldo1>; /* V1_8AUD -> V1_8D -> LDO1 */
	};

	ov2659@30 {
		compatible = "ovti,ov2659";
		reg = <0x30>;

		clocks = <&audio_mstrclk>;
		clock-names = "xvclk";

		port {
			ov2659_1: endpoint {
				remote-endpoint = <&vpfe1_ep>;
				link-frequencies = /bits/ 64 <70000000>;
			};
		};
	};
};

&i2c2 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c2_pins>;
	status = "okay";
};

&gpio0 {
	status = "okay";
};

&gpio1 {
	status = "okay";
};

&gpio2 {
	pinctrl-names = "default";
	pinctrl-0 = <&display_mux_pins>;
	status = "okay";

	sel-lcd-hdmi-hog {
		/*
		 * SelLCDorHDMI selects between display and audio paths:
		 * Low: HDMI display with audio via HDMI
		 * High: LCD display with analog audio via aic3111 codec
		 */
		gpio-hog;
		gpios = <1 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "SelLCDorHDMI";
	};
};

&gpio3 {
	status = "okay";
};

&elm {
	status = "okay";
};

&gpmc {
	status = "okay";	/* Disable QSPI when enabling GPMC (NAND) */
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&nand_flash_x8_default>;
	pinctrl-1 = <&nand_flash_x8_sleep>;
	ranges = <0 0 0x08000000 0x01000000>;	/* CS0 space. Min partition = 16MB */
	nand@0,0 {
		compatible = "ti,omap2-nand";
		reg = <0 0 4>; /* CS0, offset 0, IO size 4 */
		interrupt-parent = <&gpmc>;
		interrupts = <0 IRQ_TYPE_NONE>, /* fifoevent */
			     <1 IRQ_TYPE_NONE>;	/* termcount */
		rb-gpios = <&gpmc 0 GPIO_ACTIVE_HIGH>;	/* gpmc_wait0 */
		ti,nand-xfer-type = "prefetch-dma";
		ti,nand-ecc-opt = "bch16";
		ti,elm-id = <&elm>;
		nand-bus-width = <8>;
		gpmc,device-width = <1>;
		gpmc,sync-clk-ps = <0>;
		gpmc,cs-on-ns = <0>;
		gpmc,cs-rd-off-ns = <40>; /* tCEA + tCHZ + 1 */
		gpmc,cs-wr-off-ns = <40>;
		gpmc,adv-on-ns = <0>;  /* cs-on-ns */
		gpmc,adv-rd-off-ns = <25>; /* min( tALH + tALS + 1) */
		gpmc,adv-wr-off-ns = <25>; /* min( tALH + tALS + 1) */
		gpmc,we-on-ns = <0>;   /* cs-on-ns */
		gpmc,we-off-ns = <20>; /* we-on-time + tWP + 2 */
		gpmc,oe-on-ns = <3>;  /* cs-on-ns + tRR + 2 */
		gpmc,oe-off-ns = <30>; /* oe-on-ns + tRP + 2 */
		gpmc,access-ns = <30>; /* tCEA + 4*/
		gpmc,rd-cycle-ns = <40>;
		gpmc,wr-cycle-ns = <40>;
		gpmc,bus-turnaround-ns = <0>;
		gpmc,cycle2cycle-delay-ns = <0>;
		gpmc,clk-activation-ns = <0>;
		gpmc,wr-access-ns = <40>;
		gpmc,wr-data-mux-bus-ns = <0>;
		/* MTD partition table */
		/* All SPL-* partitions are sized to minimal length
		 * which can be independently programmable. For
		 * NAND flash this is equal to size of erase-block */
		#address-cells = <1>;
		#size-cells = <1>;
		partition@0 {
			label = "NAND.SPL";
			reg = <0x00000000 0x00040000>;
		};
		partition@1 {
			label = "NAND.SPL.backup1";
			reg = <0x00040000 0x00040000>;
		};
		partition@2 {
			label = "NAND.SPL.backup2";
			reg = <0x00080000 0x00040000>;
		};
		partition@3 {
			label = "NAND.SPL.backup3";
			reg = <0x000C0000 0x00040000>;
		};
		partition@4 {
			label = "NAND.u-boot-spl-os";
			reg = <0x00100000 0x00080000>;
		};
		partition@5 {
			label = "NAND.u-boot";
			reg = <0x00180000 0x00100000>;
		};
		partition@6 {
			label = "NAND.u-boot-env";
			reg = <0x00280000 0x00040000>;
		};
		partition@7 {
			label = "NAND.u-boot-env.backup1";
			reg = <0x002C0000 0x00040000>;
		};
		partition@8 {
			label = "NAND.kernel";
			reg = <0x00300000 0x00700000>;
		};
		partition@9 {
			label = "NAND.file-system";
			reg = <0x00a00000 0x1f600000>;
		};
	};
};

&epwmss0 {
	status = "okay";
};

&rtc_target {
	status = "disabled";
};

&tscadc {
	status = "okay";

	adc {
		ti,adc-channels = <0 1 2 3 4 5 6 7>;
	};
};

&ecap0 {
		status = "okay";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&ecap0_pins_default>;
		pinctrl-1 = <&ecap0_pins_sleep>;
};

&spi0 {
	status = "okay";
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&spi0_pins_default>;
	pinctrl-1 = <&spi0_pins_sleep>;
	ti,pindir-d0-out-d1-in;
};

&spi1 {
	status = "okay";
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&spi1_pins_default>;
	pinctrl-1 = <&spi1_pins_sleep>;
	ti,pindir-d0-out-d1-in;
};

&usb2_phy1 {
	status = "okay";
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&usb2_phy1_default>;
	pinctrl-1 = <&usb2_phy1_sleep>;
};

&usb1 {
	dr_mode = "otg";
	status = "okay";
};

&usb2_phy2 {
	status = "okay";
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&usb2_phy2_default>;
	pinctrl-1 = <&usb2_phy2_sleep>;
};

&usb2 {
	dr_mode = "host";
	status = "okay";
};

&qspi {
	status = "disabled";	/* Disable GPMC (NAND) when enabling QSPI */
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&qspi1_pins_default>;
	pinctrl-1 = <&qspi1_pins_sleep>;

	spi-max-frequency = <48000000>;
	flash@0 {
		compatible = "mx66l51235l";
		spi-max-frequency = <48000000>;
		reg = <0>;
		spi-cpol;
		spi-cpha;
		spi-tx-bus-width = <1>;
		spi-rx-bus-width = <4>;
		#address-cells = <1>;
		#size-cells = <1>;

		/* MTD partition table.
		 * The ROM checks the first 512KiB
		 * for a valid file to boot(XIP).
		 */
		partition@0 {
			label = "QSPI.U_BOOT";
			reg = <0x00000000 0x00080000>;
		};
		partition@1 {
			label = "QSPI.U_BOOT.backup";
			reg = <0x00080000 0x00080000>;
		};
		partition@2 {
			label = "QSPI.U-BOOT-SPL_OS";
			reg = <0x00100000 0x00010000>;
		};
		partition@3 {
			label = "QSPI.U_BOOT_ENV";
			reg = <0x00110000 0x00010000>;
		};
		partition@4 {
			label = "QSPI.U-BOOT-ENV.backup";
			reg = <0x00120000 0x00010000>;
		};
		partition@5 {
			label = "QSPI.KERNEL";
			reg = <0x00130000 0x0800000>;
		};
		partition@6 {
			label = "QSPI.FILESYSTEM";
			reg = <0x00930000 0x36D0000>;
		};
	};
};

&hdq {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&hdq_pins>;
};

&dss {
	status = "okay";

	pinctrl-names = "default";
	pinctrl-0 = <&dss_pins>;

	port {
		dpi_out: endpoint {
			remote-endpoint = <&lcd_in>;
			data-lines = <24>;
		};
	};
};

&vpfe1 {
	status = "okay";
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&vpfe1_pins_default>;
	pinctrl-1 = <&vpfe1_pins_sleep>;

	port {
		vpfe1_ep: endpoint {
			remote-endpoint = <&ov2659_1>;
			ti,am437x-vpfe-interface = <0>;
			bus-width = <8>;
			hsync-active = <0>;
			vsync-active = <0>;
		};
	};
};

&uart0 {
	status = "okay";
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&uart0_pins_default>;
	pinctrl-1 = <&uart0_pins_sleep>;
};

&mcasp1 {
	#sound-dai-cells = <0>;
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&mcasp1_pins>;
	pinctrl-1 = <&mcasp1_sleep_pins>;

	status = "okay";

	op-mode = <0>;          /* MCASP_IIS_MODE */
	tdm-slots = <2>;
	/* 4 serializer */
	serial-dir = <  /* 0: INACTIVE, 1: TX, 2: RX */
		1 2 0 0
	>;
	tx-num-evt = <32>;
	rx-num-evt = <32>;
};

&mux_synctimer32k_ck {
	assigned-clocks = <&mux_synctimer32k_ck>;
	assigned-clock-parents = <&clkdiv32k_ick>;
};

&cpu {
	cpu0-supply = <&dcdc2>;
};

&wkup_m3_ipc {
	firmware-name = "am43x-evm-scale-data.bin";
};

&pruss1_mdio {
	status = "disabled";
};
