// SPDX-License-Identifier: (GPL-2.0 OR MIT)
//
// Copyright 2013 Freescale Semiconductor, Inc.

#include "vf610-pinfunc.h"
#include <dt-bindings/clock/vf610-clock.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/gpio/gpio.h>

/ {
	aliases {
		can0 = &can0;
		can1 = &can1;
		ethernet0 = &fec0;
		ethernet1 = &fec1;
		serial0 = &uart0;
		serial1 = &uart1;
		serial2 = &uart2;
		serial3 = &uart3;
		serial4 = &uart4;
		serial5 = &uart5;
		gpio0 = &gpio0;
		gpio1 = &gpio1;
		gpio2 = &gpio2;
		gpio3 = &gpio3;
		gpio4 = &gpio4;
		usbphy0 = &usbphy0;
		usbphy1 = &usbphy1;
	};

	fxosc: fxosc {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <24000000>;
	};

	sxosc: sxosc {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <32768>;
	};

	reboot: syscon-reboot {
		compatible = "syscon-reboot";
		regmap = <&src>;
		offset = <0x0>;
		mask = <0x1000>;
	};

	tempsensor: iio-hwmon {
		compatible = "iio-hwmon";
		io-channels = <&adc0 16>, <&adc1 16>;
	};

	soc {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "simple-bus";
		interrupt-parent = <&mscm_ir>;
		ranges;

		aips0: bus@40000000 {
			compatible = "fsl,aips-bus", "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x40000000 0x00070000>;
			ranges;

			mscm_cpucfg: cpucfg@40001000 {
				compatible = "fsl,vf610-mscm-cpucfg", "syscon";
				reg = <0x40001000 0x800>;
			};

			mscm_ir: interrupt-controller@40001800 {
				compatible = "fsl,vf610-mscm-ir";
				reg = <0x40001800 0x400>;
				fsl,cpucfg = <&mscm_cpucfg>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			edma0: dma-controller@40018000 {
				#dma-cells = <2>;
				compatible = "fsl,vf610-edma";
				reg = <0x40018000 0x2000>,
					<0x40024000 0x1000>,
					<0x40025000 0x1000>;
				dma-channels = <32>;
				interrupts = <8 IRQ_TYPE_LEVEL_HIGH>,
						<9 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "edma-tx", "edma-err";
				clock-names = "dmamux0", "dmamux1";
				clocks = <&clks VF610_CLK_DMAMUX0>,
					<&clks VF610_CLK_DMAMUX1>;
				status = "disabled";
			};

			can0: can@40020000 {
				compatible = "fsl,vf610-flexcan";
				reg = <0x40020000 0x4000>;
				interrupts = <58 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_FLEXCAN0>,
					 <&clks VF610_CLK_FLEXCAN0>;
				clock-names = "ipg", "per";
				status = "disabled";
			};

			uart0: serial@40027000 {
				compatible = "fsl,vf610-lpuart";
				reg = <0x40027000 0x1000>;
				interrupts = <61 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_UART0>;
				clock-names = "ipg";
				dmas = <&edma0 0 2>, <&edma0 0 3>;
				dma-names = "rx","tx";
				status = "disabled";
			};

			uart1: serial@40028000 {
				compatible = "fsl,vf610-lpuart";
				reg = <0x40028000 0x1000>;
				interrupts = <62 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_UART1>;
				clock-names = "ipg";
				dmas = <&edma0 0 4>, <&edma0 0 5>;
				dma-names = "rx","tx";
				status = "disabled";
			};

			uart2: serial@40029000 {
				compatible = "fsl,vf610-lpuart";
				reg = <0x40029000 0x1000>;
				interrupts = <63 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_UART2>;
				clock-names = "ipg";
				dmas = <&edma0 0 6>, <&edma0 0 7>;
				dma-names = "rx","tx";
				status = "disabled";
			};

			uart3: serial@4002a000 {
				compatible = "fsl,vf610-lpuart";
				reg = <0x4002a000 0x1000>;
				interrupts = <64 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_UART3>;
				clock-names = "ipg";
				dmas = <&edma0 0 8>, <&edma0 0 9>;
				dma-names = "rx","tx";
				status = "disabled";
			};

			dspi0: spi@4002c000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,vf610-dspi";
				reg = <0x4002c000 0x1000>;
				interrupts = <67 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_DSPI0>;
				clock-names = "dspi";
				spi-num-chipselects = <6>;
				dmas = <&edma1 1 12>, <&edma1 1 13>;
				dma-names = "rx", "tx";
				status = "disabled";
			};

			dspi1: spi@4002d000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,vf610-dspi";
				reg = <0x4002d000 0x1000>;
				interrupts = <68 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_DSPI1>;
				clock-names = "dspi";
				spi-num-chipselects = <4>;
				dmas = <&edma1 1 14>, <&edma1 1 15>;
				dma-names = "rx", "tx";
				status = "disabled";
			};

			sai0: sai@4002f000 {
				compatible = "fsl,vf610-sai";
				reg = <0x4002f000 0x1000>;
				interrupts = <84 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_SAI0>,
					<&clks VF610_CLK_SAI0_DIV>,
					<&clks 0>, <&clks 0>;
				clock-names = "bus", "mclk1", "mclk2", "mclk3";
				dma-names = "rx", "tx";
				dmas = <&edma0 0 16>, <&edma0 0 17>;
				status = "disabled";
			};

			sai1: sai@40030000 {
				compatible = "fsl,vf610-sai";
				reg = <0x40030000 0x1000>;
				interrupts = <85 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_SAI1>,
					<&clks VF610_CLK_SAI1_DIV>,
					<&clks 0>, <&clks 0>;
				clock-names = "bus", "mclk1", "mclk2", "mclk3";
				dma-names = "rx", "tx";
				dmas = <&edma0 0 18>, <&edma0 0 19>;
				status = "disabled";
			};

			sai2: sai@40031000 {
				compatible = "fsl,vf610-sai";
				reg = <0x40031000 0x1000>;
				interrupts = <86 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_SAI2>,
					<&clks VF610_CLK_SAI2_DIV>,
					<&clks 0>, <&clks 0>;
				clock-names = "bus", "mclk1", "mclk2", "mclk3";
				dma-names = "rx", "tx";
				dmas = <&edma0 0 20>, <&edma0 0 21>;
				status = "disabled";
			};

			sai3: sai@40032000 {
				compatible = "fsl,vf610-sai";
				reg = <0x40032000 0x1000>;
				interrupts = <87 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_SAI3>,
					<&clks VF610_CLK_SAI3_DIV>,
					<&clks 0>, <&clks 0>;
				clock-names = "bus", "mclk1", "mclk2", "mclk3";
				dma-names = "rx", "tx";
				dmas = <&edma0 1 8>, <&edma0 1 9>;
				status = "disabled";
			};

			pit: pit@40037000 {
				compatible = "fsl,vf610-pit";
				reg = <0x40037000 0x1000>;
				interrupts = <39 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_PIT>;
				clock-names = "pit";
			};

			pwm0: pwm@40038000 {
				compatible = "fsl,vf610-ftm-pwm";
				#pwm-cells = <3>;
				reg = <0x40038000 0x1000>;
				clock-names = "ftm_sys", "ftm_ext",
					      "ftm_fix", "ftm_cnt_clk_en";
				clocks = <&clks VF610_CLK_FTM0>,
					<&clks VF610_CLK_FTM0_EXT_SEL>,
					<&clks VF610_CLK_FTM0_FIX_SEL>,
					<&clks VF610_CLK_FTM0_EXT_FIX_EN>;
				status = "disabled";
			};

			pwm1: pwm@40039000 {
				compatible = "fsl,vf610-ftm-pwm";
				#pwm-cells = <3>;
				reg = <0x40039000 0x1000>;
				clock-names = "ftm_sys", "ftm_ext",
					      "ftm_fix", "ftm_cnt_clk_en";
				clocks = <&clks VF610_CLK_FTM1>,
					<&clks VF610_CLK_FTM1_EXT_SEL>,
					<&clks VF610_CLK_FTM1_FIX_SEL>,
					<&clks VF610_CLK_FTM1_EXT_FIX_EN>;
				status = "disabled";
			};

			adc0: adc@4003b000 {
				compatible = "fsl,vf610-adc";
				reg = <0x4003b000 0x1000>;
				interrupts = <53 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_ADC0>;
				clock-names = "adc";
				#io-channel-cells = <1>;
				status = "disabled";
				fsl,adck-max-frequency = <30000000>, <40000000>,
							<20000000>;
			};

			tcon0: timing-controller@4003d000 {
				compatible = "fsl,vf610-tcon";
				reg = <0x4003d000 0x1000>;
				clocks = <&clks VF610_CLK_TCON0>;
				clock-names = "ipg";
				status = "disabled";
			};

			wdoga5: watchdog@4003e000 {
				compatible = "fsl,vf610-wdt", "fsl,imx21-wdt";
				reg = <0x4003e000 0x1000>;
				interrupts = <20 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_WDT>;
				status = "disabled";
			};

			qspi0: spi@40044000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,vf610-qspi";
				reg = <0x40044000 0x1000>, <0x20000000 0x10000000>;
				reg-names = "QuadSPI", "QuadSPI-memory";
				interrupts = <24 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_QSPI0_EN>,
					<&clks VF610_CLK_QSPI0>;
				clock-names = "qspi_en", "qspi";
				status = "disabled";
			};

			iomuxc: iomuxc@40048000 {
				compatible = "fsl,vf610-iomuxc";
				reg = <0x40048000 0x1000>;
			};

			gpio0: gpio@40049000 {
				compatible = "fsl,vf610-gpio";
				reg = <0x40049000 0x1000 0x400ff000 0x40>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupts = <107 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 0 32>;
			};

			gpio1: gpio@4004a000 {
				compatible = "fsl,vf610-gpio";
				reg = <0x4004a000 0x1000 0x400ff040 0x40>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupts = <108 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 32 32>;
			};

			gpio2: gpio@4004b000 {
				compatible = "fsl,vf610-gpio";
				reg = <0x4004b000 0x1000 0x400ff080 0x40>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupts = <109 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 64 32>;
			};

			gpio3: gpio@4004c000 {
				compatible = "fsl,vf610-gpio";
				reg = <0x4004c000 0x1000 0x400ff0c0 0x40>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupts = <110 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 96 32>;
			};

			gpio4: gpio@4004d000 {
				compatible = "fsl,vf610-gpio";
				reg = <0x4004d000 0x1000 0x400ff100 0x40>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupts = <111 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-controller;
				#interrupt-cells = <2>;
				gpio-ranges = <&iomuxc 0 128 7>;
			};

			anatop: anatop@40050000 {
				compatible = "fsl,vf610-anatop", "syscon";
				reg = <0x40050000 0x400>;
			};

			usbphy0: usbphy@40050800 {
				compatible = "fsl,vf610-usbphy";
				reg = <0x40050800 0x400>;
				interrupts = <50 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_USBPHY0>;
				fsl,anatop = <&anatop>;
				status = "disabled";
			};

			usbphy1: usbphy@40050c00 {
				compatible = "fsl,vf610-usbphy";
				reg = <0x40050c00 0x400>;
				interrupts = <51 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_USBPHY1>;
				fsl,anatop = <&anatop>;
				status = "disabled";
			};

			dcu0: dcu@40058000 {
				compatible = "fsl,vf610-dcu";
				reg = <0x40058000 0x1200>;
				interrupts = <30 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_DCU0>,
					<&clks VF610_CLK_DCU0_DIV>;
				clock-names = "dcu", "pix";
				fsl,tcon = <&tcon0>;
				status = "disabled";
			};

			i2c0: i2c@40066000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,vf610-i2c";
				reg = <0x40066000 0x1000>;
				interrupts = <71 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_I2C0>;
				clock-names = "ipg";
				dmas = <&edma0 0 50>,
					<&edma0 0 51>;
				dma-names = "rx","tx";
				status = "disabled";
			};

			i2c1: i2c@40067000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,vf610-i2c";
				reg = <0x40067000 0x1000>;
				interrupts = <72 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_I2C1>;
				clock-names = "ipg";
				dmas = <&edma0 0 52>, <&edma0 0 53>;
				dma-names = "rx","tx";
				status = "disabled";
			};

			clks: ccm@4006b000 {
				compatible = "fsl,vf610-ccm";
				reg = <0x4006b000 0x1000>;
				clocks = <&sxosc>, <&fxosc>;
				clock-names = "sxosc", "fxosc";
				#clock-cells = <1>;
			};

			usbdev0: usb@40034000 {
				compatible = "fsl,vf610-usb", "fsl,imx27-usb";
				reg = <0x40034000 0x800>;
				interrupts = <75 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_USBC0>;
				fsl,usbphy = <&usbphy0>;
				fsl,usbmisc = <&usbmisc0 0>;
				dr_mode = "peripheral";
				status = "disabled";
			};

			usbmisc0: usb@40034800 {
				#index-cells = <1>;
				compatible = "fsl,vf610-usbmisc";
				reg = <0x40034800 0x200>;
				clocks = <&clks VF610_CLK_USBC0>;
				status = "disabled";
			};

			src: src@4006e000 {
				compatible = "fsl,vf610-src", "syscon";
				reg = <0x4006e000 0x1000>;
				interrupts = <96 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		aips1: bus@40080000 {
			compatible = "fsl,aips-bus", "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x40080000 0x0007f000>;
			ranges;

			edma1: dma-controller@40098000 {
				#dma-cells = <2>;
				compatible = "fsl,vf610-edma";
				reg = <0x40098000 0x2000>,
					<0x400a1000 0x1000>,
					<0x400a2000 0x1000>;
				dma-channels = <32>;
				interrupts = <10 IRQ_TYPE_LEVEL_HIGH>,
						<11 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "edma-tx", "edma-err";
				clock-names = "dmamux0", "dmamux1";
				clocks = <&clks VF610_CLK_DMAMUX2>,
					<&clks VF610_CLK_DMAMUX3>;
				status = "disabled";
			};

			ocotp: ocotp@400a5000 {
				compatible = "fsl,vf610-ocotp", "syscon";
				reg = <0x400a5000 0x1000>;
				clocks = <&clks VF610_CLK_OCOTP>;
			};

			snvs0: snvs@400a7000 {
			    compatible = "fsl,sec-v4.0-mon", "syscon", "simple-mfd";
				reg = <0x400a7000 0x2000>;

				snvsrtc: snvs-rtc-lp {
					compatible = "fsl,sec-v4.0-mon-rtc-lp";
					regmap = <&snvs0>;
					offset = <0x34>;
					interrupts = <100 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&clks VF610_CLK_SNVS>;
					clock-names = "snvs-rtc";
				};
			};

			uart4: serial@400a9000 {
				compatible = "fsl,vf610-lpuart";
				reg = <0x400a9000 0x1000>;
				interrupts = <65 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_UART4>;
				clock-names = "ipg";
				status = "disabled";
			};

			uart5: serial@400aa000 {
				compatible = "fsl,vf610-lpuart";
				reg = <0x400aa000 0x1000>;
				interrupts = <66 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_UART5>;
				clock-names = "ipg";
				status = "disabled";
			};

			dspi2: spi@400ac000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,vf610-dspi";
				reg = <0x400ac000 0x1000>;
				interrupts = <69 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_DSPI2>;
				clock-names = "dspi";
				spi-num-chipselects = <2>;
				dmas = <&edma1 0 10>,
					<&edma1 0 11>;
				dma-names = "rx", "tx";
				status = "disabled";
			};

			dspi3: spi@400ad000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,vf610-dspi";
				reg = <0x400ad000 0x1000>;
				interrupts = <70 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_DSPI3>;
				clock-names = "dspi";
				spi-num-chipselects = <2>;
				dmas = <&edma1 0 12>, <&edma1 0 13>;
				dma-names = "rx", "tx";
				status = "disabled";
			};

			adc1: adc@400bb000 {
				compatible = "fsl,vf610-adc";
				reg = <0x400bb000 0x1000>;
				interrupts = <54 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_ADC1>;
				clock-names = "adc";
				#io-channel-cells = <1>;
				status = "disabled";
				fsl,adck-max-frequency = <30000000>, <40000000>,
							<20000000>;
			};

			esdhc0: mmc@400b1000 {
				compatible = "fsl,imx53-esdhc";
				reg = <0x400b1000 0x1000>;
				interrupts = <27 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_IPG_BUS>,
					<&clks VF610_CLK_PLATFORM_BUS>,
					<&clks VF610_CLK_ESDHC0>;
				clock-names = "ipg", "ahb", "per";
				status = "disabled";
			};

			esdhc1: mmc@400b2000 {
				compatible = "fsl,imx53-esdhc";
				reg = <0x400b2000 0x1000>;
				interrupts = <28 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_IPG_BUS>,
					<&clks VF610_CLK_PLATFORM_BUS>,
					<&clks VF610_CLK_ESDHC1>;
				clock-names = "ipg", "ahb", "per";
				status = "disabled";
			};

			usbh1: usb@400b4000 {
				compatible = "fsl,vf610-usb", "fsl,imx27-usb";
				reg = <0x400b4000 0x800>;
				interrupts = <76 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_USBC1>;
				fsl,usbphy = <&usbphy1>;
				fsl,usbmisc = <&usbmisc1 0>;
				dr_mode = "host";
				status = "disabled";
			};

			usbmisc1: usb@400b4800 {
				#index-cells = <1>;
				compatible = "fsl,vf610-usbmisc";
				reg = <0x400b4800 0x200>;
				clocks = <&clks VF610_CLK_USBC1>;
				status = "disabled";
			};

			ftm: ftm@400b8000 {
				compatible = "fsl,ftm-timer";
				reg = <0x400b8000 0x1000>, <0x400b9000 0x1000>;
				interrupts = <44 IRQ_TYPE_LEVEL_HIGH>;
				clock-names = "ftm-evt", "ftm-src",
					"ftm-evt-counter-en", "ftm-src-counter-en";
				clocks = <&clks VF610_CLK_FTM2>,
					<&clks VF610_CLK_FTM3>,
					<&clks VF610_CLK_FTM2_EXT_FIX_EN>,
					<&clks VF610_CLK_FTM3_EXT_FIX_EN>;
				status = "disabled";
			};

			qspi1: spi@400c4000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,vf610-qspi";
				reg = <0x400c4000 0x1000>, <0x50000000 0x10000000>;
				reg-names = "QuadSPI", "QuadSPI-memory";
				interrupts = <25 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_QSPI1_EN>,
					<&clks VF610_CLK_QSPI1>;
				clock-names = "qspi_en", "qspi";
				status = "disabled";
			};

			dac0: dac@400cc000 {
				compatible = "fsl,vf610-dac";
				reg = <0x400cc000 1000>;
				interrupts = <55 IRQ_TYPE_LEVEL_HIGH>;
				clock-names = "dac";
				clocks = <&clks VF610_CLK_DAC0>;
				status = "disabled";
			};

			dac1: dac@400cd000 {
				compatible = "fsl,vf610-dac";
				reg = <0x400cd000 1000>;
				interrupts = <56 IRQ_TYPE_LEVEL_HIGH>;
				clock-names = "dac";
				clocks = <&clks VF610_CLK_DAC1>;
				status = "disabled";
			};

			fec0: ethernet@400d0000 {
				compatible = "fsl,mvf600-fec";
				reg = <0x400d0000 0x1000>;
				interrupts = <78 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_ENET0>,
					<&clks VF610_CLK_ENET0>,
					<&clks VF610_CLK_ENET>;
				clock-names = "ipg", "ahb", "ptp";
				status = "disabled";
			};

			fec1: ethernet@400d1000 {
				compatible = "fsl,mvf600-fec";
				reg = <0x400d1000 0x1000>;
				interrupts = <79 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_ENET1>,
					<&clks VF610_CLK_ENET1>,
					<&clks VF610_CLK_ENET>;
				clock-names = "ipg", "ahb", "ptp";
				status = "disabled";
			};

			can1: can@400d4000 {
				compatible = "fsl,vf610-flexcan";
				reg = <0x400d4000 0x4000>;
				interrupts = <59 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_FLEXCAN1>,
					 <&clks VF610_CLK_FLEXCAN1>;
				clock-names = "ipg", "per";
				status = "disabled";
			};

			nfc: nand@400e0000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,vf610-nfc";
				reg = <0x400e0000 0x4000>;
				interrupts = <83 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_NFC>;
				clock-names = "nfc";
				status = "disabled";
			};

			i2c2: i2c@400e6000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,vf610-i2c";
				reg = <0x400e6000 0x1000>;
				interrupts = <73 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_I2C2>;
				clock-names = "ipg";
				dmas = <&edma0 1 36>,
					<&edma0 1 37>;
				dma-names = "rx","tx";
				status = "disabled";
			};

			i2c3: i2c@400e7000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,vf610-i2c";
				reg = <0x400e7000 0x1000>;
				interrupts = <74 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clks VF610_CLK_I2C3>;
				clock-names = "ipg";
				dmas = <&edma0 1 38>, <&edma0 1 39>;
				dma-names = "rx","tx";
				status = "disabled";
			};

			crypto: crypto@400f0000 {
				compatible = "fsl,sec-v4.0";
				#address-cells = <1>;
				#size-cells = <1>;
				reg = <0x400f0000 0x9000>;
				ranges = <0 0x400f0000 0x9000>;
				clocks = <&clks VF610_CLK_CAAM>;
				clock-names = "ipg";

				sec_jr0: jr0@1000 {
					compatible = "fsl,sec-v4.0-job-ring";
					reg = <0x1000 0x1000>;
					interrupts = <102 IRQ_TYPE_LEVEL_HIGH>;
				};

				sec_jr1: jr1@2000 {
					compatible = "fsl,sec-v4.0-job-ring";
					reg = <0x2000 0x1000>;
					interrupts = <102 IRQ_TYPE_LEVEL_HIGH>;
				};
			};
		};
	};
};
