// SPDX-License-Identifier: GPL-2.0
/dts-v1/;

#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/clock/qcom,gcc-msm8960.h>
#include <dt-bindings/reset/qcom,gcc-msm8960.h>
#include <dt-bindings/clock/qcom,lcc-msm8960.h>
#include <dt-bindings/mfd/qcom-rpm.h>
#include <dt-bindings/soc/qcom,gsbi.h>

/ {
	#address-cells = <1>;
	#size-cells = <1>;
	model = "Qualcomm MSM8960";
	compatible = "qcom,msm8960";
	interrupt-parent = <&intc>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;
		interrupts = <GIC_PPI 14 0x304>;

		cpu@0 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <0>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc0>;
			qcom,saw = <&saw0>;
		};

		cpu@1 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <1>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc1>;
			qcom,saw = <&saw1>;
		};

		L2: l2-cache {
			compatible = "cache";
			cache-level = <2>;
			cache-unified;
		};
	};

	memory@80000000 {
		device_type = "memory";
		reg = <0x80000000 0>;
	};

	cpu-pmu {
		compatible = "qcom,krait-pmu";
		interrupts = <GIC_PPI 10 0x304>;
		qcom,no-pc-write;
	};

	clocks {
		cxo_board: cxo_board {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <19200000>;
			clock-output-names = "cxo_board";
		};

		pxo_board: pxo_board {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <27000000>;
			clock-output-names = "pxo_board";
		};

		sleep_clk: sleep_clk {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <32768>;
			clock-output-names = "sleep_clk";
		};
	};

	/* Temporary fixed regulator */
	vsdcc_fixed: vsdcc-regulator {
		compatible = "regulator-fixed";
		regulator-name = "SDCC Power";
		regulator-min-microvolt = <2700000>;
		regulator-max-microvolt = <2700000>;
		regulator-always-on;
	};

	soc: soc {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		compatible = "simple-bus";

		intc: interrupt-controller@2000000 {
			compatible = "qcom,msm-qgic2";
			interrupt-controller;
			#interrupt-cells = <3>;
			reg = <0x02000000 0x1000>,
			      <0x02002000 0x1000>;
		};

		timer@200a000 {
			compatible = "qcom,kpss-wdt-msm8960", "qcom,kpss-timer",
				     "qcom,msm-timer";
			interrupts = <GIC_PPI 1 0x301>,
				     <GIC_PPI 2 0x301>,
				     <GIC_PPI 3 0x301>;
			reg = <0x0200a000 0x100>;
			clock-frequency = <27000000>;
			cpu-offset = <0x80000>;
		};

		msmgpio: pinctrl@800000 {
			compatible = "qcom,msm8960-pinctrl";
			gpio-controller;
			gpio-ranges = <&msmgpio 0 0 152>;
			#gpio-cells = <2>;
			interrupts = <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			reg = <0x800000 0x4000>;
		};

		gcc: clock-controller@900000 {
			compatible = "qcom,gcc-msm8960";
			#clock-cells = <1>;
			#reset-cells = <1>;
			reg = <0x900000 0x4000>;
			clocks = <&cxo_board>,
				 <&pxo_board>,
				 <&lcc PLL4>;
			clock-names = "cxo", "pxo", "pll4";
		};

		lcc: clock-controller@28000000 {
			compatible = "qcom,lcc-msm8960";
			reg = <0x28000000 0x1000>;
			#clock-cells = <1>;
			#reset-cells = <1>;
			clocks = <&pxo_board>,
				 <&gcc PLL4_VOTE>,
				 <0>,
				 <0>, <0>,
				 <0>, <0>,
				 <0>;
			clock-names = "pxo",
				      "pll4_vote",
				      "mi2s_codec_clk",
				      "codec_i2s_mic_codec_clk",
				      "spare_i2s_mic_codec_clk",
				      "codec_i2s_spkr_codec_clk",
				      "spare_i2s_spkr_codec_clk",
				      "pcm_codec_clk";
		};

		clock-controller@4000000 {
			compatible = "qcom,mmcc-msm8960";
			reg = <0x4000000 0x1000>;
			#clock-cells = <1>;
			#power-domain-cells = <1>;
			#reset-cells = <1>;
			clocks = <&pxo_board>,
				 <&gcc PLL3>,
				 <&gcc PLL8_VOTE>,
				 <0>,
				 <0>,
				 <0>,
				 <0>,
				 <0>;
			clock-names = "pxo",
				      "pll3",
				      "pll8_vote",
				      "dsi1pll",
				      "dsi1pllbyte",
				      "dsi2pll",
				      "dsi2pllbyte",
				      "hdmipll";
		};

		l2cc: clock-controller@2011000 {
			compatible = "qcom,kpss-gcc-msm8960", "qcom,kpss-gcc", "syscon";
			reg = <0x2011000 0x1000>;
			clocks = <&gcc PLL8_VOTE>, <&pxo_board>;
			clock-names = "pll8_vote", "pxo";
			#clock-cells = <0>;
		};

		rpm: rpm@108000 {
			compatible = "qcom,rpm-msm8960";
			reg = <0x108000 0x1000>;
			qcom,ipc = <&l2cc 0x8 2>;

			interrupts = <GIC_SPI 19 IRQ_TYPE_EDGE_RISING>,
				     <GIC_SPI 21 IRQ_TYPE_EDGE_RISING>,
				     <GIC_SPI 22 IRQ_TYPE_EDGE_RISING>;
			interrupt-names = "ack", "err", "wakeup";
		};

		acc0: clock-controller@2088000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x02088000 0x1000>, <0x02008000 0x1000>;
			clocks = <&gcc PLL8_VOTE>, <&pxo_board>;
			clock-names = "pll8_vote", "pxo";
			clock-output-names = "acpu0_aux";
			#clock-cells = <0>;
		};

		acc1: clock-controller@2098000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x02098000 0x1000>, <0x02008000 0x1000>;
			clocks = <&gcc PLL8_VOTE>, <&pxo_board>;
			clock-names = "pll8_vote", "pxo";
			clock-output-names = "acpu1_aux";
			#clock-cells = <0>;
		};

		saw0: power-manager@2089000 {
			compatible = "qcom,msm8960-saw2-cpu", "qcom,saw2";
			reg = <0x02089000 0x1000>, <0x02009000 0x1000>;

			saw0_vreg: regulator {
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1300000>;
			};
		};

		saw1: power-manager@2099000 {
			compatible = "qcom,msm8960-saw2-cpu", "qcom,saw2";
			reg = <0x02099000 0x1000>, <0x02009000 0x1000>;

			saw1_vreg: regulator {
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1300000>;
			};
		};

		gsbi5: gsbi@16400000 {
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <5>;
			reg = <0x16400000 0x100>;
			clocks = <&gcc GSBI5_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			syscon-tcsr = <&tcsr>;

			gsbi5_serial: serial@16440000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x16440000 0x1000>,
				      <0x16400000 0x1000>;
				interrupts = <GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI5_UART_CLK>, <&gcc GSBI5_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};
		};

		ssbi: ssbi@500000 {
			compatible = "qcom,ssbi";
			reg = <0x500000 0x1000>;
			qcom,controller-type = "pmic-arbiter";
		};

		rng@1a500000 {
			compatible = "qcom,prng";
			reg = <0x1a500000 0x200>;
			clocks = <&gcc PRNG_CLK>;
			clock-names = "core";
		};

		sdcc3: mmc@12180000 {
			compatible = "arm,pl18x", "arm,primecell";
			arm,primecell-periphid = <0x00051180>;
			status = "disabled";
			reg = <0x12180000 0x8000>;
			interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc SDC3_CLK>, <&gcc SDC3_H_CLK>;
			clock-names = "mclk", "apb_pclk";
			bus-width = <4>;
			cap-sd-highspeed;
			cap-mmc-highspeed;
			max-frequency = <192000000>;
			no-1-8-v;
			vmmc-supply = <&vsdcc_fixed>;
		};

		sdcc1: mmc@12400000 {
			status = "disabled";
			compatible = "arm,pl18x", "arm,primecell";
			arm,primecell-periphid = <0x00051180>;
			reg = <0x12400000 0x8000>;
			interrupts = <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc SDC1_CLK>, <&gcc SDC1_H_CLK>;
			clock-names = "mclk", "apb_pclk";
			bus-width = <8>;
			max-frequency = <96000000>;
			non-removable;
			cap-sd-highspeed;
			cap-mmc-highspeed;
			vmmc-supply = <&vsdcc_fixed>;
		};

		tcsr: syscon@1a400000 {
			compatible = "qcom,tcsr-msm8960", "syscon";
			reg = <0x1a400000 0x100>;
		};

		gsbi1: gsbi@16000000 {
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <1>;
			reg = <0x16000000 0x100>;
			clocks = <&gcc GSBI1_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			gsbi1_spi: spi@16080000 {
				compatible = "qcom,spi-qup-v1.1.1";
				#address-cells = <1>;
				#size-cells = <0>;
				reg = <0x16080000 0x1000>;
				interrupts = <GIC_SPI 147 IRQ_TYPE_LEVEL_HIGH>;
				cs-gpios = <&msmgpio 8 0>;

				clocks = <&gcc GSBI1_QUP_CLK>, <&gcc GSBI1_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};
		};

		usb1: usb@12500000 {
			compatible = "qcom,ci-hdrc";
			reg = <0x12500000 0x200>,
			      <0x12500200 0x200>;
			interrupts = <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc USB_HS1_XCVR_CLK>, <&gcc USB_HS1_H_CLK>;
			clock-names = "core", "iface";
			assigned-clocks = <&gcc USB_HS1_XCVR_CLK>;
			assigned-clock-rates = <60000000>;
			resets = <&gcc USB_HS1_RESET>;
			reset-names = "core";
			phy_type = "ulpi";
			ahb-burst-config = <0>;
			phys = <&usb_hs1_phy>;
			phy-names = "usb-phy";
			#reset-cells = <1>;
			status = "disabled";

			ulpi {
				usb_hs1_phy: phy {
					compatible = "qcom,usb-hs-phy-msm8960",
						     "qcom,usb-hs-phy";
					clocks = <&sleep_clk>, <&cxo_board>;
					clock-names = "sleep", "ref";
					resets = <&usb1 0>;
					reset-names = "por";
					#phy-cells = <0>;
				};
			};
		};

		gsbi3: gsbi@16200000 {
			compatible = "qcom,gsbi-v1.0.0";
			reg = <0x16200000 0x100>;
			ranges;
			cell-index = <3>;
			clocks = <&gcc GSBI3_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			status = "disabled";

			gsbi3_i2c: i2c@16280000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x16280000 0x1000>;
				pinctrl-0 = <&i2c3_default_state>;
				pinctrl-1 = <&i2c3_sleep_state>;
				pinctrl-names = "default", "sleep";
				interrupts = <GIC_SPI 151 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI3_QUP_CLK>,
					 <&gcc GSBI3_H_CLK>;
				clock-names = "core", "iface";
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};
	};
};
#include "qcom-msm8960-pins.dtsi"
