// SPDX-License-Identifier: GPL-2.0
/dts-v1/;

#include <dt-bindings/input/input.h>
#include "tegra124.dtsi"

#include "tegra124-jetson-tk1-emc.dtsi"

/ {
	model = "NVIDIA Tegra124 Jetson TK1";
	compatible = "nvidia,jetson-tk1", "nvidia,tegra124";

	aliases {
		rtc0 = "/i2c@7000d000/pmic@40";
		rtc1 = "/rtc@7000e000";

		/* This order keeps the mapping DB9 connector <-> ttyS0 */
		serial0 = &uartd;
		serial1 = &uarta;
		serial2 = &uartb;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	memory@80000000 {
		reg = <0x0 0x80000000 0x0 0x80000000>;
	};

	pcie@1003000 {
		status = "okay";

		avddio-pex-supply = <&vdd_1v05_run>;
		dvddio-pex-supply = <&vdd_1v05_run>;
		avdd-pex-pll-supply = <&vdd_1v05_run>;
		hvdd-pex-supply = <&vdd_3v3_lp0>;
		hvdd-pex-pll-e-supply = <&vdd_3v3_lp0>;
		vddio-pex-ctl-supply = <&vdd_3v3_lp0>;
		avdd-pll-erefe-supply = <&avdd_1v05_run>;

		/* Mini PCIe */
		pci@1,0 {
			phys = <&{/padctl@7009f000/pads/pcie/lanes/pcie-4}>;
			phy-names = "pcie-0";
			status = "okay";
		};

		/* Gigabit Ethernet */
		pci@2,0 {
			phys = <&{/padctl@7009f000/pads/pcie/lanes/pcie-2}>;
			phy-names = "pcie-0";
			status = "okay";
		};
	};

	host1x@50000000 {
		hdmi@54280000 {
			status = "okay";

			hdmi-supply = <&vdd_5v0_hdmi>;
			pll-supply = <&vdd_hdmi_pll>;
			vdd-supply = <&vdd_3v3_hdmi>;

			nvidia,ddc-i2c-bus = <&hdmi_ddc>;
			nvidia,hpd-gpio =
				<&gpio TEGRA_GPIO(N, 7) GPIO_ACTIVE_HIGH>;
		};
	};

	gpu@57000000 {
		/*
		 * Node left disabled on purpose - the bootloader will enable
		 * it after having set the VPR up
		 */
		vdd-supply = <&vdd_gpu>;
	};

	pinmux: pinmux@70000868 {
		pinctrl-names = "boot";
		pinctrl-0 = <&state_boot>;

		state_boot: pinmux {
			clk_32k_out_pa0 {
				nvidia,pins = "clk_32k_out_pa0";
				nvidia,function = "soc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			uart3_cts_n_pa1 {
				nvidia,pins = "uart3_cts_n_pa1";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap2_fs_pa2 {
				nvidia,pins = "dap2_fs_pa2";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap2_sclk_pa3 {
				nvidia,pins = "dap2_sclk_pa3";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap2_din_pa4 {
				nvidia,pins = "dap2_din_pa4";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dap2_dout_pa5 {
				nvidia,pins = "dap2_dout_pa5";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sdmmc3_clk_pa6 {
				nvidia,pins = "sdmmc3_clk_pa6";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_cmd_pa7 {
				nvidia,pins = "sdmmc3_cmd_pa7";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pb0 {
				nvidia,pins = "pb0";
				nvidia,function = "uartd";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pb1 {
				nvidia,pins = "pb1";
				nvidia,function = "uartd";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_dat3_pb4 {
				nvidia,pins = "sdmmc3_dat3_pb4";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_dat2_pb5 {
				nvidia,pins = "sdmmc3_dat2_pb5";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_dat1_pb6 {
				nvidia,pins = "sdmmc3_dat1_pb6";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_dat0_pb7 {
				nvidia,pins = "sdmmc3_dat0_pb7";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			uart3_rts_n_pc0 {
				nvidia,pins = "uart3_rts_n_pc0";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			uart2_txd_pc2 {
				nvidia,pins = "uart2_txd_pc2";
				nvidia,function = "irda";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			uart2_rxd_pc3 {
				nvidia,pins = "uart2_rxd_pc3";
				nvidia,function = "irda";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gen1_i2c_scl_pc4 {
				nvidia,pins = "gen1_i2c_scl_pc4";
				nvidia,function = "i2c1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			gen1_i2c_sda_pc5 {
				nvidia,pins = "gen1_i2c_sda_pc5";
				nvidia,function = "i2c1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			pc7 {
				nvidia,pins = "pc7";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pg0 {
				nvidia,pins = "pg0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pg1 {
				nvidia,pins = "pg1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pg2 {
				nvidia,pins = "pg2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pg3 {
				nvidia,pins = "pg3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pg4 {
				nvidia,pins = "pg4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pg5 {
				nvidia,pins = "pg5";
				nvidia,function = "spi4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pg6 {
				nvidia,pins = "pg6";
				nvidia,function = "spi4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pg7 {
				nvidia,pins = "pg7";
				nvidia,function = "spi4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ph0 {
				nvidia,pins = "ph0";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ph1 {
				nvidia,pins = "ph1";
				nvidia,function = "pwm1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ph2 {
				nvidia,pins = "ph2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ph3 {
				nvidia,pins = "ph3";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ph4 {
				nvidia,pins = "ph4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ph5 {
				nvidia,pins = "ph5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ph6 {
				nvidia,pins = "ph6";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ph7 {
				nvidia,pins = "ph7";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pi0 {
				nvidia,pins = "pi0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pi1 {
				nvidia,pins = "pi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pi2 {
				nvidia,pins = "pi2";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pi3 {
				nvidia,pins = "pi3";
				nvidia,function = "spi4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pi4 {
				nvidia,pins = "pi4";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pi5 {
				nvidia,pins = "pi5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pi6 {
				nvidia,pins = "pi6";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pi7 {
				nvidia,pins = "pi7";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pj0 {
				nvidia,pins = "pj0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pj2 {
				nvidia,pins = "pj2";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			uart2_cts_n_pj5 {
				nvidia,pins = "uart2_cts_n_pj5";
				nvidia,function = "uartb";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			uart2_rts_n_pj6 {
				nvidia,pins = "uart2_rts_n_pj6";
				nvidia,function = "uartb";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pj7 {
				nvidia,pins = "pj7";
				nvidia,function = "uartd";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pk0 {
				nvidia,pins = "pk0";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pk1 {
				nvidia,pins = "pk1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pk2 {
				nvidia,pins = "pk2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pk3 {
				nvidia,pins = "pk3";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pk4 {
				nvidia,pins = "pk4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			spdif_out_pk5 {
				nvidia,pins = "spdif_out_pk5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			spdif_in_pk6 {
				nvidia,pins = "spdif_in_pk6";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pk7 {
				nvidia,pins = "pk7";
				nvidia,function = "uartd";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap1_fs_pn0 {
				nvidia,pins = "dap1_fs_pn0";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap1_din_pn1 {
				nvidia,pins = "dap1_din_pn1";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap1_dout_pn2 {
				nvidia,pins = "dap1_dout_pn2";
				nvidia,function = "sata";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap1_sclk_pn3 {
				nvidia,pins = "dap1_sclk_pn3";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			usb_vbus_en0_pn4 {
				nvidia,pins = "usb_vbus_en0_pn4";
				nvidia,function = "usb";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_DISABLE>;
			};
			usb_vbus_en1_pn5 {
				nvidia,pins = "usb_vbus_en1_pn5";
				nvidia,function = "usb";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_DISABLE>;
			};
			hdmi_int_pn7 {
				nvidia,pins = "hdmi_int_pn7";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,rcv-sel = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data7_po0 {
				nvidia,pins = "ulpi_data7_po0";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data0_po1 {
				nvidia,pins = "ulpi_data0_po1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ulpi_data1_po2 {
				nvidia,pins = "ulpi_data1_po2";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data2_po3 {
				nvidia,pins = "ulpi_data2_po3";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data3_po4 {
				nvidia,pins = "ulpi_data3_po4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ulpi_data4_po5 {
				nvidia,pins = "ulpi_data4_po5";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data5_po6 {
				nvidia,pins = "ulpi_data5_po6";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data6_po7 {
				nvidia,pins = "ulpi_data6_po7";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap3_fs_pp0 {
				nvidia,pins = "dap3_fs_pp0";
				nvidia,function = "i2s2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap3_din_pp1 {
				nvidia,pins = "dap3_din_pp1";
				nvidia,function = "i2s2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap3_dout_pp2 {
				nvidia,pins = "dap3_dout_pp2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap3_sclk_pp3 {
				nvidia,pins = "dap3_sclk_pp3";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap4_fs_pp4 {
				nvidia,pins = "dap4_fs_pp4";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap4_din_pp5 {
				nvidia,pins = "dap4_din_pp5";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap4_dout_pp6 {
				nvidia,pins = "dap4_dout_pp6";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap4_sclk_pp7 {
				nvidia,pins = "dap4_sclk_pp7";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_col0_pq0 {
				nvidia,pins = "kb_col0_pq0";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_col1_pq1 {
				nvidia,pins = "kb_col1_pq1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_col2_pq2 {
				nvidia,pins = "kb_col2_pq2";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_col3_pq3 {
				nvidia,pins = "kb_col3_pq3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_col4_pq4 {
				nvidia,pins = "kb_col4_pq4";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_col5_pq5 {
				nvidia,pins = "kb_col5_pq5";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_col6_pq6 {
				nvidia,pins = "kb_col6_pq6";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_col7_pq7 {
				nvidia,pins = "kb_col7_pq7";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row0_pr0 {
				nvidia,pins = "kb_row0_pr0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row1_pr1 {
				nvidia,pins = "kb_row1_pr1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row2_pr2 {
				nvidia,pins = "kb_row2_pr2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row3_pr3 {
				nvidia,pins = "kb_row3_pr3";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row4_pr4 {
				nvidia,pins = "kb_row4_pr4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_row5_pr5 {
				nvidia,pins = "kb_row5_pr5";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row6_pr6 {
				nvidia,pins = "kb_row6_pr6";
				nvidia,function = "displaya_alt";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_row7_pr7 {
				nvidia,pins = "kb_row7_pr7";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_row8_ps0 {
				nvidia,pins = "kb_row8_ps0";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row9_ps1 {
				nvidia,pins = "kb_row9_ps1";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row10_ps2 {
				nvidia,pins = "kb_row10_ps2";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_row11_ps3 {
				nvidia,pins = "kb_row11_ps3";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row12_ps4 {
				nvidia,pins = "kb_row12_ps4";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row13_ps5 {
				nvidia,pins = "kb_row13_ps5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row14_ps6 {
				nvidia,pins = "kb_row14_ps6";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row15_ps7 {
				nvidia,pins = "kb_row15_ps7";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_row16_pt0 {
				nvidia,pins = "kb_row16_pt0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row17_pt1 {
				nvidia,pins = "kb_row17_pt1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gen2_i2c_scl_pt5 {
				nvidia,pins = "gen2_i2c_scl_pt5";
				nvidia,function = "i2c2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			gen2_i2c_sda_pt6 {
				nvidia,pins = "gen2_i2c_sda_pt6";
				nvidia,function = "i2c2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_cmd_pt7 {
				nvidia,pins = "sdmmc4_cmd_pt7";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu0 {
				nvidia,pins = "pu0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu1 {
				nvidia,pins = "pu1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu2 {
				nvidia,pins = "pu2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu3 {
				nvidia,pins = "pu3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu4 {
				nvidia,pins = "pu4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu5 {
				nvidia,pins = "pu5";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu6 {
				nvidia,pins = "pu6";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pv0 {
				nvidia,pins = "pv0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pv1 {
				nvidia,pins = "pv1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_cd_n_pv2 {
				nvidia,pins = "sdmmc3_cd_n_pv2";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc1_wp_n_pv3 {
				nvidia,pins = "sdmmc1_wp_n_pv3";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ddc_scl_pv4 {
				nvidia,pins = "ddc_scl_pv4";
				nvidia,function = "i2c4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,rcv-sel = <TEGRA_PIN_DISABLE>;
			};
			ddc_sda_pv5 {
				nvidia,pins = "ddc_sda_pv5";
				nvidia,function = "i2c4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,rcv-sel = <TEGRA_PIN_DISABLE>;
			};
			gpio_w2_aud_pw2 {
				nvidia,pins = "gpio_w2_aud_pw2";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gpio_w3_aud_pw3 {
				nvidia,pins = "gpio_w3_aud_pw3";
				nvidia,function = "spi6";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap_mclk1_pw4 {
				nvidia,pins = "dap_mclk1_pw4";
				nvidia,function = "extperiph1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			clk2_out_pw5 {
				nvidia,pins = "clk2_out_pw5";
				nvidia,function = "extperiph2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			uart3_txd_pw6 {
				nvidia,pins = "uart3_txd_pw6";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			uart3_rxd_pw7 {
				nvidia,pins = "uart3_rxd_pw7";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dvfs_pwm_px0 {
				nvidia,pins = "dvfs_pwm_px0";
				nvidia,function = "cldvfs";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gpio_x1_aud_px1 {
				nvidia,pins = "gpio_x1_aud_px1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dvfs_clk_px2 {
				nvidia,pins = "dvfs_clk_px2";
				nvidia,function = "cldvfs";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gpio_x3_aud_px3 {
				nvidia,pins = "gpio_x3_aud_px3";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gpio_x4_aud_px4 {
				nvidia,pins = "gpio_x4_aud_px4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gpio_x5_aud_px5 {
				nvidia,pins = "gpio_x5_aud_px5";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gpio_x6_aud_px6 {
				nvidia,pins = "gpio_x6_aud_px6";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gpio_x7_aud_px7 {
				nvidia,pins = "gpio_x7_aud_px7";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_clk_py0 {
				nvidia,pins = "ulpi_clk_py0";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_dir_py1 {
				nvidia,pins = "ulpi_dir_py1";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ulpi_nxt_py2 {
				nvidia,pins = "ulpi_nxt_py2";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_stp_py3 {
				nvidia,pins = "ulpi_stp_py3";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sdmmc1_dat3_py4 {
				nvidia,pins = "sdmmc1_dat3_py4";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sdmmc1_dat2_py5 {
				nvidia,pins = "sdmmc1_dat2_py5";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sdmmc1_dat1_py6 {
				nvidia,pins = "sdmmc1_dat1_py6";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sdmmc1_dat0_py7 {
				nvidia,pins = "sdmmc1_dat0_py7";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sdmmc1_clk_pz0 {
				nvidia,pins = "sdmmc1_clk_pz0";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sdmmc1_cmd_pz1 {
				nvidia,pins = "sdmmc1_cmd_pz1";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pwr_i2c_scl_pz6 {
				nvidia,pins = "pwr_i2c_scl_pz6";
				nvidia,function = "i2cpwr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			pwr_i2c_sda_pz7 {
				nvidia,pins = "pwr_i2c_sda_pz7";
				nvidia,function = "i2cpwr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat0_paa0 {
				nvidia,pins = "sdmmc4_dat0_paa0";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat1_paa1 {
				nvidia,pins = "sdmmc4_dat1_paa1";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat2_paa2 {
				nvidia,pins = "sdmmc4_dat2_paa2";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat3_paa3 {
				nvidia,pins = "sdmmc4_dat3_paa3";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat4_paa4 {
				nvidia,pins = "sdmmc4_dat4_paa4";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat5_paa5 {
				nvidia,pins = "sdmmc4_dat5_paa5";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat6_paa6 {
				nvidia,pins = "sdmmc4_dat6_paa6";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_dat7_paa7 {
				nvidia,pins = "sdmmc4_dat7_paa7";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pbb0 {
				nvidia,pins = "pbb0";
				nvidia,function = "vimclk2_alt";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			cam_i2c_scl_pbb1 {
				nvidia,pins = "cam_i2c_scl_pbb1";
				nvidia,function = "i2c3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			cam_i2c_sda_pbb2 {
				nvidia,pins = "cam_i2c_sda_pbb2";
				nvidia,function = "i2c3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			pbb3 {
				nvidia,pins = "pbb3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pbb4 {
				nvidia,pins = "pbb4";
				nvidia,function = "vgp4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pbb5 {
				nvidia,pins = "pbb5";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pbb6 {
				nvidia,pins = "pbb6";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pbb7 {
				nvidia,pins = "pbb7";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			cam_mclk_pcc0 {
				nvidia,pins = "cam_mclk_pcc0";
				nvidia,function = "vi_alt3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pcc1 {
				nvidia,pins = "pcc1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pcc2 {
				nvidia,pins = "pcc2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_clk_pcc4 {
				nvidia,pins = "sdmmc4_clk_pcc4";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			clk2_req_pcc5 {
				nvidia,pins = "clk2_req_pcc5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pex_l0_rst_n_pdd1 {
				nvidia,pins = "pex_l0_rst_n_pdd1";
				nvidia,function = "pe0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pex_l0_clkreq_n_pdd2 {
				nvidia,pins = "pex_l0_clkreq_n_pdd2";
				nvidia,function = "pe0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pex_wake_n_pdd3 {
				nvidia,pins = "pex_wake_n_pdd3";
				nvidia,function = "pe";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pex_l1_rst_n_pdd5 {
				nvidia,pins = "pex_l1_rst_n_pdd5";
				nvidia,function = "pe1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pex_l1_clkreq_n_pdd6 {
				nvidia,pins = "pex_l1_clkreq_n_pdd6";
				nvidia,function = "pe1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			clk3_out_pee0 {
				nvidia,pins = "clk3_out_pee0";
				nvidia,function = "extperiph3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			clk3_req_pee1 {
				nvidia,pins = "clk3_req_pee1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap_mclk1_req_pee2 {
				nvidia,pins = "dap_mclk1_req_pee2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			hdmi_cec_pee3 {
				nvidia,pins = "hdmi_cec_pee3";
				nvidia,function = "cec";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_DISABLE>;
			};
			sdmmc3_clk_lb_out_pee4 {
				nvidia,pins = "sdmmc3_clk_lb_out_pee4";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_clk_lb_in_pee5 {
				nvidia,pins = "sdmmc3_clk_lb_in_pee5";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dp_hpd_pff0 {
				nvidia,pins = "dp_hpd_pff0";
				nvidia,function = "dp";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			usb_vbus_en2_pff1 {
				nvidia,pins = "usb_vbus_en2_pff1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
				nvidia,open-drain = <TEGRA_PIN_DISABLE>;
			};
			pff2 {
				nvidia,pins = "pff2";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
				nvidia,open-drain = <TEGRA_PIN_DISABLE>;
			};
			core_pwr_req {
				nvidia,pins = "core_pwr_req";
				nvidia,function = "pwron";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			cpu_pwr_req {
				nvidia,pins = "cpu_pwr_req";
				nvidia,function = "cpu";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pwr_int_n {
				nvidia,pins = "pwr_int_n";
				nvidia,function = "pmi";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			reset_out_n {
				nvidia,pins = "reset_out_n";
				nvidia,function = "reset_out_n";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			clk_32k_in {
				nvidia,pins = "clk_32k_in";
				nvidia,function = "clk";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			jtag_rtck {
				nvidia,pins = "jtag_rtck";
				nvidia,function = "rtck";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dsi_b {
				nvidia,pins = "mipi_pad_ctrl_dsi_b";
				nvidia,function = "dsi_b";
			};
		};
	};

	/*
	 * First high speed UART, exposed on the expansion connector J3A2
	 *   Pin 41: BR_UART1_TXD
	 *   Pin 44: BR_UART1_RXD
	 */
	serial@70006000 {
		compatible = "nvidia,tegra124-hsuart", "nvidia,tegra30-hsuart";
		reset-names = "serial";
		/delete-property/ reg-shift;
		status = "okay";
	};

	/*
	 * Second high speed UART, exposed on the expansion connector J3A2
	 *   Pin 65: UART2_RXD
	 *   Pin 68: UART2_TXD
	 *   Pin 71: UART2_CTS_L
	 *   Pin 74: UART2_RTS_L
	 */
	serial@70006040 {
		compatible = "nvidia,tegra124-hsuart", "nvidia,tegra30-hsuart";
		reset-names = "serial";
		/delete-property/ reg-shift;
		status = "okay";
	};

	/* DB9 serial port */
	serial@70006300 {
		/delete-property/ dmas;
		/delete-property/ dma-names;
		status = "okay";
	};

	/* Expansion GEN1_I2C_*, mini-PCIe I2C, on-board components */
	i2c@7000c000 {
		status = "okay";
		clock-frequency = <100000>;

		rt5639: audio-codec@1c {
			compatible = "realtek,rt5639";
			reg = <0x1c>;
			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(H, 4) IRQ_TYPE_EDGE_FALLING>;
			realtek,ldo1-en-gpios =
				<&gpio TEGRA_GPIO(R, 2) GPIO_ACTIVE_HIGH>;
		};

		temperature-sensor@4c {
			compatible = "ti,tmp451";
			reg = <0x4c>;
			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(I, 6) IRQ_TYPE_EDGE_FALLING>;
		};

		eeprom@56 {
			compatible = "atmel,24c02";
			reg = <0x56>;
			pagesize = <8>;
		};
	};

	/* Expansion GEN2_I2C_* */
	i2c@7000c400 {
		status = "okay";
		clock-frequency = <100000>;
	};

	/* Expansion CAM_I2C_* */
	i2c@7000c500 {
		status = "okay";
		clock-frequency = <100000>;
	};

	/* HDMI DDC */
	hdmi_ddc: i2c@7000c700 {
		status = "okay";
		clock-frequency = <100000>;
	};

	/* Expansion PWR_I2C_*, on-board components */
	i2c@7000d000 {
		status = "okay";
		clock-frequency = <400000>;

		pmic: pmic@40 {
			compatible = "ams,as3722";
			reg = <0x40>;
			interrupts = <0 86 IRQ_TYPE_LEVEL_HIGH>;

			ams,system-power-controller;

			#interrupt-cells = <2>;
			interrupt-controller;

			gpio-controller;
			#gpio-cells = <2>;

			pinctrl-names = "default";
			pinctrl-0 = <&as3722_default>;

			as3722_default: pinmux {
				gpio0 {
					pins = "gpio0";
					function = "gpio";
					bias-pull-down;
				};

				gpio1_2_4_7 {
					pins = "gpio1", "gpio2", "gpio4", "gpio7";
					function = "gpio";
					bias-pull-up;
				};

				gpio3_5_6 {
					pins = "gpio3", "gpio5", "gpio6";
					bias-high-impedance;
				};
			};

			regulators {
				vsup-sd2-supply = <&vdd_5v0_sys>;
				vsup-sd3-supply = <&vdd_5v0_sys>;
				vsup-sd4-supply = <&vdd_5v0_sys>;
				vsup-sd5-supply = <&vdd_5v0_sys>;
				vin-ldo0-supply = <&vdd_1v35_lp0>;
				vin-ldo1-6-supply = <&vdd_3v3_run>;
				vin-ldo2-5-7-supply = <&vddio_1v8>;
				vin-ldo3-4-supply = <&vdd_3v3_sys>;
				vin-ldo9-10-supply = <&vdd_5v0_sys>;
				vin-ldo11-supply = <&vdd_3v3_run>;

				vdd_cpu: sd0 {
					regulator-name = "+VDD_CPU_AP";
					regulator-min-microvolt = <700000>;
					regulator-max-microvolt = <1400000>;
					regulator-min-microamp = <3500000>;
					regulator-max-microamp = <3500000>;
					regulator-always-on;
					regulator-boot-on;
					ams,ext-control = <2>;
				};

				sd1 {
					regulator-name = "+VDD_CORE";
					regulator-min-microvolt = <700000>;
					regulator-max-microvolt = <1350000>;
					regulator-min-microamp = <2500000>;
					regulator-max-microamp = <2500000>;
					regulator-always-on;
					regulator-boot-on;
					ams,ext-control = <1>;
				};

				vdd_1v35_lp0: sd2 {
					regulator-name = "+1.35V_LP0(sd2)";
					regulator-min-microvolt = <1350000>;
					regulator-max-microvolt = <1350000>;
					regulator-always-on;
					regulator-boot-on;
				};

				sd3 {
					regulator-name = "+1.35V_LP0(sd3)";
					regulator-min-microvolt = <1350000>;
					regulator-max-microvolt = <1350000>;
					regulator-always-on;
					regulator-boot-on;
				};

				vdd_1v05_run: sd4 {
					regulator-name = "+1.05V_RUN";
					regulator-min-microvolt = <1050000>;
					regulator-max-microvolt = <1050000>;
				};

				vddio_1v8: sd5 {
					regulator-name = "+1.8V_VDDIO";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-boot-on;
					regulator-always-on;
				};

				vdd_gpu: sd6 {
					regulator-name = "+VDD_GPU_AP";
					regulator-min-microvolt = <650000>;
					regulator-max-microvolt = <1200000>;
					regulator-min-microamp = <3500000>;
					regulator-max-microamp = <3500000>;
					regulator-boot-on;
					regulator-always-on;
				};

				avdd_1v05_run: ldo0 {
					regulator-name = "+1.05V_RUN_AVDD";
					regulator-min-microvolt = <1050000>;
					regulator-max-microvolt = <1050000>;
					regulator-boot-on;
					regulator-always-on;
					ams,ext-control = <1>;
				};

				ldo1 {
					regulator-name = "+1.8V_RUN_CAM";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo2 {
					regulator-name = "+1.2V_GEN_AVDD";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
					regulator-boot-on;
					regulator-always-on;
				};

				ldo3 {
					regulator-name = "+1.05V_LP0_VDD_RTC";
					regulator-min-microvolt = <1000000>;
					regulator-max-microvolt = <1000000>;
					regulator-boot-on;
					regulator-always-on;
					ams,enable-tracking;
				};

				ldo4 {
					regulator-name = "+2.8V_RUN_CAM";
					regulator-min-microvolt = <2800000>;
					regulator-max-microvolt = <2800000>;
				};

				ldo5 {
					regulator-name = "+1.2V_RUN_CAM_FRONT";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
				};

				vddio_sdmmc3: ldo6 {
					regulator-name = "+VDDIO_SDMMC3";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <3300000>;
				};

				ldo7 {
					regulator-name = "+1.05V_RUN_CAM_REAR";
					regulator-min-microvolt = <1050000>;
					regulator-max-microvolt = <1050000>;
				};

				ldo9 {
					regulator-name = "+3.3V_RUN_TOUCH";
					regulator-min-microvolt = <2800000>;
					regulator-max-microvolt = <2800000>;
				};

				ldo10 {
					regulator-name = "+2.8V_RUN_CAM_AF";
					regulator-min-microvolt = <2800000>;
					regulator-max-microvolt = <2800000>;
				};

				ldo11 {
					regulator-name = "+1.8V_RUN_VPP_FUSE";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};
			};
		};
	};

	/* Expansion TS_SPI_* */
	spi@7000d400 {
		status = "okay";
	};

	/* Internal SPI */
	spi@7000da00 {
		status = "okay";
		spi-max-frequency = <25000000>;

		flash@0 {
			compatible = "winbond,w25q32dw", "jedec,spi-nor";
			reg = <0>;
			spi-max-frequency = <20000000>;
		};
	};

	pmc@7000e400 {
		nvidia,invert-interrupt;
		nvidia,suspend-mode = <1>;
		nvidia,cpu-pwr-good-time = <500>;
		nvidia,cpu-pwr-off-time = <300>;
		nvidia,core-pwr-good-time = <641 3845>;
		nvidia,core-pwr-off-time = <61036>;
		nvidia,core-power-req-active-high;
		nvidia,sys-clock-req-active-high;

		i2c-thermtrip {
			nvidia,i2c-controller-id = <4>;
			nvidia,bus-addr = <0x40>;
			nvidia,reg-addr = <0x36>;
			nvidia,reg-data = <0x2>;
		};
	};

	cec@70015000 {
		status = "okay";
	};

	/* Serial ATA */
	sata@70020000 {
		status = "okay";

		phys = <&{/padctl@7009f000/pads/sata/lanes/sata-0}>;
		phy-names = "sata-0";

		hvdd-supply = <&vdd_3v3_lp0>;
		vddio-supply = <&vdd_1v05_run>;
		avdd-supply = <&vdd_1v05_run>;

		target-5v-supply = <&vdd_5v0_sata>;
		target-12v-supply = <&vdd_12v0_sata>;
	};

	hda@70030000 {
		status = "okay";
	};

	usb@70090000 {
		phys = <&{/padctl@7009f000/pads/usb2/lanes/usb2-0}>, /* Micro A/B */
		       <&{/padctl@7009f000/pads/usb2/lanes/usb2-1}>, /* Mini PCIe */
		       <&{/padctl@7009f000/pads/usb2/lanes/usb2-2}>, /* USB3 */
		       <&{/padctl@7009f000/pads/pcie/lanes/pcie-0}>; /* USB3 */
		phy-names = "usb2-0", "usb2-1", "usb2-2", "usb3-0";

		avddio-pex-supply = <&vdd_1v05_run>;
		dvddio-pex-supply = <&vdd_1v05_run>;
		avdd-usb-supply = <&vdd_3v3_lp0>;
		avdd-pll-utmip-supply = <&vddio_1v8>;
		avdd-pll-erefe-supply = <&avdd_1v05_run>;
		avdd-usb-ss-pll-supply = <&vdd_1v05_run>;
		hvdd-usb-ss-supply = <&vdd_3v3_lp0>;
		hvdd-usb-ss-pll-e-supply = <&vdd_3v3_lp0>;

		status = "okay";
	};

	padctl@7009f000 {
		status = "okay";

		avdd-pll-utmip-supply = <&vddio_1v8>;
		avdd-pll-erefe-supply = <&avdd_1v05_run>;
		avdd-pex-pll-supply = <&vdd_1v05_run>;
		hvdd-pex-pll-e-supply = <&vdd_3v3_lp0>;

		pads {
			usb2 {
				status = "okay";

				lanes {
					usb2-0 {
						nvidia,function = "snps";
						status = "okay";
					};

					usb2-1 {
						nvidia,function = "xusb";
						status = "okay";
					};

					usb2-2 {
						nvidia,function = "xusb";
						status = "okay";
					};
				};
			};

			pcie {
				status = "okay";

				lanes {
					pcie-0 {
						nvidia,function = "usb3-ss";
						status = "okay";
					};

					pcie-2 {
						nvidia,function = "pcie";
						status = "okay";
					};

					pcie-4 {
						nvidia,function = "pcie";
						status = "okay";
					};
				};
			};

			sata {
				status = "okay";

				lanes {
					sata-0 {
						nvidia,function = "sata";
						status = "okay";
					};
				};
			};
		};

		ports {
			/* Micro A/B */
			usb2-0 {
				status = "okay";
				mode = "host";
			};

			/* Mini PCIe */
			usb2-1 {
				status = "okay";
				mode = "host";
			};

			/* USB3 */
			usb2-2 {
				status = "okay";
				mode = "host";

				vbus-supply = <&vdd_usb3_vbus>;
			};

			usb3-0 {
				nvidia,usb2-companion = <2>;
				status = "okay";
			};
		};
	};

	/* SD card */
	mmc@700b0400 {
		status = "okay";
		cd-gpios = <&gpio TEGRA_GPIO(V, 2) GPIO_ACTIVE_LOW>;
		power-gpios = <&gpio TEGRA_GPIO(R, 0) GPIO_ACTIVE_HIGH>;
		wp-gpios = <&gpio TEGRA_GPIO(Q, 4) GPIO_ACTIVE_HIGH>;
		bus-width = <4>;
		vqmmc-supply = <&vddio_sdmmc3>;
	};

	/* eMMC */
	mmc@700b0600 {
		status = "okay";
		bus-width = <8>;
		non-removable;
	};

	/* CPU DFLL clock */
	clock@70110000 {
		status = "okay";
		vdd-cpu-supply = <&vdd_cpu>;
		nvidia,i2c-fs-rate = <400000>;
	};

	ahub@70300000 {
		i2s@70301100 {
			status = "okay";
		};
	};

	usb@7d000000 {
		compatible = "nvidia,tegra124-udc";
		status = "okay";
		dr_mode = "peripheral";
	};

	usb-phy@7d000000 {
		status = "okay";
	};

	/* mini-PCIe USB */
	usb@7d004000 {
		status = "okay";
	};

	usb-phy@7d004000 {
		status = "okay";
	};

	/* USB A connector */
	usb@7d008000 {
		status = "okay";
	};

	usb-phy@7d008000 {
		status = "okay";
		vbus-supply = <&vdd_usb3_vbus>;
	};

	clk32k_in: clock-32k {
		compatible = "fixed-clock";
		clock-frequency = <32768>;
		#clock-cells = <0>;
	};

	cpus {
		cpu@0 {
			vdd-cpu-supply = <&vdd_cpu>;
		};
	};

	gpio-keys {
		compatible = "gpio-keys";

		key-power {
			label = "Power";
			gpios = <&gpio TEGRA_GPIO(Q, 0) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_POWER>;
			debounce-interval = <10>;
			wakeup-source;
		};
	};

	vdd_mux: regulator-mux {
		compatible = "regulator-fixed";
		regulator-name = "+VDD_MUX";
		regulator-min-microvolt = <12000000>;
		regulator-max-microvolt = <12000000>;
		regulator-always-on;
		regulator-boot-on;
	};

	vdd_5v0_sys: regulator-5v0sys {
		compatible = "regulator-fixed";
		regulator-name = "+5V_SYS";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-always-on;
		regulator-boot-on;
		vin-supply = <&vdd_mux>;
	};

	vdd_3v3_sys: regulator-3v3sys {
		compatible = "regulator-fixed";
		regulator-name = "+3.3V_SYS";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
		regulator-boot-on;
		vin-supply = <&vdd_mux>;
	};

	vdd_3v3_run: regulator-3v3run {
		compatible = "regulator-fixed";
		regulator-name = "+3.3V_RUN";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
		regulator-boot-on;
		gpio = <&pmic 1 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_3v3_sys>;
	};

	vdd_3v3_hdmi: regulator-3v3hdmi {
		compatible = "regulator-fixed";
		regulator-name = "+3.3V_AVDD_HDMI_AP_GATED";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&vdd_3v3_run>;
	};

	vdd_usb1_vbus: regulator-usb1 {
		compatible = "regulator-fixed";
		regulator-name = "+USB0_VBUS_SW";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio TEGRA_GPIO(N, 4) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		gpio-open-drain;
		vin-supply = <&vdd_5v0_sys>;
	};

	vdd_usb3_vbus: regulator-usb3 {
		compatible = "regulator-fixed";
		regulator-name = "+5V_USB_HS";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio TEGRA_GPIO(N, 5) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		gpio-open-drain;
		vin-supply = <&vdd_5v0_sys>;
	};

	vdd_3v3_lp0: regulator-lp0 {
		compatible = "regulator-fixed";
		regulator-name = "+3.3V_LP0";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
		regulator-boot-on;
		gpio = <&pmic 2 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_3v3_sys>;
	};

	vdd_hdmi_pll: regulator-hdmipll {
		compatible = "regulator-fixed";
		regulator-name = "+1.05V_RUN_AVDD_HDMI_PLL";
		regulator-min-microvolt = <1050000>;
		regulator-max-microvolt = <1050000>;
		gpio = <&gpio TEGRA_GPIO(H, 7) GPIO_ACTIVE_LOW>;
		vin-supply = <&vdd_1v05_run>;
	};

	vdd_5v0_hdmi: regulator-hdmicon {
		compatible = "regulator-fixed";
		regulator-name = "+5V_HDMI_CON";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio TEGRA_GPIO(K, 6) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_5v0_sys>;
	};

	/* Molex power connector */
	vdd_5v0_sata: regulator-5v0sata {
		compatible = "regulator-fixed";
		regulator-name = "+5V_SATA";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio TEGRA_GPIO(EE, 2) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_5v0_sys>;
	};

	vdd_12v0_sata: regulator-12v0sata {
		compatible = "regulator-fixed";
		regulator-name = "+12V_SATA";
		regulator-min-microvolt = <12000000>;
		regulator-max-microvolt = <12000000>;
		gpio = <&gpio TEGRA_GPIO(EE, 2) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_mux>;
	};

	sound {
		compatible = "nvidia,tegra-audio-rt5640-jetson-tk1",
			     "nvidia,tegra-audio-rt5640";
		nvidia,model = "NVIDIA Tegra Jetson TK1";

		nvidia,audio-routing =
			"Headphones", "HPOR",
			"Headphones", "HPOL",
			"Mic Jack", "MICBIAS1",
			"IN2P", "Mic Jack";

		nvidia,i2s-controller = <&tegra_i2s1>;
		nvidia,audio-codec = <&rt5639>;

		nvidia,hp-det-gpios = <&gpio TEGRA_GPIO(R, 7) GPIO_ACTIVE_LOW>;

		clocks = <&tegra_car TEGRA124_CLK_PLL_A>,
			 <&tegra_car TEGRA124_CLK_PLL_A_OUT0>,
			 <&tegra_pmc TEGRA_PMC_CLK_OUT_1>;
		clock-names = "pll_a", "pll_a_out0", "mclk";

		assigned-clocks = <&tegra_car TEGRA124_CLK_EXTERN1>,
				  <&tegra_pmc TEGRA_PMC_CLK_OUT_1>;

		assigned-clock-parents = <&tegra_car TEGRA124_CLK_PLL_A_OUT0>,
					 <&tegra_car TEGRA124_CLK_EXTERN1>;
	};

	thermal-zones {
		cpu-thermal {
			trips {
				cpu-shutdown-trip {
					temperature = <101000>;
					hysteresis = <0>;
					type = "critical";
				};
			};
		};

		mem-thermal {
			trips {
				mem-shutdown-trip {
					temperature = <101000>;
					hysteresis = <0>;
					type = "critical";
				};
			};
		};

		gpu-thermal {
			trips {
				gpu-shutdown-trip {
					temperature = <101000>;
					hysteresis = <0>;
					type = "critical";
				};
			};
		};
	};
};
