// SPDX-License-Identifier: GPL-2.0+
#include <dt-bindings/clock/aspeed-clock.h>
#include <dt-bindings/interrupt-controller/aspeed-scu-ic.h>

/ {
	model = "Aspeed BMC";
	compatible = "aspeed,ast2500";
	#address-cells = <1>;
	#size-cells = <1>;
	interrupt-parent = <&vic>;

	aliases {
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		i2c2 = &i2c2;
		i2c3 = &i2c3;
		i2c4 = &i2c4;
		i2c5 = &i2c5;
		i2c6 = &i2c6;
		i2c7 = &i2c7;
		i2c8 = &i2c8;
		i2c9 = &i2c9;
		i2c10 = &i2c10;
		i2c11 = &i2c11;
		i2c12 = &i2c12;
		i2c13 = &i2c13;
		serial0 = &uart1;
		serial1 = &uart2;
		serial2 = &uart3;
		serial3 = &uart4;
		serial4 = &uart5;
		serial5 = &vuart;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu@0 {
			compatible = "arm,arm1176jzf-s";
			device_type = "cpu";
			reg = <0>;
		};
	};

	memory@80000000 {
		device_type = "memory";
		reg = <0x80000000 0>;
	};

	ahb {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		fmc: spi@1e620000 {
			reg = <0x1e620000 0xc4>, <0x20000000 0x10000000>;
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "aspeed,ast2500-fmc";
			clocks = <&syscon ASPEED_CLK_AHB>;
			status = "disabled";
			interrupts = <19>;
			flash@0 {
				reg = < 0 >;
				compatible = "jedec,spi-nor";
				spi-max-frequency = <50000000>;
				spi-rx-bus-width = <2>;
				status = "disabled";
			};
			flash@1 {
				reg = < 1 >;
				compatible = "jedec,spi-nor";
				spi-max-frequency = <50000000>;
				spi-rx-bus-width = <2>;
				status = "disabled";
			};
			flash@2 {
				reg = < 2 >;
				compatible = "jedec,spi-nor";
				spi-max-frequency = <50000000>;
				spi-rx-bus-width = <2>;
				status = "disabled";
			};
		};

		spi1: spi@1e630000 {
			reg = <0x1e630000 0xc4>, <0x30000000 0x08000000>;
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "aspeed,ast2500-spi";
			clocks = <&syscon ASPEED_CLK_AHB>;
			status = "disabled";
			flash@0 {
				reg = < 0 >;
				compatible = "jedec,spi-nor";
				spi-max-frequency = <50000000>;
				spi-rx-bus-width = <2>;
				status = "disabled";
			};
			flash@1 {
				reg = < 1 >;
				compatible = "jedec,spi-nor";
				spi-max-frequency = <50000000>;
				spi-rx-bus-width = <2>;
				status = "disabled";
			};
		};

		spi2: spi@1e631000 {
			reg = <0x1e631000 0xc4>, <0x38000000 0x08000000>;
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "aspeed,ast2500-spi";
			clocks = <&syscon ASPEED_CLK_AHB>;
			status = "disabled";
			flash@0 {
				reg = < 0 >;
				compatible = "jedec,spi-nor";
				spi-max-frequency = <50000000>;
				spi-rx-bus-width = <2>;
				status = "disabled";
			};
			flash@1 {
				reg = < 1 >;
				compatible = "jedec,spi-nor";
				spi-max-frequency = <50000000>;
				spi-rx-bus-width = <2>;
				status = "disabled";
			};
		};

		vic: interrupt-controller@1e6c0080 {
			compatible = "aspeed,ast2400-vic";
			interrupt-controller;
			#interrupt-cells = <1>;
			valid-sources = <0xfefff7ff 0x0807ffff>;
			reg = <0x1e6c0080 0x80>;
		};

		cvic: interrupt-controller@1e6c2000 {
			compatible = "aspeed,ast2500-cvic", "aspeed,cvic";
			valid-sources = <0xffffffff>;
			copro-sw-interrupts = <1>;
			reg = <0x1e6c2000 0x80>;
		};

		mac0: ethernet@1e660000 {
			compatible = "aspeed,ast2500-mac", "faraday,ftgmac100";
			reg = <0x1e660000 0x180>;
			interrupts = <2>;
			clocks = <&syscon ASPEED_CLK_GATE_MAC1CLK>;
			status = "disabled";
		};

		mac1: ethernet@1e680000 {
			compatible = "aspeed,ast2500-mac", "faraday,ftgmac100";
			reg = <0x1e680000 0x180>;
			interrupts = <3>;
			clocks = <&syscon ASPEED_CLK_GATE_MAC2CLK>;
			status = "disabled";
		};

		ehci0: usb@1e6a1000 {
			compatible = "aspeed,ast2500-ehci", "generic-ehci";
			reg = <0x1e6a1000 0x100>;
			interrupts = <5>;
			clocks = <&syscon ASPEED_CLK_GATE_USBPORT1CLK>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_usb2ah_default>;
			status = "disabled";
		};

		ehci1: usb@1e6a3000 {
			compatible = "aspeed,ast2500-ehci", "generic-ehci";
			reg = <0x1e6a3000 0x100>;
			interrupts = <13>;
			clocks = <&syscon ASPEED_CLK_GATE_USBPORT2CLK>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_usb2bh_default>;
			status = "disabled";
		};

		uhci: usb@1e6b0000 {
			compatible = "aspeed,ast2500-uhci", "generic-uhci";
			reg = <0x1e6b0000 0x100>;
			interrupts = <14>;
			#ports = <2>;
			clocks = <&syscon ASPEED_CLK_GATE_USBUHCICLK>;
			status = "disabled";
			/*
			 * No default pinmux, it will follow EHCI, use an explicit pinmux
			 * override if you don't enable EHCI
			 */
		};

		vhub: usb-vhub@1e6a0000 {
			compatible = "aspeed,ast2500-usb-vhub";
			reg = <0x1e6a0000 0x300>;
			interrupts = <5>;
			clocks = <&syscon ASPEED_CLK_GATE_USBPORT1CLK>;
			aspeed,vhub-downstream-ports = <5>;
			aspeed,vhub-generic-endpoints = <15>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_usb2ad_default>;
			status = "disabled";
		};

		apb {
			compatible = "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			edac: memory-controller@1e6e0000 {
				compatible = "aspeed,ast2500-sdram-edac";
				reg = <0x1e6e0000 0x174>;
				interrupts = <0>;
				status = "disabled";
			};

			syscon: syscon@1e6e2000 {
				compatible = "aspeed,ast2500-scu", "syscon", "simple-mfd";
				reg = <0x1e6e2000 0x1a8>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0x1e6e2000 0x1000>;
				#clock-cells = <1>;
				#reset-cells = <1>;

				scu_ic: interrupt-controller@18 {
					#interrupt-cells = <1>;
					compatible = "aspeed,ast2500-scu-ic";
					reg = <0x18 0x4>;
					interrupts = <21>;
					interrupt-controller;
				};

				p2a: p2a-control@2c {
					compatible = "aspeed,ast2500-p2a-ctrl";
					reg = <0x2c 0x4>;
					status = "disabled";
				};

				silicon-id@7c {
					compatible = "aspeed,ast2500-silicon-id", "aspeed,silicon-id";
					reg = <0x7c 0x4 0x150 0x8>;
				};

				pinctrl: pinctrl@80 {
					compatible = "aspeed,ast2500-pinctrl";
					reg = <0x80 0x18>, <0xa0 0x10>;
					aspeed,external-nodes = <&gfx>, <&lhc>;
				};
			};

			rng: hwrng@1e6e2078 {
				compatible = "timeriomem_rng";
				reg = <0x1e6e2078 0x4>;
				period = <1>;
				quality = <100>;
			};

			hace: crypto@1e6e3000 {
				compatible = "aspeed,ast2500-hace";
				reg = <0x1e6e3000 0x100>;
				interrupts = <4>;
				clocks = <&syscon ASPEED_CLK_GATE_YCLK>;
				resets = <&syscon ASPEED_RESET_HACE>;
			};

			gfx: display@1e6e6000 {
				compatible = "aspeed,ast2500-gfx", "syscon";
				reg = <0x1e6e6000 0x1000>;
				reg-io-width = <4>;
				clocks = <&syscon ASPEED_CLK_GATE_D1CLK>;
				resets = <&syscon ASPEED_RESET_CRT1>;
				syscon = <&syscon>;
				status = "disabled";
				interrupts = <0x19>;
			};

			adc: adc@1e6e9000 {
				compatible = "aspeed,ast2500-adc";
				reg = <0x1e6e9000 0xb0>;
				clocks = <&syscon ASPEED_CLK_APB>;
				resets = <&syscon ASPEED_RESET_ADC>;
				#io-channel-cells = <1>;
				status = "disabled";
			};

			video: video@1e700000 {
				compatible = "aspeed,ast2500-video-engine";
				reg = <0x1e700000 0x1000>;
				clocks = <&syscon ASPEED_CLK_GATE_VCLK>,
					 <&syscon ASPEED_CLK_GATE_ECLK>;
				clock-names = "vclk", "eclk";
				interrupts = <7>;
				status = "disabled";
			};

			sram: sram@1e720000 {
				compatible = "mmio-sram";
				reg = <0x1e720000 0x9000>;	// 36K
				ranges;
				#address-cells = <1>;
				#size-cells = <1>;
			};

			sdmmc: sd-controller@1e740000 {
				compatible = "aspeed,ast2500-sd-controller";
				reg = <0x1e740000 0x100>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0x1e740000 0x10000>;
				clocks = <&syscon ASPEED_CLK_GATE_SDCLK>;
				status = "disabled";

				sdhci0: sdhci@100 {
					compatible = "aspeed,ast2500-sdhci";
					reg = <0x100 0x100>;
					interrupts = <26>;
					sdhci,auto-cmd12;
					clocks = <&syscon ASPEED_CLK_SDIO>;
					status = "disabled";
				};

				sdhci1: sdhci@200 {
					compatible = "aspeed,ast2500-sdhci";
					reg = <0x200 0x100>;
					interrupts = <26>;
					sdhci,auto-cmd12;
					clocks = <&syscon ASPEED_CLK_SDIO>;
					status = "disabled";
				};
			};

			gpio: gpio@1e780000 {
				#gpio-cells = <2>;
				gpio-controller;
				compatible = "aspeed,ast2500-gpio";
				reg = <0x1e780000 0x200>;
				interrupts = <20>;
				gpio-ranges = <&pinctrl 0 0 232>;
				clocks = <&syscon ASPEED_CLK_APB>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			sgpio: sgpio@1e780200 {
				#gpio-cells = <2>;
				compatible = "aspeed,ast2500-sgpio";
				gpio-controller;
				interrupts = <40>;
				reg = <0x1e780200 0x0100>;
				clocks = <&syscon ASPEED_CLK_APB>;
				#interrupt-cells = <2>;
				interrupt-controller;
				bus-frequency = <12000000>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_sgpm_default>;
				status = "disabled";
			};

			rtc: rtc@1e781000 {
				compatible = "aspeed,ast2500-rtc";
				reg = <0x1e781000 0x18>;
				status = "disabled";
			};

			timer: timer@1e782000 {
				/* This timer is a Faraday FTTMR010 derivative */
				compatible = "aspeed,ast2400-timer";
				reg = <0x1e782000 0x90>;
				interrupts = <16 17 18 35 36 37 38 39>;
				clocks = <&syscon ASPEED_CLK_APB>;
				clock-names = "PCLK";
			};

			uart1: serial@1e783000 {
				compatible = "ns16550a";
				reg = <0x1e783000 0x20>;
				reg-shift = <2>;
				interrupts = <9>;
				clocks = <&syscon ASPEED_CLK_GATE_UART1CLK>;
				resets = <&lpc_reset 4>;
				no-loopback-test;
				status = "disabled";
			};

			uart5: serial@1e784000 {
				compatible = "ns16550a";
				reg = <0x1e784000 0x20>;
				reg-shift = <2>;
				interrupts = <10>;
				clocks = <&syscon ASPEED_CLK_GATE_UART5CLK>;
				no-loopback-test;
				status = "disabled";
			};

			wdt1: watchdog@1e785000 {
				compatible = "aspeed,ast2500-wdt";
				reg = <0x1e785000 0x20>;
				clocks = <&syscon ASPEED_CLK_APB>;
			};

			wdt2: watchdog@1e785020 {
				compatible = "aspeed,ast2500-wdt";
				reg = <0x1e785020 0x20>;
				clocks = <&syscon ASPEED_CLK_APB>;
			};

			wdt3: watchdog@1e785040 {
				compatible = "aspeed,ast2500-wdt";
				reg = <0x1e785040 0x20>;
				clocks = <&syscon ASPEED_CLK_APB>;
				status = "disabled";
			};

			pwm_tacho: pwm-tacho-controller@1e786000 {
				compatible = "aspeed,ast2500-pwm-tacho";
				#address-cells = <1>;
				#size-cells = <0>;
				reg = <0x1e786000 0x1000>;
				clocks = <&syscon ASPEED_CLK_24M>;
				resets = <&syscon ASPEED_RESET_PWM>;
				status = "disabled";
			};

			vuart: serial@1e787000 {
				compatible = "aspeed,ast2500-vuart";
				reg = <0x1e787000 0x40>;
				reg-shift = <2>;
				interrupts = <8>;
				clocks = <&syscon ASPEED_CLK_APB>;
				no-loopback-test;
				status = "disabled";
			};

			lpc: lpc@1e789000 {
				compatible = "aspeed,ast2500-lpc-v2", "simple-mfd", "syscon";
				reg = <0x1e789000 0x1000>;
				reg-io-width = <4>;

				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0x0 0x1e789000 0x1000>;

				kcs1: kcs@24 {
					compatible = "aspeed,ast2500-kcs-bmc-v2";
					reg = <0x24 0x1>, <0x30 0x1>, <0x3c 0x1>;
					interrupts = <8>;
					clocks = <&syscon ASPEED_CLK_GATE_LCLK>;
					status = "disabled";
				};

				kcs2: kcs@28 {
					compatible = "aspeed,ast2500-kcs-bmc-v2";
					reg = <0x28 0x1>, <0x34 0x1>, <0x40 0x1>;
					interrupts = <8>;
					clocks = <&syscon ASPEED_CLK_GATE_LCLK>;
					status = "disabled";
				};

				kcs3: kcs@2c {
					compatible = "aspeed,ast2500-kcs-bmc-v2";
					reg = <0x2c 0x1>, <0x38 0x1>, <0x44 0x1>;
					interrupts = <8>;
					clocks = <&syscon ASPEED_CLK_GATE_LCLK>;
					status = "disabled";
				};

				kcs4: kcs@114 {
					compatible = "aspeed,ast2500-kcs-bmc-v2";
					reg = <0x114 0x1>, <0x118 0x1>, <0x11c 0x1>;
					interrupts = <8>;
					clocks = <&syscon ASPEED_CLK_GATE_LCLK>;
					status = "disabled";
				};

				lpc_ctrl: lpc-ctrl@80 {
					compatible = "aspeed,ast2500-lpc-ctrl";
					reg = <0x80 0x10>;
					clocks = <&syscon ASPEED_CLK_GATE_LCLK>;
					status = "disabled";
				};

				lpc_snoop: lpc-snoop@90 {
					compatible = "aspeed,ast2500-lpc-snoop";
					reg = <0x90 0x8>;
					interrupts = <8>;
					clocks = <&syscon ASPEED_CLK_GATE_LCLK>;
					status = "disabled";
				};

				lpc_reset: reset-controller@98 {
					compatible = "aspeed,ast2500-lpc-reset";
					reg = <0x98 0x4>;
					#reset-cells = <1>;
				};

				uart_routing: uart-routing@9c {
					compatible = "aspeed,ast2500-uart-routing";
					reg = <0x9c 0x4>;
					status = "disabled";
				};

				lhc: lhc@a0 {
					compatible = "aspeed,ast2500-lhc";
					reg = <0xa0 0x24 0xc8 0x8>;
				};


				ibt: ibt@140 {
					compatible = "aspeed,ast2500-ibt-bmc";
					reg = <0x140 0x18>;
					interrupts = <8>;
					clocks = <&syscon ASPEED_CLK_GATE_LCLK>;
					status = "disabled";
				};
			};

			peci0: peci-controller@1e78b000 {
				compatible = "aspeed,ast2500-peci";
				reg = <0x1e78b000 0x60>;
				interrupts = <15>;
				clocks = <&syscon ASPEED_CLK_GATE_REFCLK>;
				resets = <&syscon ASPEED_RESET_PECI>;
				cmd-timeout-ms = <1000>;
				clock-frequency = <1000000>;
				status = "disabled";
			};

			uart2: serial@1e78d000 {
				compatible = "ns16550a";
				reg = <0x1e78d000 0x20>;
				reg-shift = <2>;
				interrupts = <32>;
				clocks = <&syscon ASPEED_CLK_GATE_UART2CLK>;
				resets = <&lpc_reset 5>;
				no-loopback-test;
				status = "disabled";
			};

			uart3: serial@1e78e000 {
				compatible = "ns16550a";
				reg = <0x1e78e000 0x20>;
				reg-shift = <2>;
				interrupts = <33>;
				clocks = <&syscon ASPEED_CLK_GATE_UART3CLK>;
				resets = <&lpc_reset 6>;
				no-loopback-test;
				status = "disabled";
			};

			uart4: serial@1e78f000 {
				compatible = "ns16550a";
				reg = <0x1e78f000 0x20>;
				reg-shift = <2>;
				interrupts = <34>;
				clocks = <&syscon ASPEED_CLK_GATE_UART4CLK>;
				resets = <&lpc_reset 7>;
				no-loopback-test;
				status = "disabled";
			};

			i2c: bus@1e78a000 {
				compatible = "simple-bus";
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0x1e78a000 0x1000>;
			};
		};
	};
};

&i2c {
	i2c_ic: interrupt-controller@0 {
		#interrupt-cells = <1>;
		compatible = "aspeed,ast2500-i2c-ic";
		reg = <0x0 0x40>;
		interrupts = <12>;
		interrupt-controller;
	};

	i2c0: i2c@40 {
		#address-cells = <1>;
		#size-cells = <0>;

		reg = <0x40 0x40>;
		compatible = "aspeed,ast2500-i2c-bus";
		clocks = <&syscon ASPEED_CLK_APB>;
		resets = <&syscon ASPEED_RESET_I2C>;
		bus-frequency = <100000>;
		interrupts = <0>;
		interrupt-parent = <&i2c_ic>;
		status = "disabled";
		/* Does not need pinctrl properties */
	};

	i2c1: i2c@80 {
		#address-cells = <1>;
		#size-cells = <0>;

		reg = <0x80 0x40>;
		compatible = "aspeed,ast2500-i2c-bus";
		clocks = <&syscon ASPEED_CLK_APB>;
		resets = <&syscon ASPEED_RESET_I2C>;
		bus-frequency = <100000>;
		interrupts = <1>;
		interrupt-parent = <&i2c_ic>;
		status = "disabled";
		/* Does not need pinctrl properties */
	};

	i2c2: i2c@c0 {
		#address-cells = <1>;
		#size-cells = <0>;

		reg = <0xc0 0x40>;
		compatible = "aspeed,ast2500-i2c-bus";
		clocks = <&syscon ASPEED_CLK_APB>;
		resets = <&syscon ASPEED_RESET_I2C>;
		bus-frequency = <100000>;
		interrupts = <2>;
		interrupt-parent = <&i2c_ic>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c3_default>;
		status = "disabled";
	};

	i2c3: i2c@100 {
		#address-cells = <1>;
		#size-cells = <0>;

		reg = <0x100 0x40>;
		compatible = "aspeed,ast2500-i2c-bus";
		clocks = <&syscon ASPEED_CLK_APB>;
		resets = <&syscon ASPEED_RESET_I2C>;
		bus-frequency = <100000>;
		interrupts = <3>;
		interrupt-parent = <&i2c_ic>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c4_default>;
		status = "disabled";
	};

	i2c4: i2c@140 {
		#address-cells = <1>;
		#size-cells = <0>;

		reg = <0x140 0x40>;
		compatible = "aspeed,ast2500-i2c-bus";
		clocks = <&syscon ASPEED_CLK_APB>;
		resets = <&syscon ASPEED_RESET_I2C>;
		bus-frequency = <100000>;
		interrupts = <4>;
		interrupt-parent = <&i2c_ic>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c5_default>;
		status = "disabled";
	};

	i2c5: i2c@180 {
		#address-cells = <1>;
		#size-cells = <0>;

		reg = <0x180 0x40>;
		compatible = "aspeed,ast2500-i2c-bus";
		clocks = <&syscon ASPEED_CLK_APB>;
		resets = <&syscon ASPEED_RESET_I2C>;
		bus-frequency = <100000>;
		interrupts = <5>;
		interrupt-parent = <&i2c_ic>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c6_default>;
		status = "disabled";
	};

	i2c6: i2c@1c0 {
		#address-cells = <1>;
		#size-cells = <0>;

		reg = <0x1c0 0x40>;
		compatible = "aspeed,ast2500-i2c-bus";
		clocks = <&syscon ASPEED_CLK_APB>;
		resets = <&syscon ASPEED_RESET_I2C>;
		bus-frequency = <100000>;
		interrupts = <6>;
		interrupt-parent = <&i2c_ic>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c7_default>;
		status = "disabled";
	};

	i2c7: i2c@300 {
		#address-cells = <1>;
		#size-cells = <0>;

		reg = <0x300 0x40>;
		compatible = "aspeed,ast2500-i2c-bus";
		clocks = <&syscon ASPEED_CLK_APB>;
		resets = <&syscon ASPEED_RESET_I2C>;
		bus-frequency = <100000>;
		interrupts = <7>;
		interrupt-parent = <&i2c_ic>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c8_default>;
		status = "disabled";
	};

	i2c8: i2c@340 {
		#address-cells = <1>;
		#size-cells = <0>;

		reg = <0x340 0x40>;
		compatible = "aspeed,ast2500-i2c-bus";
		clocks = <&syscon ASPEED_CLK_APB>;
		resets = <&syscon ASPEED_RESET_I2C>;
		bus-frequency = <100000>;
		interrupts = <8>;
		interrupt-parent = <&i2c_ic>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c9_default>;
		status = "disabled";
	};

	i2c9: i2c@380 {
		#address-cells = <1>;
		#size-cells = <0>;

		reg = <0x380 0x40>;
		compatible = "aspeed,ast2500-i2c-bus";
		clocks = <&syscon ASPEED_CLK_APB>;
		resets = <&syscon ASPEED_RESET_I2C>;
		bus-frequency = <100000>;
		interrupts = <9>;
		interrupt-parent = <&i2c_ic>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c10_default>;
		status = "disabled";
	};

	i2c10: i2c@3c0 {
		#address-cells = <1>;
		#size-cells = <0>;

		reg = <0x3c0 0x40>;
		compatible = "aspeed,ast2500-i2c-bus";
		clocks = <&syscon ASPEED_CLK_APB>;
		resets = <&syscon ASPEED_RESET_I2C>;
		bus-frequency = <100000>;
		interrupts = <10>;
		interrupt-parent = <&i2c_ic>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c11_default>;
		status = "disabled";
	};

	i2c11: i2c@400 {
		#address-cells = <1>;
		#size-cells = <0>;

		reg = <0x400 0x40>;
		compatible = "aspeed,ast2500-i2c-bus";
		clocks = <&syscon ASPEED_CLK_APB>;
		resets = <&syscon ASPEED_RESET_I2C>;
		bus-frequency = <100000>;
		interrupts = <11>;
		interrupt-parent = <&i2c_ic>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c12_default>;
		status = "disabled";
	};

	i2c12: i2c@440 {
		#address-cells = <1>;
		#size-cells = <0>;

		reg = <0x440 0x40>;
		compatible = "aspeed,ast2500-i2c-bus";
		clocks = <&syscon ASPEED_CLK_APB>;
		resets = <&syscon ASPEED_RESET_I2C>;
		bus-frequency = <100000>;
		interrupts = <12>;
		interrupt-parent = <&i2c_ic>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c13_default>;
		status = "disabled";
	};

	i2c13: i2c@480 {
		#address-cells = <1>;
		#size-cells = <0>;

		reg = <0x480 0x40>;
		compatible = "aspeed,ast2500-i2c-bus";
		clocks = <&syscon ASPEED_CLK_APB>;
		resets = <&syscon ASPEED_RESET_I2C>;
		bus-frequency = <100000>;
		interrupts = <13>;
		interrupt-parent = <&i2c_ic>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c14_default>;
		status = "disabled";
	};
};

&pinctrl {
	pinctrl_acpi_default: acpi_default {
		function = "ACPI";
		groups = "ACPI";
	};

	pinctrl_adc0_default: adc0_default {
		function = "ADC0";
		groups = "ADC0";
	};

	pinctrl_adc1_default: adc1_default {
		function = "ADC1";
		groups = "ADC1";
	};

	pinctrl_adc10_default: adc10_default {
		function = "ADC10";
		groups = "ADC10";
	};

	pinctrl_adc11_default: adc11_default {
		function = "ADC11";
		groups = "ADC11";
	};

	pinctrl_adc12_default: adc12_default {
		function = "ADC12";
		groups = "ADC12";
	};

	pinctrl_adc13_default: adc13_default {
		function = "ADC13";
		groups = "ADC13";
	};

	pinctrl_adc14_default: adc14_default {
		function = "ADC14";
		groups = "ADC14";
	};

	pinctrl_adc15_default: adc15_default {
		function = "ADC15";
		groups = "ADC15";
	};

	pinctrl_adc2_default: adc2_default {
		function = "ADC2";
		groups = "ADC2";
	};

	pinctrl_adc3_default: adc3_default {
		function = "ADC3";
		groups = "ADC3";
	};

	pinctrl_adc4_default: adc4_default {
		function = "ADC4";
		groups = "ADC4";
	};

	pinctrl_adc5_default: adc5_default {
		function = "ADC5";
		groups = "ADC5";
	};

	pinctrl_adc6_default: adc6_default {
		function = "ADC6";
		groups = "ADC6";
	};

	pinctrl_adc7_default: adc7_default {
		function = "ADC7";
		groups = "ADC7";
	};

	pinctrl_adc8_default: adc8_default {
		function = "ADC8";
		groups = "ADC8";
	};

	pinctrl_adc9_default: adc9_default {
		function = "ADC9";
		groups = "ADC9";
	};

	pinctrl_bmcint_default: bmcint_default {
		function = "BMCINT";
		groups = "BMCINT";
	};

	pinctrl_ddcclk_default: ddcclk_default {
		function = "DDCCLK";
		groups = "DDCCLK";
	};

	pinctrl_ddcdat_default: ddcdat_default {
		function = "DDCDAT";
		groups = "DDCDAT";
	};

	pinctrl_espi_default: espi_default {
		function = "ESPI";
		groups = "ESPI";
	};

	pinctrl_fwspics1_default: fwspics1_default {
		function = "FWSPICS1";
		groups = "FWSPICS1";
	};

	pinctrl_fwspics2_default: fwspics2_default {
		function = "FWSPICS2";
		groups = "FWSPICS2";
	};

	pinctrl_gpid0_default: gpid0_default {
		function = "GPID0";
		groups = "GPID0";
	};

	pinctrl_gpid2_default: gpid2_default {
		function = "GPID2";
		groups = "GPID2";
	};

	pinctrl_gpid4_default: gpid4_default {
		function = "GPID4";
		groups = "GPID4";
	};

	pinctrl_gpid6_default: gpid6_default {
		function = "GPID6";
		groups = "GPID6";
	};

	pinctrl_gpie0_default: gpie0_default {
		function = "GPIE0";
		groups = "GPIE0";
	};

	pinctrl_gpie2_default: gpie2_default {
		function = "GPIE2";
		groups = "GPIE2";
	};

	pinctrl_gpie4_default: gpie4_default {
		function = "GPIE4";
		groups = "GPIE4";
	};

	pinctrl_gpie6_default: gpie6_default {
		function = "GPIE6";
		groups = "GPIE6";
	};

	pinctrl_i2c10_default: i2c10_default {
		function = "I2C10";
		groups = "I2C10";
	};

	pinctrl_i2c11_default: i2c11_default {
		function = "I2C11";
		groups = "I2C11";
	};

	pinctrl_i2c12_default: i2c12_default {
		function = "I2C12";
		groups = "I2C12";
	};

	pinctrl_i2c13_default: i2c13_default {
		function = "I2C13";
		groups = "I2C13";
	};

	pinctrl_i2c14_default: i2c14_default {
		function = "I2C14";
		groups = "I2C14";
	};

	pinctrl_i2c3_default: i2c3_default {
		function = "I2C3";
		groups = "I2C3";
	};

	pinctrl_i2c4_default: i2c4_default {
		function = "I2C4";
		groups = "I2C4";
	};

	pinctrl_i2c5_default: i2c5_default {
		function = "I2C5";
		groups = "I2C5";
	};

	pinctrl_i2c6_default: i2c6_default {
		function = "I2C6";
		groups = "I2C6";
	};

	pinctrl_i2c7_default: i2c7_default {
		function = "I2C7";
		groups = "I2C7";
	};

	pinctrl_i2c8_default: i2c8_default {
		function = "I2C8";
		groups = "I2C8";
	};

	pinctrl_i2c9_default: i2c9_default {
		function = "I2C9";
		groups = "I2C9";
	};

	pinctrl_lad0_default: lad0_default {
		function = "LAD0";
		groups = "LAD0";
	};

	pinctrl_lad1_default: lad1_default {
		function = "LAD1";
		groups = "LAD1";
	};

	pinctrl_lad2_default: lad2_default {
		function = "LAD2";
		groups = "LAD2";
	};

	pinctrl_lad3_default: lad3_default {
		function = "LAD3";
		groups = "LAD3";
	};

	pinctrl_lclk_default: lclk_default {
		function = "LCLK";
		groups = "LCLK";
	};

	pinctrl_lframe_default: lframe_default {
		function = "LFRAME";
		groups = "LFRAME";
	};

	pinctrl_lpchc_default: lpchc_default {
		function = "LPCHC";
		groups = "LPCHC";
	};

	pinctrl_lpcpd_default: lpcpd_default {
		function = "LPCPD";
		groups = "LPCPD";
	};

	pinctrl_lpcplus_default: lpcplus_default {
		function = "LPCPLUS";
		groups = "LPCPLUS";
	};

	pinctrl_lpcpme_default: lpcpme_default {
		function = "LPCPME";
		groups = "LPCPME";
	};

	pinctrl_lpcrst_default: lpcrst_default {
		function = "LPCRST";
		groups = "LPCRST";
	};

	pinctrl_lpcsmi_default: lpcsmi_default {
		function = "LPCSMI";
		groups = "LPCSMI";
	};

	pinctrl_lsirq_default: lsirq_default {
		function = "LSIRQ";
		groups = "LSIRQ";
	};

	pinctrl_mac1link_default: mac1link_default {
		function = "MAC1LINK";
		groups = "MAC1LINK";
	};

	pinctrl_mac2link_default: mac2link_default {
		function = "MAC2LINK";
		groups = "MAC2LINK";
	};

	pinctrl_mdio1_default: mdio1_default {
		function = "MDIO1";
		groups = "MDIO1";
	};

	pinctrl_mdio2_default: mdio2_default {
		function = "MDIO2";
		groups = "MDIO2";
	};

	pinctrl_ncts1_default: ncts1_default {
		function = "NCTS1";
		groups = "NCTS1";
	};

	pinctrl_ncts2_default: ncts2_default {
		function = "NCTS2";
		groups = "NCTS2";
	};

	pinctrl_ncts3_default: ncts3_default {
		function = "NCTS3";
		groups = "NCTS3";
	};

	pinctrl_ncts4_default: ncts4_default {
		function = "NCTS4";
		groups = "NCTS4";
	};

	pinctrl_ndcd1_default: ndcd1_default {
		function = "NDCD1";
		groups = "NDCD1";
	};

	pinctrl_ndcd2_default: ndcd2_default {
		function = "NDCD2";
		groups = "NDCD2";
	};

	pinctrl_ndcd3_default: ndcd3_default {
		function = "NDCD3";
		groups = "NDCD3";
	};

	pinctrl_ndcd4_default: ndcd4_default {
		function = "NDCD4";
		groups = "NDCD4";
	};

	pinctrl_ndsr1_default: ndsr1_default {
		function = "NDSR1";
		groups = "NDSR1";
	};

	pinctrl_ndsr2_default: ndsr2_default {
		function = "NDSR2";
		groups = "NDSR2";
	};

	pinctrl_ndsr3_default: ndsr3_default {
		function = "NDSR3";
		groups = "NDSR3";
	};

	pinctrl_ndsr4_default: ndsr4_default {
		function = "NDSR4";
		groups = "NDSR4";
	};

	pinctrl_ndtr1_default: ndtr1_default {
		function = "NDTR1";
		groups = "NDTR1";
	};

	pinctrl_ndtr2_default: ndtr2_default {
		function = "NDTR2";
		groups = "NDTR2";
	};

	pinctrl_ndtr3_default: ndtr3_default {
		function = "NDTR3";
		groups = "NDTR3";
	};

	pinctrl_ndtr4_default: ndtr4_default {
		function = "NDTR4";
		groups = "NDTR4";
	};

	pinctrl_nri1_default: nri1_default {
		function = "NRI1";
		groups = "NRI1";
	};

	pinctrl_nri2_default: nri2_default {
		function = "NRI2";
		groups = "NRI2";
	};

	pinctrl_nri3_default: nri3_default {
		function = "NRI3";
		groups = "NRI3";
	};

	pinctrl_nri4_default: nri4_default {
		function = "NRI4";
		groups = "NRI4";
	};

	pinctrl_nrts1_default: nrts1_default {
		function = "NRTS1";
		groups = "NRTS1";
	};

	pinctrl_nrts2_default: nrts2_default {
		function = "NRTS2";
		groups = "NRTS2";
	};

	pinctrl_nrts3_default: nrts3_default {
		function = "NRTS3";
		groups = "NRTS3";
	};

	pinctrl_nrts4_default: nrts4_default {
		function = "NRTS4";
		groups = "NRTS4";
	};

	pinctrl_oscclk_default: oscclk_default {
		function = "OSCCLK";
		groups = "OSCCLK";
	};

	pinctrl_pewake_default: pewake_default {
		function = "PEWAKE";
		groups = "PEWAKE";
	};

	pinctrl_pnor_default: pnor_default {
		function = "PNOR";
		groups = "PNOR";
	};

	pinctrl_pwm0_default: pwm0_default {
		function = "PWM0";
		groups = "PWM0";
	};

	pinctrl_pwm1_default: pwm1_default {
		function = "PWM1";
		groups = "PWM1";
	};

	pinctrl_pwm2_default: pwm2_default {
		function = "PWM2";
		groups = "PWM2";
	};

	pinctrl_pwm3_default: pwm3_default {
		function = "PWM3";
		groups = "PWM3";
	};

	pinctrl_pwm4_default: pwm4_default {
		function = "PWM4";
		groups = "PWM4";
	};

	pinctrl_pwm5_default: pwm5_default {
		function = "PWM5";
		groups = "PWM5";
	};

	pinctrl_pwm6_default: pwm6_default {
		function = "PWM6";
		groups = "PWM6";
	};

	pinctrl_pwm7_default: pwm7_default {
		function = "PWM7";
		groups = "PWM7";
	};

	pinctrl_rgmii1_default: rgmii1_default {
		function = "RGMII1";
		groups = "RGMII1";
	};

	pinctrl_rgmii2_default: rgmii2_default {
		function = "RGMII2";
		groups = "RGMII2";
	};

	pinctrl_rmii1_default: rmii1_default {
		function = "RMII1";
		groups = "RMII1";
	};

	pinctrl_rmii2_default: rmii2_default {
		function = "RMII2";
		groups = "RMII2";
	};

	pinctrl_rxd1_default: rxd1_default {
		function = "RXD1";
		groups = "RXD1";
	};

	pinctrl_rxd2_default: rxd2_default {
		function = "RXD2";
		groups = "RXD2";
	};

	pinctrl_rxd3_default: rxd3_default {
		function = "RXD3";
		groups = "RXD3";
	};

	pinctrl_rxd4_default: rxd4_default {
		function = "RXD4";
		groups = "RXD4";
	};

	pinctrl_salt1_default: salt1_default {
		function = "SALT1";
		groups = "SALT1";
	};

	pinctrl_salt10_default: salt10_default {
		function = "SALT10";
		groups = "SALT10";
	};

	pinctrl_salt11_default: salt11_default {
		function = "SALT11";
		groups = "SALT11";
	};

	pinctrl_salt12_default: salt12_default {
		function = "SALT12";
		groups = "SALT12";
	};

	pinctrl_salt13_default: salt13_default {
		function = "SALT13";
		groups = "SALT13";
	};

	pinctrl_salt14_default: salt14_default {
		function = "SALT14";
		groups = "SALT14";
	};

	pinctrl_salt2_default: salt2_default {
		function = "SALT2";
		groups = "SALT2";
	};

	pinctrl_salt3_default: salt3_default {
		function = "SALT3";
		groups = "SALT3";
	};

	pinctrl_salt4_default: salt4_default {
		function = "SALT4";
		groups = "SALT4";
	};

	pinctrl_salt5_default: salt5_default {
		function = "SALT5";
		groups = "SALT5";
	};

	pinctrl_salt6_default: salt6_default {
		function = "SALT6";
		groups = "SALT6";
	};

	pinctrl_salt7_default: salt7_default {
		function = "SALT7";
		groups = "SALT7";
	};

	pinctrl_salt8_default: salt8_default {
		function = "SALT8";
		groups = "SALT8";
	};

	pinctrl_salt9_default: salt9_default {
		function = "SALT9";
		groups = "SALT9";
	};

	pinctrl_scl1_default: scl1_default {
		function = "SCL1";
		groups = "SCL1";
	};

	pinctrl_scl2_default: scl2_default {
		function = "SCL2";
		groups = "SCL2";
	};

	pinctrl_sd1_default: sd1_default {
		function = "SD1";
		groups = "SD1";
	};

	pinctrl_sd2_default: sd2_default {
		function = "SD2";
		groups = "SD2";
	};

	pinctrl_sda1_default: sda1_default {
		function = "SDA1";
		groups = "SDA1";
	};

	pinctrl_sda2_default: sda2_default {
		function = "SDA2";
		groups = "SDA2";
	};

	pinctrl_sgpm_default: sgpm_default {
		function = "SGPM";
		groups = "SGPM";
	};

	pinctrl_sgps1_default: sgps1_default {
		function = "SGPS1";
		groups = "SGPS1";
	};

	pinctrl_sgps2_default: sgps2_default {
		function = "SGPS2";
		groups = "SGPS2";
	};

	pinctrl_sioonctrl_default: sioonctrl_default {
		function = "SIOONCTRL";
		groups = "SIOONCTRL";
	};

	pinctrl_siopbi_default: siopbi_default {
		function = "SIOPBI";
		groups = "SIOPBI";
	};

	pinctrl_siopbo_default: siopbo_default {
		function = "SIOPBO";
		groups = "SIOPBO";
	};

	pinctrl_siopwreq_default: siopwreq_default {
		function = "SIOPWREQ";
		groups = "SIOPWREQ";
	};

	pinctrl_siopwrgd_default: siopwrgd_default {
		function = "SIOPWRGD";
		groups = "SIOPWRGD";
	};

	pinctrl_sios3_default: sios3_default {
		function = "SIOS3";
		groups = "SIOS3";
	};

	pinctrl_sios5_default: sios5_default {
		function = "SIOS5";
		groups = "SIOS5";
	};

	pinctrl_siosci_default: siosci_default {
		function = "SIOSCI";
		groups = "SIOSCI";
	};

	pinctrl_spi1_default: spi1_default {
		function = "SPI1";
		groups = "SPI1";
	};

	pinctrl_spi1cs1_default: spi1cs1_default {
		function = "SPI1CS1";
		groups = "SPI1CS1";
	};

	pinctrl_spi1debug_default: spi1debug_default {
		function = "SPI1DEBUG";
		groups = "SPI1DEBUG";
	};

	pinctrl_spi1passthru_default: spi1passthru_default {
		function = "SPI1PASSTHRU";
		groups = "SPI1PASSTHRU";
	};

	pinctrl_spi2ck_default: spi2ck_default {
		function = "SPI2CK";
		groups = "SPI2CK";
	};

	pinctrl_spi2cs0_default: spi2cs0_default {
		function = "SPI2CS0";
		groups = "SPI2CS0";
	};

	pinctrl_spi2cs1_default: spi2cs1_default {
		function = "SPI2CS1";
		groups = "SPI2CS1";
	};

	pinctrl_spi2miso_default: spi2miso_default {
		function = "SPI2MISO";
		groups = "SPI2MISO";
	};

	pinctrl_spi2mosi_default: spi2mosi_default {
		function = "SPI2MOSI";
		groups = "SPI2MOSI";
	};

	pinctrl_timer3_default: timer3_default {
		function = "TIMER3";
		groups = "TIMER3";
	};

	pinctrl_timer4_default: timer4_default {
		function = "TIMER4";
		groups = "TIMER4";
	};

	pinctrl_timer5_default: timer5_default {
		function = "TIMER5";
		groups = "TIMER5";
	};

	pinctrl_timer6_default: timer6_default {
		function = "TIMER6";
		groups = "TIMER6";
	};

	pinctrl_timer7_default: timer7_default {
		function = "TIMER7";
		groups = "TIMER7";
	};

	pinctrl_timer8_default: timer8_default {
		function = "TIMER8";
		groups = "TIMER8";
	};

	pinctrl_txd1_default: txd1_default {
		function = "TXD1";
		groups = "TXD1";
	};

	pinctrl_txd2_default: txd2_default {
		function = "TXD2";
		groups = "TXD2";
	};

	pinctrl_txd3_default: txd3_default {
		function = "TXD3";
		groups = "TXD3";
	};

	pinctrl_txd4_default: txd4_default {
		function = "TXD4";
		groups = "TXD4";
	};

	pinctrl_uart6_default: uart6_default {
		function = "UART6";
		groups = "UART6";
	};

	pinctrl_usbcki_default: usbcki_default {
		function = "USBCKI";
		groups = "USBCKI";
	};

	pinctrl_usb2ah_default: usb2ah_default {
		function = "USB2AH";
		groups = "USB2AH";
	};

	pinctrl_usb2ad_default: usb2ad_default {
		function = "USB2AD";
		groups = "USB2AD";
	};

	pinctrl_usb11bhid_default: usb11bhid_default {
		function = "USB11BHID";
		groups = "USB11BHID";
	};

	pinctrl_usb2bh_default: usb2bh_default {
		function = "USB2BH";
		groups = "USB2BH";
	};

	pinctrl_vgabiosrom_default: vgabiosrom_default {
		function = "VGABIOSROM";
		groups = "VGABIOSROM";
	};

	pinctrl_vgahs_default: vgahs_default {
		function = "VGAHS";
		groups = "VGAHS";
	};

	pinctrl_vgavs_default: vgavs_default {
		function = "VGAVS";
		groups = "VGAVS";
	};

	pinctrl_vpi24_default: vpi24_default {
		function = "VPI24";
		groups = "VPI24";
	};

	pinctrl_vpo_default: vpo_default {
		function = "VPO";
		groups = "VPO";
	};

	pinctrl_wdtrst1_default: wdtrst1_default {
		function = "WDTRST1";
		groups = "WDTRST1";
	};

	pinctrl_wdtrst2_default: wdtrst2_default {
		function = "WDTRST2";
		groups = "WDTRST2";
	};
};
